2013 Chrysler 200 Convertible
CANADIAN SPECIFICATIONS

All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions are measured at curb weight with standard wheels and tires unless otherwise noted.
NOTE: Information shown is correct at time of publication and is subject to change. 

GENERAL INFORMATION	
Body Style	Two-door Convertible 	
Assembly Plant 	Sterling Heights, Michigan, U.S.A.	
EnerGuide Vehicle Class 	Mid-Size	
Introduction Date	January 2011	
		
ENGINE: 2.4-LITRE, GASOLINE, DOHC, 16-VALVE, VVT, SMPI I-4    	
Availability	Standard on 200 Convertible LX 	
Type and Description	Four-cylinder inline, tuned intake manifold with electronic active charge motion control valves with dual counter-rotating balance shafts	
Displacement, cu. cm (cu. in.)	2360 	
Bore x Stroke	88 x 97 (3.46 x 3.82) 	
Valve System	Chain-driven DOHC, 16 valves, electronically controlled dual variable-valve timing (VVT), direct-acting shimless mechanical bucket tappets	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	High-pressure die-cast aluminum block with dry iron liners, cast-aluminum cylinder heads, cast-aluminum ladder frame, forged-steel crankshaft	
Compression 	10.5:1	
Power 	173 bhp @ 6,000 rpm 	
Torque 	166 lb.-ft. @ 4,400 rpm	
Max. Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity, L (qt.)	4.23 (4.5) 	
Coolant Capacity, L (qt.)	7.3 (7.7) 	
Emission Controls	Single catalytic converter dual heated oxygen sensors and engine features	
2012 EnerGuide Fuel Economy 
L/100 km (mpg)  (City/Hwy) 	10.3 (27) / 6.9 (41) with four-speed automatic transmission
11.5 (25) / 6.8 (42) with six-speed automatic transmission	
	
ENGINE: 3.6-LITRE, GASOLINE, DOHC, 24-VALVE, SMPI VVT V6	
Availability	Standard on 200 Convertible Touring, Limited, and S. Available on LX	
Type and Description	60-degree bank angle, liquid-cooled, three-plenum intake manifold with electronically controlled manifold tuning valve and short-runner valves with variable valve timing	
Displacement, (cu. cm)	3605 	
Bore x Stroke	96 x 83 (3.78 x 3.28) 	
Valve System	DOHC, 24 valves, hydraulic, electronically controlled dual variable-valve timing (VVT), roller finger followers	
Fuel Injection	Sequential, multi-port, electronic	
Construction	High-pressure die-cast A380 aluminum block with iron liners and 
semi-permanent mold A319 aluminum heads	
Compression Ratio	10.2:1	
Power 	283 bhp @ 6,400 rpm	
Torque 	260 lb.-ft. @ 4,400 rpm	
Max. Engine Speed	6,800 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity, L (qt.) 	5.7(6) with dry filter 	
Coolant Capacity, L (qt.)	10.98 (11.6) 	
Emission Controls	Dual catalytic converters, four heated oxygen sensors, electronic EGR, 
and internal engine features	
2012 EnerGuide Fuel Economy 
L/100 km (mpg) - City/Hwy 	11.0 (26) / 6.8 (42)	
		
TRANSAXLE: 40TES, AUTOMATIC FOUR-SPEED OVERDRIVE	
Availability	Standard on 200 Convertible LX 	
Description	Four-speed overdrive, adaptive electronic control, electronically modulated converter clutch	
Gear Ratios		
1st 	2.842   	
2nd	1.57    	
3rd	1.00	
4th 	0.69  	
Reverse 	2.21    	
Final Drive Ratio 	3.91 with 2.4L engine	
Overall Top Gear	2.69 with 2.4L engine	
	
TRANSAXLE: 62TE, AUTOMATIC SIX-SPEED OVERDRIVE	
Availability	Standard on 200 Convertible Touring, Limited and S. Available on LX	
Description	Six-speed, adaptive electronic control or Auto/Stick™ driver-interactive manual control and electronically modulated torque converter clutch	
Gear Ratios		
1st	4.127  	
2nd	2.842   	
3rd	2.283     	
4th	1.452   	
5th	1   	
6th 	0.69    	
Reverse	3.214	
Transfer Ratio 	0.95	
Final Drive Ratio	3.16 with 3.6L engine, 3.43 with 2.4L engine	
Overall Top Gear 	2.06 with 3.6L engine, 2.24 with 2.4L engine	
		
DRIVETRAIN		
Front-wheel Drive	Standard with all engines	
 		
DIMENSIONS AND CAPACITIES		
General		
Wheelbase	2765 (108.9) 	
Track, Front	1567 (61.7) 	
Track, Rear	1594 (62.7) 	
Overall Length	4947 (194.8) 	
Overall Width	1842 (72.5) without side mirrors / 2,089 (82.3) with side mirrors	
Overall Height with Cloth Convertible Top	1470 (57.9) with 225/55R17 	
Overall Height with Retractable Hard Top	1469 (57.8) with 225/55R17	
Aero Coefficient of Drag (Cd)	0.342	
		
Fuel Tank Capacity, L (gal.)	64.0 (14) Standard and FFV
	
Towing Capabilities, NAFTA Markets kg (lb.) 	
2.4L Auto. Trans 	454 (1000) 	
3.6L Auto. Trans	454 (1000) 	
(e) Maximum frontal area of trailer or boat: 2.04 sq. m (22 sq. ft.) 3.6L engine and 1.02 sq. m (11 sq. ft.) 2.4L engine.	

Curb Weight, Base Vehicle, kg (lb) 	
3.6L Gasoline Engine - 200 Touring	1814 (4000) 	

ACCOMMODATIONS		
Seating Capacity - F/R	2/2	
Total Interior Passenger Volume, L (cu. ft.) 	2503 (88.4)	
Front		
Head Room with Cloth Convertible Top	984 (38.7) 	
Head Room with Retractable Hard Top	992 (39.0) 	
Leg Room	1077 (42.4) 	
Shoulder Room	1432 (56.4) 	
Hip Room	1339 (52.7)	
Seat Travel 	260 (10.2) 	
Front Compartment Volume, L (cu. ft.) 	1517 (53.6) 	
Rear		
Head Room with Cloth Convertible Top	939 (37.0) 	
Head Room with Retractable Hard Top	921 (36.3) 	
Leg Room	850 (33.5) 	
Shoulder Room 	1197 (47.1) 	
Hip Room	1123 (44.2) 	
Rear Compartment Volume, L (cu. ft.) 	985 (34.8) 	
Cargo		
Trunk Lift-over Height	792 (31.2) 	
Total Trunk Volume – Top Up, L (cu. ft.)	376 (13.3) 	
Total Trunk Volume – Top Down, L (cu. ft.)	198 (7.0) 	
		
BODY/CHASSIS		
Layout 	Transverse front engine with front-wheel drive 	
Construction 	Steel unibody 	
		
SUSPENSION		
Front	Independent MacPherson strut, coil spring over gas-charged shock absorbers, stabilizer bar 	
Rear 	Multi-link independent with coil springs, link-type stabilizer bar, gas-charged shock absorbers and isolated rear suspension cradle	
 		
STEERING		
Type	Power rack and pinion 	
Overall Ratio	16.65:1	
Turning Diameter (curb-to-curb) m (ft.)	11.1 (36.5) (17-in. wheels), 11.5 (37.7) (18-in. wheels)	
Steering Turns (lock-to-lock)	2.98 (17-in. wheels), 2.89 (18-in. wheels)	
		
BRAKES		
Power-assist Type	204 x 230 (8 x 9) tandem-diaphragm vacuum	
Availability	Standard on LX, Touring, Limited and S models 	
Front		
Size and Type, in. (mm)	11.5 x 1.0 (294 x 26) vented rotors with 2.2 (57.0) single-piston floating caliper	
Swept Area (Total Front), sq. cm (sq. in.)	1442 (223.5) 	
Rear		
Size and Type, in. (mm)	Standard: 10.3 x 0.4 (262 x 10) solid rotor with 1.4 (35.0) single-piston floating caliper; Optional: 11.9 x 0.4 (302 x 10) solid rotor with 1.4 (35.0) single-piston floating caliper	
Swept Area (Total Rear), sq. cm (sq. in.)	Standard: 894 (138.6); Optional: 1230 (190.8) 	
Parking Brake Type	Drum-in-hat  	
Anti-lock Brake System (ABS)	Standard    	
Electronic Stability Control (ESC) 	Standard	
Traction Control	Standard	
Brake Assist	Standard	

WHEELS		
Availability	Standard on 200 Convertible LX model	
Type and Material	Machined cast-aluminum, Sparkle Silver 	
Size 	17 in. x 6.5 in.    	
		
Availability	Standard on 200 Convertible Touring and Limited models	
Type and Material	Polished aluminum	
Size	18 in. x 7.0 in.	
		
Availability	Standard on 200 Convertible S model	
Type and Material	Polished Aluminum with Black Painted Pockets, 	
Size	18 in. x 7.0 in.	
		
TIRES		
Availability	Standard on 200 Convertible LX model	
Size and Type	P225/55R17, All-season Touring	
Model	Continental ProContact Touring	
Revs per km (Mile)	779 (1262)	
		
Availability	Standard on 200 Convertible Touring, Limited, and S models	
Size and Type	P225/50R18, All-season Touring	
Model 	Goodyear Eagle LS-2 Touring	
Revs per km (Mile) 	777 (1250.4)	
• • •