2013 Jeep® Compass
CANADIAN SPECIFICATIONS

All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions are measured at curb weight with standard wheels and tires unless otherwise noted.
NOTE: Information shown is correct at time of publication and is subject to change. 

GENERAL INFORMATION		
Body Style	Sport-utility vehicle	
Assembly Plant	Belvidere, Illinois, USA	
EnerGuide Vehicle Class	Special Purpose	
Introduction Date	August 2006	
		
ENGINE: 2.0-LITRE DOHC 16-VALVE I-4 WITH DUAL VVT	
Availability	Available on Sport and North 4x2 models	
Type and Description 	Four-cylinder inline, tuned intake manifold with electronic active charge motion control valves, dual counter-rotating balance shafts	
Displacement, cu. cm (cu. in.)	1998 (121.9) 	
Bore x Stroke	86 x 86 (3.39 x 3.39)	
Valve System	Chain-driven DOHC, 16 valves, electronically controlled dual VVT, direct-acting shimless mechanical bucket tappets	
Fuel Injection 	Sequential, multiport, electronic, returnless	
Construction 	High-pressure die-cast aluminum block with dry iron liners, cast-aluminum cylinder head, cast-aluminum ladder frame, forged steel crankshaft	
Compression Ratio	10.5:1	
Power 	158 bhp @ 6,400 rpm 	
Torque 	141 lb.-ft. @ 5,000 rpm 	
Maximum Engine Speed	6,750 rpm (electronically limited)	
Fuel Requirement 	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity, L (qt.)	4.7  (5.0) 	
Coolant Capacity, L (qt.)	6.8 (7.2) 	
Emission Controls	Single catalytic converter, dual heated oxygen sensors and engine features 0.56 g/km (0.9 g/mile) 	
2012 EnerGuide Fuel Economy 
L/100 km (mpg) - City/Hwy 	9.1 (31)/6.8 (42) — 2WD with five-speed manual transaxle
9.0 (31)/7.3 (39)— 2WD CVT 	

ENGINE: 2.4-LITRE DOHC 16-VALVE I-4 WITH DUAL VVT	
Availability	Standard on Sport, North and Limited 4x2 and 4x4 models	
Type and Description
		Four-cylinder inline, tuned intake manifold with electronic active charge motion control valves dual counter-rotating balance shafts	
Displacement, cu. cm (cu. in.)	2360 (144)	
Bore x Stroke	88 x 97 (3.46 x 3.82)	
Valve System	Chain-driven DOHC, 16 valves, electronically controlled dual VVT, direct-acting shimless mechanical bucket tappets	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	High-pressure die-cast aluminum block with dry iron liners, 
cast-aluminum cylinder head, cast-aluminum ladder frame, 
forged steel crankshaft	
Compression Ratio	10.5:1	
Power 	172 bhp @ 6,000 rpm 	
Torque 	165 lb-ft @ 4,400 rpm	
Maximum Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity, L (qt.)	4.7 (5.0) 	
Coolant Capacity, L (qt.)	6.8 (7.2) 	
Emission Controls	Single catalytic converter, 2WD, Dual catalytic converter, 4WD 
Dual heated oxygen sensors and engine features	
Smog-forming Pollution, g/km (g/mile)	0.56 (0.9) 	
Maximum Gross Trailer Weight, kg (lb.)	454 (1000) 
907 (2000) — with Trailer-tow Prep Group	
2012 EnerGuide Fuel Economy 
L/100 km (mpg) - City/Hwy 
	9.0 (31)/7.0 (40) — 2WD with five-speed manual transaxle
9.6 (29)/7.4 (38) — 2WD with CVT2
9.2 (31)7.2 (39) — 4WD with five-speed manual transaxle
9.9 (29)/7.7 (37) — 4WD with CVT2 	

TRANSAXLE: MANUAL MAGNA DRIVELINE T355 FIVE-SPEED	
Availability	Standard — 2.0L engine
Standard — 2.4L engine	
Description	5-speed, overdrive, synchronized in all forward ratios, cable-operated, 3-plane shifter	
Gear Ratios		
1st	3.77	
2nd	2.16	
3rd	1.41	
4th	1.026	
5th	0.72 	
Reverse	3.417	
Final-drive Ratio	4.12	
Overall Top-gear	2.97	
TRANSAXLE: AUTOMATIC JATCO MODEL CVT2 WITH AUTO/STICK™	
Availability	Optional — 2.0L engine 
Optional — 2.4L engine	
Description	Continuously variable ratio, lockup torque converter, 
electronic controls	
Gear Ratios		
Forward	2.349:1 to 0.394:1 continuously variable	
Reverse	1.75:1	
Final-drive Ratio	2.0L 6.12:1; 2.4L 5.798 with 2.4L and Freedom Drive I
8.14 with 2.4L and Freedom Drive II	
Overall Top-gear Ratio	2.411; 2.28 with 2.4L and Freedom Drive I	
Auto/Stick™	Standard with CVT2	
		
TRANSAXLE: AUTOMATIC JATCO MODEL CVT2L (Freedom Drive II)	
Availability	Optional on 4WD with 2.4L engine	
Description	Continuously variable ratio, lockup torque converter, electronic controls	
Gear Ratios		
Forward	2.349:1 to 0.394:1 continuously variable	
Reverse	1.75:1	
Final-drive Ratio	8.135:1	
Overall Top-gear Ratio	3.21:1	
Effective Maximum Low-gear Ratio	19.11:1	
		
DRIVETRAIN		
Front-wheel Drive		
Availability	Standard	
Front Differential	Open	
Four-wheel Drive		
Availability	Optional	
Type	Electronically-controlled coupling (ECC) with four-wheel-drive lock	
Rear Differential	Open	
		
ELECTRICAL SYSTEM		
Alternator	120-amp; 140-amp with CVT2L (Freedom Drive II)	
Battery	525 CCA, maintenance-free	
		
DIMENSIONS AND CAPACITIES(d)		
Wheelbase	2635 (103.7)	
Track, Front	1520 (59.8)	
Track, Rear	1520 (59.8) 	
Overall Length	4448 (175.1) 	
Overall Width	1812 (71.4) 	
Overall Height	1651 (65.0)	
Overhang, Front	916 (36.1) 	
Overhang, Rear	897 (35.3) 	
Approach Angle with P215/60/R17 Tire	19.5°	
Breakover Angle with P215/60/R17 Tire	20.6°	
Departure Angle with P215/60/R17 Tire	28.5°	
Ground Clearance with P215/60/R17 Tire	206 (8.1) 	
Approach Angle with Freedom Drive II Off-road Package P215/65/R17 Tire	29.6°	
Breakover Angle with Freedom Drive II Off-road Package P215/65/R17 Tire	23.6°	
Departure Angle with Freedom Drive II Off-road Package P215/65/R17 Tire	31.2°	
Ground Clearance with Freedom Drive II Off-road Package P215/65/R17 Tire	231 (9.1) 	
Aero (CdA)	10.5 — 2WD
10.6 — 4WD	
Curb Weight, kg (lb.)	Sport 2WD —1407 (3101) 2.0 L MTX
Sport 4WD —1479 (3261) 2.4 L MTX
Limited 2WD — 1478 (3258) 2.4 L MTX 
Limited 4WD — 1544 (3403) 2.4L MTX	
Weight Distribution, per cent F/R	59/41 — 2WD
58/42 — 4WD	
Fuel Tank Capacity, L (gal.) 	51.5 (11.3) — 2WD; 51.1 (11.2) — 4WD	
(d) All dimensions measured at curb weight with standard tires.	
	
ACCOMMODATIONS		
Seating Capacity, F/R	2/3	
Front		
Head Room without Sunroof	1033 (40.7) 	
Leg Room	1032 (40.6)	
Shoulder Room	1387 (54.6) 	
Hip Room	1328 (52.3) 	
Seat Travel	Driver — 260 (10.2); Passenger — 260 (10.2) 	
Recliner Angle Range 	Driver — up to 88˚
Passenger — 76˚ fold-flat/88˚ non-fold-flat	
Front Seat Volume Index, L (cu. ft.)	1478 (52.2) 	

Rear		
Head Room	1013 (39.9) 	
Leg Room	1001 (39.4) 	
Knee Clearance	44 (1.7) 	
Shoulder Room	1372 (54.0)	
Hip Room	1295 (51.0) 	
Rear-Seat Volume Index, L (cu. ft.)	1390 (49.1) 	
Interior Volume, L (cu. ft.)	2868 (101.3) 	
Cargo Volume Indexes		
Rear Seats Up, L (cu. ft.)	642 (22.7) 	
Rear Seats Folded, L (cu. ft.)	1517 (53.6) 	
Interior Volume Index, L (cu. ft.)	3511 (124) 	
Trunk Lift-over Height	775 (30.5) 	
Cargo Volume with Front Passenger Seat and Rear Seat Folded, L (cu. ft.)	1775 (62.7) 	
Minimum Cargo Width at Liftgate Opening	976 (38.5) 	
Minimum Cargo Height at Liftgate Opening	634 (25.0) 	
Maximum Cargo Width at Liftgate Opening	1150 (45.3) 	
Maximum Cargo Height at Liftgate Opening	681 (26.7) 	
Distance Between Wheelhouse Interior Trim	966 (38.0) 	
		
BODY AND CHASSIS		
Layout	Transverse front-engine, front-wheel drive or four-wheel drive	
Construction	Unitized steel body	

SUSPENSION		
Front	Independent MacPherson strut, coil spring over gas-charged shock absorbers and stabilizer bar	
Rear	Multi-link independent with coil springs, link-type stabilizer bar, 
gas-charged shock absorbers	
		
STEERING		
Type	Rack-and-pinion with hydraulic power assist	
Overall Ratio	16.4:1	
Turning Diameter (curb-to-curb)	17-in. wheels and tires — 10.8 m (35.6 ft.) 
18-in. wheels and tires — 11.3 m (37.2 ft.) 	
Steering Turns (lock-to-lock)	17-in. wheels and tires — 2.88
18-in. wheels and tires — 2.76	
		
WHEELS		
Availability	Standard on Sport, North with 2.4L; available on Sport North with 2.0L	
Type and Material	Aluminum	
Size (in.)	17 x 6.5	
		
Availability	Standard on Sport, North with 2.0L engine	
Type and Material	Aluminum	
Size	16 x 16.5	
		
Availability	Standard on Limited	
Type and Material	Aluminum	
Size (in.)	18 x 7.0	
		
Availability	Optional on Limited	
Type and Material	Chrome-clad Aluminum	
Size (in.)	18 x 7.0	
		
TIRES		
Availability	Standard on Sport, North with 2.4L; available on Sport North with 2.0L	
Size and Type	P215/60R17 BSW All-season Touring	
Manufacturer and Model	Firestone Affinity S3	
Revs per km (mile) 	479 (771) 	
		
Availability	Standard on Sport, North with 2.0 L engine	
Size and Type	P205/70R16 BSW All-season tires	
Manufacturer and Model	Goodyear Eagle LS	
Revs per km (mile) 	475 (765)	
		
Availability	Standard on Limited	
Size and Type	P215/55R18 All-season Performance	
Manufacturer and Model	Firestone Firehawk GTA 03	
Revs per km (mile) 	476 (765) 	
		
Availability	Optional on Sport, North	
Size and Type	P215/65R17 outlined white letter (OWL) all-terrain	
Manufacturer and Model	Goodyear Wrangler GTA 03	
Revs per km (mile) 	462 (743) 	
		
BRAKES		
Availability	Standard on 4x2 Sport and North	
Front		
Size and Type	11.5 x 1.0 in. (294 x 26 mm) vented disc with 2.2 in. (57 mm) 
single-piston floating caliper	
Swept Area, sq. cm (sq. in.)	1442.12 (223.52) 	
Rear		
Size and Type	9.0 x 1.38 in. (229 x 35) drums 	
Swept Area, sq. cm (sq. in.)	503 (78.1) 	
Power-assist Type	254 (10) single-diaphragm vacuum	
Anti-lock Brake System (ABS)	Standard	
Electronic Stability Control (ESC)	Standard	
Hill-start Assist (HSA)	Standard with manual transmission	
		
Availability	Standard on Sport 4x4, North 4x4 and Limited 4x2 and 4x4 	
Front		
Size and Type	11.5 x 1.0 in. (294 x 26 mm) vented disc with 2.2 in. (57 mm) 
single-piston floating caliper	
Swept Area, sq. cm (sq. in.)	1442.12 (223.52) 	
Rear		
Size and Type	10.3 x 0.39 in. (262 x 10) solid disc with 1.4 in. (35 mm) single-piston floating caliper	
Swept Area, sq. cm (sq. in.)	894.6 (138.64) 	
Power-assist Type	254 (10) single-diaphragm vacuum	
Anti-lock Brake System (ABS)	Standard	
Electronic Stability Control (ESC)	Standard	
Hill-start Assist (HSA)	Standard with manual transmission and 
Freedom Drive II Off-Road Package	
Off-road Brake-traction Control System (BTCS)	Included with Freedom Drive II Off-Road Package 	
Hill-descent Control (HDC)	Included with Freedom Drive II Off-Road Package 	

• • •