2013 Jeep® Grand Cherokee
CANADIAN SPECIFICATIONS

All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions are measured at curb weight with standard wheels and tires unless otherwise noted.
NOTE: Information shown is correct at time of publication and is subject to change. 

GENERAL INFORMATION 	
Body Style	Four-door sport-utility vehicle 	
Construction	Steel uniframe	
Assembly Plant	Detroit, Michigan, U.S.A.	
EnerGuide Vehicle Class	Special Purpose	
Introduction	Spring 1992 as a 1993 model 	
	
Engine: 3.6-Litre PENTAStaR™ DOHC 24-Valve VVT V6	
Availability	Standard on all models 	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	3604 cu. cm (220 cu. in.)
96.0 x 83.0 (3.78 x 3.27) 	
Bore x Stroke	96 x 83 (3.77 x 3.26) 	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads	
Compression Ratio	10.2:1	
Power 	290 hp at 6,400 rpm 	
Torque 	260 lb.-ft. at 4,800 rpm	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R + M)/2	
Oil Capacity	5.7L (6.0 qt.) 	
Coolant Capacity	13.25L (14.0 qt.) 	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors 
and internal engine features	
Max. Gross Trailer Weight	2268 kg (5,000 lb.) — 2WD and 4WD	
2012 EnerGuide Fuel Economy L/100 km (mpg) - City/Hwy 	13.0 (22) / 8.8 (32)
	
Assembly Plant	Trenton, Michigan, U.S.A.	
		
ENGINE: 5.7-Litre HEMI® V8	
Availability	Optional on all models 	
Type and Description	90-degree V-type, liquid-cooled	
Displacement	5654 cu. cm (345 cu. in.) 	
Bore x Stroke	99.5 x 90.9 (3.92 x 3.58) 	
Valve System	Variable-valve timing, pushrod-operated overhead valves, 
16 valves, eight deactivating and eight conventional hydraulic lifters, 
all with roller followers	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, 
aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.5:1	
Power 	360 hp at 5,150 rpm	
Torque 	390 lb.-ft. at 4,250 rpm	
Max. Engine Speed	5,800 rpm (electronically-limited)	
Fuel Requirement	Unleaded mid-grade, 89 octane (R+M)/2 — recommended;
unleaded regular, 87 octane (R+M)/2 — acceptable	
Oil Capacity	6.6L (7 qt.) 	
Coolant Capacity	13.72L (14.5 qt.) 	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad heated oxygen sensors and internal engine features	
Max. Gross Trailer Weight	3266 kg (7,200 lb.) (4X4)	
2012 EnerGuide Fuel Economy L/100 km (mpg) - City/Hwy 
	14.5 (18) / 10.0 (27)
	
Assembly Plant	Saltillo, Mexico	
	
TRANSMISSION: W5A580 AUTOMATIC, FIVE-SPEED OVERDRIVE	
Availability	Included with 3.6-litre V6 engine	
Description	Electronic Range Select (ERS) driver-interactive manual control and electronically-modulated torque converter clutch	
Gear Ratios		
1st	3.59	
2nd	2.19	
3rd	1.41	
4th	1	
5th	0.83	
Reverse	3.16	
Final Drive Ratio	3.06:1 	
Overall Top Gear	2.54	
		
TRANSMISSION: 65RFE AUTOMATIC, SIX-SPEED	
Availability	Included with 5.7-litre engine	
Description	Three planetary gear sets, one overrunning clutch, with Electronic Range Select (ERS) driver interactive control, electronically controlled torque converter clutch	
Gear Ratios		
1st	3	
2nd	1.67 	
3rd	1.50	
4th	1	
5th	.5	
6th	.67	
Reverse	3	
Final Drive Ratio	3.47 	
Overall Top Gear	2.32	
		
TRANSFER CASE: MP 3010	
Availability	Optional with 3.6-litre engine	
Type	Single-speed	
Operating Mode	Full-time AWD	
Low Range Ratio	None	
Torque Split, Front/Rear	50/50	
		
TRANSFER CASE: MP 3022	
Availability	Optional with the 3.6-litre and 5.7-litre engine	
Type	Two-speed, electronically shifted	
Operating Modes	4x4 Low (Lock), Neutral; full-time active 4x4	
Low Range Ratio	2.72	
Torque Split, Front/Rear	Variable	
		
FRONT AXLES	
Differential Type	Conventional	
Availability	Standard on 4x4 models with 3.6-litre and 5.7-litre engines	
Ring Gear Diameter	195 mm (7.7 in.) 	
Axle Ratios	3.07:1 — 3.6-litre engine; 3.45:1 — 5.7-litre engine	
		
REAR AXLES	
Differential Type	Conventional	
Availability	Standard on all engines	
Ring Gear Diameter	215 mm (8.4 in.)— 3.6-litre engine, 225 mm (8.9 in.)— 5.7 litre engine	
Axle Ratios	3.06:1 — 3.6-litre engine; 3.47:1 — 5.7-litre engine		
Ring Gear Diameter	Same as conventional	
ELECTRICAL SYSTEM	
Alternator	160-amp; 180-amp or 220-amp depending on option content	
Battery	Group 65 maintenance-free 750CCA	
		
DIMENSIONS AND CAPACITIES (1)	
Wheelbase	2915 (114.8) 	
Track, Front	1623 (63.9) 	
Track, Rear	1627 (64.1) 	
Overall Length	4822 (189.8) 	
Overall Width (Width at Mirrors)	2154 (84.8) 	
Body Width	1943 (76.5) 	
Overall Height (at Roof Rail / at Antenna)	1761 (69.3) / 1779 (70.0) 	
Load Floor Height 
(Std Susp. / Air Susp.)	822 (32.4) / 807 (31.8) 	
Sill Step Height 
(Std Susp. / Air Susp.)	520 (20.5) / 508 (20.0) 	
Ground Clearance (with P245/70R17 Tire and 3.6L Engine)
(Std Susp. / Air Susp. – Pos#2)	
218 (8.6) / 270 (10.6) 	
Chassis (Fuel Tank) 
(Std Susp. / Air Susp. – Pos#2)	243 (9.6) / 294 (11.6) 	
Front Axle 
(Std Susp.. / Air Susp. – Pos#2)	236 (9.3) / 269.5 (10.6) 	
Rear Axle 
(Std Susp. / Air Susp. – Pos#2)	253 (10.0) / 303.5 (12.0) 	
Approach Angle, Degrees
(Std Susp. / Air Susp. – Pos#2, 
air-dam off)	
26.3 / 34.3 	
Ramp Breakover Angle, Degrees
(Std Susp. / Air Susp. – Pos#2)	
18.8 / 23.1	
Departure Angle, Degrees
(Std Susp. / Air Susp. – Pos#2)	
26.5 / 29.3 	
Frontal Area	2.88 sq. m (31.0 sq. ft.) 	
Drag Coefficient 	Approximately 0.37	
Aero CdA	11.6 (Cd x cross-sectional area)	
Fuel Tank Capacity L (gal.)	93.1L (20.5) 	
All dimensions shown in millimetres (inches) unless otherwise noted.	
	
ACCOMMODATIONS (1)		
Seating Capacity, Front/Second	2/3	
Front Seat		
Head Room	1013 (39.9) 	
Legroom	1025 (40.3) 	
Shoulder Room	1491 (58.7) 	
Hip Room	1449 (57.0) 	
Seat Travel	280 (11.0) 	
Volume L (cu. ft.)	1546 (54.6) 	
Rear Seat		
Head Room	995 (39.2) 	
Legroom	981 (38.6) 	
Shoulder Room	1474 (58.0) 	
Hip Room	1428 (56.2) 	
Knee Clearance	110 (4.3)	
Volume L (cu. ft.)	1438 (50.8) 	
Cargo Volume		
Behind Rear Seat L (cu. ft.)	994 (35.1) 	
Rear Seats Folded L (cu. ft.)	1945 (68.7) 	
(1)	All dimensions shown in millimetres (inches) unless otherwise noted.	
	
WEIGHTS (Estimates)		
	MODEL	ENGINE	GVWR(a) kg (lb.) 	CURB WEIGHT(b) kg (lb.) 	PAYLOAD(c) kg (lb.) 	
4WD	Laredo E
Laredo X
Laredo X	3.6-litre
3.6-litre
5.7-litre	2948 (6500) 
2948 (6500) 
2948 (6500)	2114 (4660) 
2114 (4660) 
2278 (5020) 	835 (1840) 
835 (1840) 
670 (1480) 	
	Limited	3.6-litre
5.7-litre	2948 (6500)
3084(6800) 	2201 (4850) 
2336 (5150) 	750 (1660) 
750 (1660) 	
	Overland	5.7-litre	3084 (6800) 	2364 (5210) 	720 (1590) 	
(a) Gross Vehicle Weight Rating. 
(b) Curb weight includes standard equipment and full quantities of fuel, lubricant and coolant.
(c) Payload is the maximum allowable weight of driver, passengers, cargo, and options, rounded to the nearest 5 kg (10 lb.) 	
	
WEIGHT DISTRIBUTION, F/R	
	MODEL	ENGINE	DISTRIBUTION 	
4WD	Laredo	3.6-litre
5.7-litre	53/47
55/45	
	Limited	3.6-litre	
5.7-litre	52/48
54/46	
	Overland	5.7-litre	54/46	
		
BODY		
4x4		
Layout	Longitudinal front engine, transfer case with full-time
four-wheel drive	
Construction	Steel uniframe	
		
SUSPENSION		
Front	Short- and long-arm independent (SLA), coil springs, gas-charged, twin-tube coil-over shock absorbers, upper- and lower-control arms (“A” arms), stabilizer bar	
Rear	Multi-link rear suspension, coil spring, twin tube shocks (including load leveling for towing), aluminum lower control arm, independent upper links (tension and camber) plus a separate toe link.	
		
STEERING		
Type	Power rack and pinion (V8) Electro-hydraulic Power Steering (V6)	
Steering Ratio	18.9:1 — on centre; 15.7:1 — at full lock	
Turn Circle Metres (feet)	11.3 (37.1) 	
Lock-to-Lock Steering Wheel Rotations	3.67	
		
BRAKES		
Type	Power, Single-rate, tandem diaphragm vacuum, ABS	
Availability    	Standard	
Front		
Size and Type in. (mm)	12.9 x 1.2 (328 x 30) vented disc with 1.89 (48) 
two-piston pin-slider caliper and ABS	
Swept Area		1820 sq. cm (282 sq. in.) 	
Rear		
Size and Type in. (mm)	12.6 x 0.55 (320 x 14) disc with 1.89 (48) single-piston pin-slider caliper and single-channel ABS(b)	
Swept Area	1658 sq. cm (257 sq. in.) 	
(a) Turning diameter is measured at the outside of the tires at curb height. Turning diameters and steering wheel turns, 
lock-to-lock, may differ with optional tires and wheels. 
(b) Four-channel ABS 	
	
TIRES	
Standard — Laredo E	
Size and Type	P245/70R17	
Mfr. and Model	Goodyear Fortera HL Black Sidewall All-Season — OWL Optional	
Revs per kilometre  (mile) 	1102 (685)	
	
Standard — Laredo X and Limited; 	
Size and Type	P265/60R18 	
Mfr. and Model	Michelin Latitude Tour Black Sidewall All-Season 	
Revs per kilometre  (mile)	1112 (691)	
	
Standard — Overland; Optional Limited	
Size and Type	P265/50R20	
Mfr. and Model	Goodyear Fortera HL Black Sidewall All-Season 	
Revs per kilometre  (mile)	1110 (690)	
	
Optional — Laredo E, Laredo X, Limited and Overland 	
Size and Type	P265/60R18 	
Mfr. and Model	Michelin Latitude Tour OWL All-Season	
Revs per kilometre  (mile)	1112 (691)	
	
Optional — Overland 	
Size and Type	P265/50R20	
Mfr. and Model	Goodyear Fortera HL Black Sidewall All-Season	
Revs per kilometre (mile)	1110 (690)	
		
WHEELS 		
Type and Material	Cast-aluminum 	
Sizes	17 in. x 8.0 in. aluminum wheels	
	18 in. x 8.0 in. tech silver aluminum wheels	
	18 in. x 8.0 in. polished aluminum wheels	
	20 in x 8.0 in. Premium Satin Carbon Aluminum wheels
20 in. x 8.0 in Premium Satin Carbon Polished Aluminum 	
		
TRAILER TOWING(a)		
	Engine	Axle Ratio	Maximum Trailer 
Weight(b) kg (lb) 	
			 	
4WD 		3.6-litre V6
5.7-litre V8	3.09 
3.45	2269 (5000) 
3300 (7200) 	
(a) All models can tow trailers up to 2268 kilograms (5000 pounds) with the addition of a trailer hitch. For towing heavier trailers up to the Maximum Trailer Weight Ratings shown in the Trailer Towing chart, the vehicle must be equipped with the Trailer Tow Group Class IV for the 5.7-litre engines for North America.
(b) Maximum Trailer Weight = GCWR - Curb Wt. with hitch – 136 kg (300 lb.) (allowance for driver and passenger) and must be decreased by the weight of optional equipment, cargo and additional passengers. Maximum trailer weights shown are rounded to the nearest 23kg (50 lb.) 
Tongue weight should be 10-15% of loaded trailer weight but may not cause vehicle to exceed GVWR or GAWR. Load equalizing hitch recommended for trailers over 907 kilograms (2000 pounds.)	

		• • •