2013 Jeep® Patriot
CANADIAN SPECIFICATIONS

All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions are measured at curb weight with standard wheels and tires unless otherwise noted.
NOTE: Information shown is correct at time of publication and is subject to change. 

GENERAL INFORMATION		
Body Style	Sport-utility vehicle	
Assembly Plant	Belvidere, Illinois, U.S.A.	
EnerGuide Vehicle Class	Special Purpose	
Introduction Date	December 2006 as a 2007 model	
		
ENGINE: 2.0-LITRE DOHC 16-VALVE I-4 WITH DUAL VVT 	
Availability	Available on 2WD Patriot Sport and North 	
Type and Description 	Four cylinders in-line, tuned intake manifold with electronic active charge motion control valves, dual counter-rotating balance shafts	
Displacement, cu. cm (cu. in.)	1998 (121.9)	
Bore x Stroke 	 86 x 86 (3.39 x 3.39)	
Valve System	Chain-driven DOHC, 16 valves, electronically controlled dual variable valve timing (VVT), direct-acting shimless mechanical bucket tappets	
Fuel Injection 	Sequential, multiport, electronic, returnless	
Construction 	High-pressure die-cast aluminum block with dry iron liners, cast-aluminum cylinder head, cast-aluminum ladder frame, forged steel crankshaft	
Compression Ratio	10.5:1	
Power 	158 bhp @ 6,400 rpm	
Torque 	141 lb.-ft. @ 5,000 rpm 	
Maximum Engine Speed	6,750 rpm (electronically limited)	
Fuel Requirement 	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity, L (qt.)	4.7 (5.0) SAE 5W/20	
Coolant Capacity, L (qt.)	6.8 (7.2) 	
Emission Controls	Single catalytic converter, dual heated oxygen sensors and engine features	
Smog-forming Pollution, g/km (g/mile)	0.56 (0.9) 	
2012 EnerGuide Fuel Economy 
L/100 km (mpg) - City/Hwy 
	9.1 (31)/6.8 (42)— 2WD with five speed manual transaxle
9.0 (31)/7.3 (39) — 2WD with continuously variable transmission (CVT) 	
	
ENGINE: 2.4-LITRE DOHC 16-VALVE I-4 WITH DUAL VVT	
Availability	Standard on Sport, North and Limited (4x2 and 4x4)	
Type and Description	Four-cylinder in-line, tuned intake manifold with electronic active charge motion control valves, dual counter-rotating balance shafts	
Displacement, cu. cm (cu. in.)	2360 (144) 	
Bore x Stroke	88 x 97 (3.46 x 3.82) 	
Valve System	Chain-driven DOHC, 16 valves, electronically controlled dual VVT, direct-acting shimless mechanical bucket tappets	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	High-pressure die-cast aluminum block with dry iron liners, cast-aluminum cylinder head, cast-aluminum ladder frame, forged steel crankshaft	
Compression Ratio	10.5:1	
Power 	172 bhp @ 6,000 rpm 	
Torque 	165 lb.-ft. @ 4,400 rpm 	
Maximum Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity, L (qt.)	4.7 (5.0) SAE 5W/20	
Coolant Capacity, L (qt.)	6.8 (7.2) 	
Emission Controls 	Single catalytic converter — 2WD 
Dual catalytic converter — 4WD 
Dual heated oxygen sensors and engine features	
Smog-forming Pollution, g/km (g/mile)	0.56 (0.9) 	
Maximum Gross Trailer Weight, kg (lb.)	454 (1000) 
907 (2000) — with Freedom Drive II® package, trailer-tow prep group	
2012 EnerGuide Fuel Economy 
L/100 km (mpg) - City/Hwy 
	9.0 (31)/7.0 (40) — 2WD with five-speed manual transaxle
9.6 (29)/7.4 (38) — 2WD with CVT2
9.2 (31)/7.2 (39) — 4WD with five-speed manual transaxle
9.9 (29)/7.7 (37)— 4WD with CVT2 	
		
TRANSAXLE: MAGNA DRIVELINE T355 5-SPEED 	
Availability	Standard — 2.0L engine
Standard — 2.4L engine	
Description	5-speed, overdrive, synchronized in all forward ratios, cable-operated, 
3-plane shifter	
Gear Ratios		
1st	3.77	
2nd	2.16	
3rd	1.41	
4th	1.026	
5th	0.72	
Reverse	3.417	
Final-drive Ratio	4.12	
Overall Top-gear	2.97	

TRANSAXLE: AUTOMATIC JATCO MODEL CVT2 WITH AUTO/STICK™	
Availability	Optional — 2.0L engine 
Optional — 2.4L engine	
Description	Continuously variable ratio, lockup torque converter, electronic controls	
Gear Ratios		
Forward	2.349:1 to 0.394:1 continuously variable	
Reverse	1.75:1	
Final-drive Ratio	6.12:1 (2.0L), 5.798:1 (2.4L)	
Overall Top-gear Ratio	2.411:1 (2.0L); 2.28 (2.4L)	
		
TRANSAXLE: AUTOMATIC JATCO MODEL CVT2L	
Availability	Optional on 4WD with 2.4L engine	
Description	Continuously variable ratio, lockup torque converter, electronic controls	
Gear Ratios		
Forward	2.349:1 to 0.394:1 continuously variable	
Reverse	1.75:1	
Final-drive Ratio	8.135:1	
Overall Top-gear Ratio	3.21:1	
Effective Maximum Low-gear Ratio	19.11:1	
		
DRIVETRAIN		
Front-wheel Drive		
Availability	Standard	
Front Differential 	Open	
Four-wheel Drive		
Availability	Optional	
Type	Electronically-controlled coupling (ECC) with four-wheel drive Lock	
Rear Differential 	Open	
		
ELECTRICAL SYSTEM		
Alternator	120-amp
140-amp with CVT2L	
Battery	525 CCA, maintenance-free	

DIMENSIONS AND CAPACITIES		
Wheelbase	2635 (103.7) 	
Track — Front	1520 (59.8) 	
Track — Rear	1520 (59.8) 	
Overall Length	4414 (173.8) 	
Overall Width	1757 (69.2) 	
Overall Height	1663 (65.5) 2WD, 1,696 (66.8) 4x4	
Overhang — Front	885 (34.7) 	
Overhang — Rear	894 (35.1) 	
Approach Angle with P215/60/R17 Tire	26.4°	
Breakover Angle with P215/60/R17 Tire	20.9° 	
Departure Angle with P215/60/R17 Tire	28.5°	
Ground Clearance with P215/60/R17 Tire	205 (8.1)	
Approach Angle with Freedom Drive II Off-Road Package including P215/65/R17 Tire	29.0°	
Breakover Angle with Freedom Drive II Off-Road Package including P215/65/R17 Tire	23.7°	
Departure Angle with Freedom Drive II Off-Road Package including P215/65/R17 Tire	33.9°	
Ground Clearance with Freedom Drive II Off-Road Package including P215/65/R17 Tire	231 (9.1) 	
Aero (CdA)	10.4 — 2WD
11.0 — 4WD	
Curb Weight, kg (lb.) Estimated	1411 (3111) — Sport 2WD, 2.0L MTX
1480 (3263) — Sport 4WD, 2.4L MTX
1446 (3187) — Limited 2WD, 2.4L MTX
1511 (3331) — Limited 4WD, 2.4L MTX	
Weight Distribution, per cent F/R	58/42 — 2WD
57/43 — 4WD	
Fuel Tank Capacity, L (gal.)	51.5 (11.3) — 2WD
51.1  (11.2) — 4WD	

ACCOMMODATIONS		
Seating Capacity — F/R	2/3	
Front		
Head Room without Sunroof	1040 (41.0) 	
Leg Room	1032 (40.6) 	
Shoulder Room	1385 (54.5) 	
Hip Room	1329 (52.3) 	
Seat Travel	260 (10.2)— driver
260 (10.2)— passenger	
Recliner Angle Range	Up to 88° — driver
76° fold-flat/88° non-fold-flat — passenger	
Front Volume Index, 
L (cu. ft.)	1481 (52.3) 	
Rear		
Head Room	1014 (39.9) 	
Leg Room	1001 (39.4) 	
Knee Clearance	44.1 (1.7) 	
Shoulder Room	1372 (54.0)	
Hip Room	1295 (51.0) 	
Rear Seat Volume Index, L (cu. ft.)	1390 (49.1) 	
Interior Volume, L (cu. ft.)	2956 (104.4) 	
Cargo Volume Indexes		
Rear Seats Up, L (cu. ft.)	651 (23.0) 	
Rear Seats Folded, L (cu. ft.)	1515 (53.5) 	
Interior Volume Index, L (cu. ft.)	3522 (124.4) 	
Trunk Lift-over Height	780 (30.7) 	
Cargo Volume with Front Passenger Fold-flat seat and Rear seat folded L (cu. ft.)	1795 (63.4) 	
Minimum Cargo Width at 
Liftgate Opening	988 (38.9) 	
Minimum Cargo Height at 
Liftgate Opening	656 (25.9) 	
Maximum Cargo Width at 
Liftgate Opening	1146 (45.1) 	
Maximum Cargo Height at 
Liftgate Opening	696 (27.4) 	
Distance Between Wheelhouse 
Interior Trim 	965 (38.0) 	

BODY		
Layout	Transverse front-engine front-wheel drive or four-wheel drive	
Construction	Unitized steel body 	
		
SUSPENSION 		
Front	Independent MacPherson strut, coil spring over gas-charged shock absorbers and stabilizer bar — Standard	
Rear	Multi-link independent with coil springs, link-type stabilizer bar, gas-charged shock absorbers — Standard 	
		
STEERING		
Type	Rack and pinion with hydraulic power assist	
Overall Ratio	16.4:1	
Turning Diameter (curb-to-curb)	With 16- or 17-in. wheels — 10.8 m (35.6 ft.)	
Steering Turns (lock-to-lock)	With 16- or 17-in. wheels and tires — 2.88	
		
WHEELS		
Availability	Standard on Sport and North	
Type and Material	Styled steel	
Size	16 in. x 6.5 in.	
		
Availability	Standard on Limited, Optional on Sport and North	
Type and Material	Polished Aluminum	
Size	17 in. x 6.5 in.	
		
TIRES		
Availability	Standard on Sport and North	
Size and Type	P205/70R16 BSW All-season Touring	
Manufacturer and Model	Goodyear Eagle LS2	
Revs per km (mile) 	470 (758) 	
		
Availability	Standard on Limited, Optional on Sport and North	
Size and Type	P215/60R17 BSW All-season Touring	
Manufacturer and Model	Firestone Affinity	
Revs per km (mile) 	479 (771) 	
		
Availability	Included with Freedom Drive II Off-Road Package and Tire and Wheel Group	
Size and Type	P215/65R17 OWL All-terrain	
Manufacturer and Model	Goodyear Wrangler GTA 03	
Revs per km (mile) 	462 (743) 	

BRAKES 	 	
Availability	Standard on Sport and North 4x2 	
Front		
Size and Type	11.5 x 1.0 in. (294 x 26 mm) vented disc with 2.2 in. (57 mm) single-piston floating caliper	
Swept Area, sq. cm (sq. in.)	1442 (223) 	
Rear		
Size and Type	9.0 x 1.38 in. (229 x 35) drums 	
Swept Area, sq. cm (sq. in.)	503.6 (78.1) 	
Power-assist Type	254 (10) single-diaphragm vacuum	
Anti-lock Brake System (ABS)	Standard	
Electronic Stability Control (ESC)	Standard	
Availability	Standard on Sport 4x4, North 4x4 and Limited 4x2 and 4x4	
Front		
Size and Type	11.5 x 1.0 in. (294 x 26 mm) vented disc with 2.2 in. (57 mm) single-piston floating caliper	
Swept Area, sq. cm (sq. in.)	1442 (223) 	
Rear		
Size and Type	10.3 x 0.39 in. (262 x 10) solid disc with 1.4 in. (35 mm) single-piston 
floating caliper	
Swept Area, sq. cm (sq. in.)	894.6 (138.64) 	
Power-assist Type	254 (10) single-diaphragm vacuum	
Anti-lock Brakes with On- and Off-road Calibrations	Standard	
Electronic Stability Control (ESC)	Standard	
Hill-start Assist (HSA)	Standard with manual transmission and Freedom Drive II Off-Road Package	
Off-road Brake-traction Control System (BTCS)	Included with Freedom Drive II Off-Road Package 	
Hill-descent Control (HDC)	Included with Freedom Drive II Off-Road Package 	

• • •