2013 Jeep® Wrangler Unlimited
CANADIAN SPECIFICATIONS

All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions are measured at curb weight with standard wheels and tires unless otherwise noted.
NOTE: Information shown is correct at time of publication and is subject to change. 

GENERAL INFORMATION		
Body Style	Four-door sport-utility vehicle	
Assembly Plant	Toledo, Ohio, U.S.A.	
EnerGuide Vehicle Class	Special purpose vehicle	
Introduction Date	2007	
	
ENGINE: 3.6-LITRE VVT, DOHC V6	
Availability	Standard on all models	
Type and Description	60° V-type, liquid-cooled	
Displacement	220 cu. in. (3604 cu. cm)	
Bore x Stroke	3.78 x 3.27 (96 x 83)	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads 	
Compression Ratio	10.2:1	
Power 	285 hp @ 6,400 rpm	
Torque 	260 lb.-ft. @ 4,800 rpm	
Max Engine Speed	6,600 erpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R + M)/2	
Oil Capacity	5.7L (6.0 qt.) 	
Coolant Capacity	13.25L (14 qt.)	
Emission Controls	Dual three-way catalytic converters, heated oxygen sensors
and internal engine features	
2012 EnerGuide Fuel Economy L/100 km (mpg) (City/Hwy)	5-speed Automatic 13.2 (21)/10.0 (28) 
6-speed Manual 13.4 (21)/9.6 (29)	
Assembly Plant	Trenton, Michigan, U.S.A.	
	
TRANSMISSION: NSG 370—MANUAL, SIX-SPEED OVERDRIVE	
Availability	Standard on all models	
Description	Synchronized in all forward gears and Reverse, multi-rail shift system with top-mounted shift lever	
Clutch	Hydraulic actuation	
Gear Ratios		
1st	4.46	
2nd	2.61	
3rd	1.72	
4th 	1.25	
5th 	1.0	
6th	0.797	
Reverse	4.06	
	
TRANSMISSION: W5A580 AUTOMATIC, FIVE-SPEED OVERDRIVE 	
Availability	Optional	
Description	Adaptive electronic control or Electronic Range Select (ERS) 
driver-interactive manual control and electronically modulated torque converter clutch	
Gear Ratios		
1st	3.59	
2nd	2.19	
3rd	1.41	
4th	1.0	
5th 	0.83	
Reverse	3.16	
	
TRANSFER CASE: NV241 COMMAND-TRACTM	
Availability	Standard on Wrangler Sport and Sahara	
Type	Part-time	
Operating Modes	2WD High; 4WD High; Neutral; 4WD Low	
Centre Differential Type	None	
Low-range Ratio	2.72:1	
	
TRANSFER CASE: NV241OR ROCK-TRAC®	
Availability	Standard on Wrangler Rubicon	
Type	Part-time	
Operating Modes	2WD High; 4WD High; Neutral; 4WD Low	
Centre Differential Type	None	
Low-range Ratio	4.0:1	
Axle Ratio 
	3.73 standard Rubicon w/automatic 
4.10 standard Rubicon w/manual (optional for automatic)	
Overall Top-gear		2.95 standard Rubicon w/automatic, 
3.24 standard Rubicon w/manual (optional for automatic)	
	
AXLES	
Front	Dana® 30, Dana 44 on Rubicon models	
Differential Type	Open (Dana 30) or Tru-Lok electronic locking (Dana 44)	
Axle Ratios	3.21, 3.73, 4.10	
Rear	Dana 44 	
Differential Type
cvzdvdsd	Open (Sport and Sahara) with available Trac-Lok anti-spin, 
Tru-Lok electronic locking (Rubicon)	
  Axle Ratios	3.21, 3.73, 4.10	
	
ELECTRICAL SYSTEM	
Alternator 	160 amp	
Battery	600 CCA, maintenance free	
Suspension		
Front	Live axle, Link coil, leading arms, track bar, coil springs, stabilizer bar	
    Stabilizer bar	Electronic sway-bar disconnect system — Standard, Rubicon	
    Shock type	Low-pressure (on 16-in. wheel packages) gas-charged shock absorbers — Standard
Monotube high-pressure (on 17- and 18-in. wheel packages) gas-charged shock absorbers — Standard	
Rear	Live axle, Link coil, trailing arms, track bar, coil springs, stabilizer bar	
    Shock type	Low-pressure (on 16-in. wheel packages) gas-charged shock absorbers — Standard
Monotube high-pressure (on 17- and 18-in. wheel packages) gas-charged shock absorbers — Standard	
	
DIMENSIONS AND CAPACITIES	
Wheelbase	2947 (116.0) 	
Overhang, Front	679 (26.7) 	
Overhang, Rear	778 (30.6)	
General Overall Length	4404 (173.4) 	
Overall Width (without Mirrors)	1877 (73.9) 	
Track, Front	1572 (61.9) 	
Track, Rear		1572 (61.9) 	
Height	1800 (70.8) 	
Cargo width at swing-gate opening	1491 (58.7)	
Cargo height at swing-gate opening	942.3 (37.1)	
Load floor height	706.1 (27.8) 	
Fuel-tank Capacity L (gal.)	85 (18.6) 	
		
CLEARANCES	
	P225/75R16	P255/75R17	P255/70R18	LT255/75R17		
Approach Angle, Deg. 	40.6	43.6	44.4	44.4		
Breakover Angle, Deg. 	17.8	20.3	20.9	20.8		
Departure Angle, Deg. 	37.4	40.3	40.7	40.5		
Front Axle to Ground 	229 (9.0)	259 (10.2)	267 (10.5)	267 (10.5)		
Rear Axle to Ground 	221 (8.7)	254 (10.0)	259 (10.2)	257 (10.1)		
	
CURB WEIGHT kg (lb.)	
Sport, Manual Transmission	1923 (4240) 	
Sport, Automatic Transmission	1929 (4253)  	
Sahara, Manual Transmission	1987 (4382) 	
Sahara, Automatic Transmission	1933 (4395) 	
Rubicon, Manual Transmission	2050 (4521) 	
Rubicon, Automatic Transmission	2057 (4535) 	
		
ACCOMMODATIONS		
Seating Capacity (front/rear)	2/3	
Front 		
Head Room	1048 (41.3) 	
Leg Room	1041 (41.0) 	
Shoulder Room	1417 (55.8) 	
Hip Room	1413 (55.6) 	
Seat Travel	240 (9.4) 	
Front-Volume Index, L (cu. ft.)	1546 (54.6) 	

Rear 		
Head Room	1025 (40.4) 	
Leg Room	945 (37.2) 	
Shoulder Room	1443 (56.8) 	
Hip Room	1440 (56.7) 	
Rear-Seat Volume Index, L (cu. ft.)	1399 (49.4 )	
Cargo Lift-over Height	798 (31.4) 	
Maximum Cargo Width at Swing 
Gate Opening	1490 (58.7) 	
Minimum Cargo Width at Swing 
Gate Opening	1047 (41.2) 	
Maximum Cargo Height at Swing 
Gate Opening	942 (37.1) 	
Minimum Cargo Height at Swing 
Gate Opening	940 (37.0) 	
Distance Between Wheelhouses	1136 (44.7) 	
Cargo Volume,  L (cu. ft.)		
Rear Seat Folded	2456 (88.7) 	
Rear Seat Upright	1315 (46.4) 	
Total Pass plus Cargo Volume	4250 (150.4)	
		
STEERING		
Type	Power, recirculating ball with damper	
Overall Ratio (m/ft)	16.7:1 overall	
Turning Diameter (curb-to-curb)	12.56 (41.2 ft.) with 225/75R16 tires	
Steering Turns (lock-to-lock)	3.5	
P/S Pump	Hydraulic	
		
BRAKES		
Availability	Standard 	
Type	Power assisted, anti-lock braking system	
Front 		
Rotor size and type 	11.9 x 1.1 (302 x 28) vented rotor 	
Caliber size and type	10 (254) single-diaphragm vacuum	
Rear 		
Rotor size and type 	11.9 x 1.1 (302 x 28) vented rotor	
Caliber size and type	2.6 (66) single-piston floating caliper 	
		
WHEELS		
Availability	Standard on Wrangler Unlimited Sport 	
Type and Material	Painted steel	
Size	16 x 7.0 in.	
		
Availability	Standard on Wrangler Unlimited Rubicon 	
Type and Material	Painted and polished cast-aluminum	
Size	17 x 7.5 in.	
		
Availability	Standard on Wrangler Unlimited Sahara 	
Type and Material	Painted cast-aluminum	
Size	18 x 7.5 in.	
		
Availability	Optional on Wrangler Unlimited Sahara	
Type and Material	Polished aluminum	
Size	18 x 7.5 in.	
		
TIRES		
Availability	Standard on Wrangler Unlimited Sport 	
Size and Type 	P225/75R16 BSW, on/off-road	
Mfr. and Model	Goodyear® Wrangler ST	
Revs per km (mile)	712 (1146)	
		
Availability	Standard on Wrangler Unlimited Sahara 	
Size and Type	P255/70R18 OWL, on/off-road 	
Mfr. and Model	Bridgestone Dueler 693	
Revs per km (mile)	653 (1051)	
		
Availability	Optional on Wrangler Unlimited Sport Standard on Wrangler Unlimited Rubicon 	
Size and Type	LT255/75R17 BSW, on/off-road	
Mfr. and Model	BF Goodrich Mud Terrain	
Revs per km (mile)	650 (1046)	

TOWING CAPACITIES	

WRANGLER UNLIMITED SPORT 4WD - kg (lb.)	
Engine	Trans Type	Transmission	Axle Ratio	Payload	Base Wt.	GAWR Front	GAWR Rear	GCWR	Max Trailer	
3.6L V6 gas (ERB) 	M6	NSG370 6-SPD MANUAL (DEH)	3.21	454 (1000)	1923 (4240)	1259 (2775)	1451 (3200)	2915 (6427)	907 (2000)	
3.6L V6 gas (ERB) 	M6	NSG370 6-SPD MANUAL (DEH)	3.73	454 (1000)	1923 (4240)	1259 (2775)	1451 (3200)	3596 (7927)	1588 (3500)	
3.6L V6 gas (ERB) 	A5	W5A580 5-SPD AUTO (DGJ) 	3.21	454 (1000)	1929 (4253)	1259 (2775)	1451 (3200)	2922 (6441)	907 (2000)	
3.6L V6 gas (ERB) 	A5	W5A580 5-SPD AUTO (DGJ) 	3.73	454 (1000)	1929 (4253)	1259 (2775)	1451 (3200)	3602 (7941)	1588 (3500)	
1. GCWR = Base Weight + Maximum Trailer Weight + 150 lb. for driver.						
	
WRANGLER UNLIMITED SAHARA 4WD - kg (lb.)	
Engine	Trans Type	Transmission	Axle Ratio	Payload	Base Wt.	GAWR Front	GAWR Rear	GCWR	Max Trailer	
3.6L V6 gas (ERB)	M6	NSG370 6-SPD MANUAL (DEH)	3.21	399 (880)	1987 (4382)	1259 (2775)	1451 (3200)	2970 (6547)	907 (2000)	
3.6L V6 gas (ERB)	M6	NSG370 6-SPD MANUAL (DEH)	3.73	399 (880)	1987 (4382)	1259 (2775)	1451 (3200)	3650 (8047)	1588 (3500)	
3.6L V6 gas (ERB)	A5	W5A580 5-SPD AUTO (DGJ)	3.21	399 (880)	1993 (4395)	1259 (2775)	1451 (3200)	2976 (6561)	907 (2000)	
3.6L V6 gas (ERB)	A5	W5A580 5-SPD AUTO (DGJ)	3.73	399 (880)	1993 (4395)	1259 (2775)	1451 (3200)	3656 (8061)	1588 (3500)	
1. GCWR = Base Weight + Maximum Trailer Weight + 150 lb. for driver.						
	
WRANGLER UNLIMITED RUBICON® 4WD  - kg (lb.)	
Engine	Trans Type	Transmission	Axle Ratio	Payload	Base Wt.	GAWR Front	GAWR Rear	GCWR	Max Trailer	
3.6L V6 gas (ERB) 	M6	NSG370 6-SPD MANUAL (DEH)	4.1	405 (892)	2050 (4521)	1259 (2775)	1451 (3200)	3706 (8171)	1588 (3500)	
3.6L V6 gas (ERB) 	A5	W5A580 5-SPD AUTO (DGJ) 	3.73	405 (892)	2057 (4535)	1259 (2775)	1451 (3200)	3706 (8171)	1588 (3500)	
3.6L V6 gas (ERB) 	A5	W5A580 5-SPD AUTO (DGJ) 	4.1	405 (892)	2057 (4535)	1259 (2775)	1451 (3200)	3706 (8171)	1588 (3500)	
1. GCWR = Base Weight + Maximum Trailer Weight + 150 lb. for driver.	

• • •