2013 Jeep® Wrangler 
CANADIAN SPECIFICATIONS

All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions are measured at curb weight with standard wheels and tires unless otherwise noted.
NOTE: Information shown is correct at time of publication and is subject to change. 

GENERAL INFORMATION		
Body Style	Two-door sport-utility vehicle	
Assembly Plant	Toledo, Ohio, U.S.A.	
EnerGuide Vehicle Class	Special purpose vehicle	
Introduction Date	1987 	
		
BODY/CHASSIS		
Layout	Longitudinal front engine, four-wheel drive	
Construction	Ladder-type frame, open steel body	

ENGINE: 3.6-LITRE, DOHC V6	
Availability	Standard on all models	
Type and Description	60° V-type, liquid-cooled	
Displacement	220 cu. in. (3604 cu cm)	
Bore x Stroke	96 x 83 (3.78 x 3.27) 	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads 	
Compression Ratio	10.2:1	
Power 	285 hp at 6,400 rpm	
Torque 	260 lb.-ft. at 4,800 rpm	
Max Engine Speed	6,600 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R + M)/2	
Oil Capacity	5.7L (6.0 qt.) 	
Coolant Capacity	13.25L (14 qt.) 	
Emission Controls	Dual three-way catalytic converters, heated oxygen sensors 
and internal engine features	
2012 EnerGuide Fuel Economy 
L/100 km (mpg) (City/Hwy)	5-speed automatic 12.6 (22) / 9.5 (30) 
6-speed manual 12.7 (22) / 9.3 (30)	
Assembly Plant	Trenton, Michigan, U.S.A.	
	
TRANSMISSION: W5A580 AUTOMATIC, FIVE-SPEED OVERDRIVE 	
Availability	Optional	
Description	Adaptive electronic control or Electronic Range Select (ERS) driver-interactive manual control and electronically modulated torque converter clutch	
Gear Ratios		
1st	3.59	
2nd	2.19	
3rd	1.41	
4th	1	
5th 	0.83	
Reverse	3.16	
Overall Top-gear	2.54	
		
TRANSMISSION: NSG 370 MANUAL, SIX-SPEED OVERDRIVE	
Availability	Standard on all models	
Description	Synchronized in all forward gears and Reverse, multi-rail shift system 
with top-mounted shift lever	
Clutch	Hydraulic actuation	
Gear Ratios		
1st	4.46	
2nd	2.61	
3rd	1.72	
4th 	1.25	
5th 	1	
6th	0.797	
Reverse	4.06	
Axle Ratio	3.21 standard Sport and Sahara, 3.73 optional Sport and Sahara (4.10 standard Rubicon)	
Overall Top-gear	2.53 standard, 2.95 optional (3.24 Rubicon)	
	
TRANSFER CASE: NV241 COMMAND-TRAC®	
Available	Standard on Sport and Sahara	
Axle Ratio	3.21 Standard (3.73 Optional)	
Type	Part-time	
Operating Modes	2WD High; 4WD High; Neutral; 4WD Low	
Centre Differential Type	None	
Low-range Ratio	2.72:1	
	
TRANSFER CASE: NV241OR ROCK-TRAC®	
Available	Standard on Rubicon	
Type	Part-time	
Operating Modes	2WD High; 4WD High; Neutral; 4WD Low	
Centre Differential Type	None	
Low-range Ratio	4.0:1	
Axle Ratio 	3.73 standard Rubicon w/automatic 
4.10 standard Rubicon w/manual (optional for automatic)	
		
AXLES		
Front   	Dana 30, Dana 44 on Rubicon models	
Differential Type	Open (Dana 30) or Tru-Lok electronic locking (Dana 44)	
Axle Ratios	3.21, 3.73, 4.10	
Rear  	Dana 44	
Differential Type	Open (Sport and Sahara) with available Trac-Lok anti-spin, 
Tru-Lok electronic locking (Rubicon)	
Axle Ratios	3.21, 3.73, 4.10	
Electrical System		
Alternator	160 amp	
Battery	600 CCA, maintenance free	
Suspension	 	
Front	Live axle, Link coil, leading arms, track bar, coil springs, stabilizer bar	
    Stabilizer bar	Electronic sway-bar disconnect system — Standard, Rubicon	
    Shock type	Low-pressure (on 16-in. wheel packages) gas-charged shock absorbers — standard
Monotube high-pressure (on 17- and 18-in. wheel packages) 
gas-charged shock absorbers — standard	
Rear	Live axle, Link coil, trailing arms, track bar, coil springs, stabilizer bar	
Shock type	Low-pressure (on 16-in. wheel packages) gas-charged shock absorbers — standard
Monotube high-pressure (on 17- and 18-in. wheel packages) 
gas-charged shock absorbers — standard	
		
DIMENSIONS AND CAPACITIES	
Overall Length	3881 (152.8) 	
Overall Width (without Mirrors)	1873(73.7) 	
Overall Height, Hardtop	1800 (70.9) 	
Wheelbase	2424 (95.4) 	
Track, Front	1572 (61.9) 	
Track, Rear		1572 (61.9) 	
Overhang, Front	679 (26.7) 	
Overhang, Rear	778 (30.6) 	
Lift-over Height 	706 (27.8)	
Cargo Width at swing gate opening	1491(58.7)	
Cargo Height at swing gate opening	942.3 (37.1)	
Load Floor Height	706 (27.3)	
Fuel-tank Capacity L (gal)	70 L (15.4) 	
		
CLEARANCES	
	P225/75R16	P245/75R16	P255/75R17	P255/70R18	LT255/75R17	
Approach Angle, Deg. 	40.8	42.0	43.8	44.6	44.3	
Breakover Angle, Deg. 	21.8	23.1	24.9	25.5	25.4	
Departure Angle, Deg. 	37.4	38.7	40.3	40.6	40.4	
Front Axle to Ground 	231 (9.1)	244 (9.6)	262 (10.3)	269 (10.6)	267 (10.5)	
Rear Axle to Ground 	223 (8.8)	239 (9.4)	257 (10.1)	261 (10.3)	259 (10.2)

CURB WEIGHT kg (lb.)	
Wrangler Sport, Manual Transmission	1754.0 (3867) 	
Wrangler Sport, Automatic Transmission	1759.9 (3880) 	
Wrangler Sahara, Manual Transmission	1833.4 (4042) 	
Wrangler Sahara, Automatic Transmission	1839.8 (4056) 	
Wrangler Rubicon, Manual Transmission	1874.2 (4132) 	
Wrangler Rubicon, Automatic Transmission	1880.6 (4,146) 	
		
ACCOMMODATIONS		
Seating Capacity, F/R	2/2	
Front 		
Head Room	1048.4 (41.3) 	
Legroom	1041.4 (41.0) 	
Shoulder Room	1416.7 (55.8) 	
Hip Room	1412.8  (55.6) 	
Seat Travel	Driver — 239.5  (9.4) 	
Front-Volume Index, L (cu ft) 	1546 (54.6) 	
Rear 		
Head Room	1024.6  (40.3) 	
Legroom	904.2  (35.6) 	
Shoulder Room	1565.9  (61.6) 	
Hip Room	1135.6  (44.7) 	
Rear-Seat Volume Index, L (cu ft)	1368  (48.3) 	
Cargo Liftover Height	706.1 (27.8)	
Maximum Cargo Width at liftgate Opening	1491.0 (58.7) 	
Minimum Cargo Width at liftgate Opening	1046.5 (41.2) 	
Maximum Cargo Height at liftgate Opening	942.3 (37.1) 	
Minimum Cargo Height at liftgate Opening	939.8 (37.0)	
Distance Between Wheelhouses Interior Trim	1135.4 (44.7) 	
Cargo Volume - L (cu. ft.)		
Rear Seat Installed	1600 (56.5)	
Rear Seat Removed	1733 (61.2) 	
Behind Rear Seat	486 (17.15) 	
Total Passenger Plus Cargo Volume 	3399 (120.05)	
		
STEERING		
Type	Power, recirculating ball with damper	
Overall Ratio	16.7:1 overall	
Turning Diameter (curb-to-curb) 	10.6 m (34.9 ft.) 	
Steering Turns (lock-to-lock)	3.5	
Power Steering Pump	Hydraulic	
		
BRAKES		
Availability	Standard	
Type	Power-assisted, anti-lock braking system	
Front
Rotor size and type – in. (mm)	11.9 x 1.1 (302 x 28) vented rotor 
with 2.6 (66) single-piston floating caliper	
Caliper size and type	254 (10) single-diaphram vacuum	
Swept Area, sq. m (sq. in.) - Total Front	9032 (234.3)	
Rear
Rotor size and type – in. (mm)	12.44 x 0.47 (316 x 12) solid rotor 
with 1.9 (48) single-piston floating caliper	
Swept Area, (Total Rear)	5146 (202.6)	
		
WHEELS		
Availability	Standard on Wrangler Sport 	
Type and Material	Painted steel	
Size	16 x 7.0 in.	
		
Availability	Standard on Wrangler Sahara	
Type and Material	Painted cast-aluminum	
Size	18 x 7.5 in.	
		
Availability	Optional on Wrangler Sahara 	
Type and Material	Polished Satin Carbon	
Size	18 x 7.5 in.	
		
Availability	Standard on Wrangler Rubicon
Optional on Wrangler Sport	
Type and Material	Polished Mineral Grey	
Size	17 x 7.5 in.	
TIRES		
Availability	Standard on Wrangler Sport	
Size and Type 	P225/75R16, on/off-road, black sidewall	
Mfr. and Model	Goodyear Wrangler ST	
Revs per km (Mile)	1146 (712) 	
		
Availability	Standard on Wrangler Sahara	
Size and Type	P255/70R18, on/off-road, OWL	
Mfr. and Model	Bridgestone Dueler 693	
Revs per km (Mile)	1051 (653) 	
		
Availability	Standard on Wrangler Rubicon
Optional on Wrangler Sport	
Size and Type	LT255/75R17, on/off-road, black sidewall	
Mfr. and Model	BF Goodrich Mud Terrain	
Revs per km (Mile)	1046 (650) 	

• • •