2013 Dodge Dart
CANADIAN Specifications

All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions are measured at curb weight with standard wheels and tires unless otherwise noted.
NOTE: Information shown is correct at time of publication and is subject to change. 

General Information		
Body Style	Four-door sedan	
Assembly Plant	Belvidere, Illinois, U.S.A.	
EnerGuide Vehicle Class	Compact car	
		
ENGINE: 2.0-LITRE DOHC 16-VALVE TIGERSHARK™ INLINE FOUR-CYLINDER 	
Availability	Standard — SE, SXT, Rallye and Limited 	
Type and Description 	Inline four-cylinder, dual overhead cam variable-valve timing, 16-valves with multiport fuel injection	
Displacement	1,995 cu. cm	
Bore x Stroke	88 X 82	
Valve System	DOHC, variable-valve timing, 4 valves per cylinder (16 total)	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	Aluminum block and cylinder head	
Compression Ratio	10.2:1	
Power 	160 bhp @ 6,300 rpm	
Torque 	148 lb.-ft. @ 4,600 rpm	
Max. Engine Speed	6,750 rpm	
Fuel Requirement	Unleaded regular, 87 Octane	
Oil Capacity L (qt.)	4.7(5.0) 	
Coolant Capacity L (qt.)	6.7 (7.1)  	
Emission Controls 	Single catalyst, dual heated oxygen sensors (1 upstream, one mid catalyst)	
Estimated EnerGuide Fuel Economy L/100 km (mpg) (City/Hwy)	MTX –  8.1 L/100 km (35 mpg) city / 5.4 L/100 km (52 mpg) highway
ATX – 8.7 L/100 km (32 mpg) city / 5.8 L/100 km (49 mpg) highway	
Engine Assembly Plant 	Dundee Engine Plant, Dundee, Mich.	
		
ENGINE: 1.4-LITRE SOHC 16-VALVE TURBOCHARGED INTERCOOLED MULTIAIR® INLINE FOUR-CYLINDER 	
Availability	Standard – Aero; Optional — SXT, Rallye and Limited models	
Type and Description 	Inline turbocharged four-cylinder, liquid-cooled	
Displacement, cu. cm	1,368	
Bore x Stroke	72 X 84	
Valve System	SOHC with MultiAir, 4 valves per cylinder (16 total)	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	Iron block, aluminum cylinder head	
Compression Ratio	9.8:1	
Power 	160 bhp @ 5,500 rpm	
Torque 	184 lb.-ft. @ 2,500-4,000 rpm	
Max. Engine Speed	6,500 rpm	
Fuel Requirement	Unleaded regular, 87 octane accepted;
Unleaded premium, 93 octane preferred	
Oil Capacity L (qt.)	3.8 (4.0) 	
Coolant Capacity L (qt.)	5.7 (6.0) 	
Emission Controls	Single catalytic converter, Heated Wide Band Lambda Sensor upstream and mid catalyst heated oxygen sensor	
Estimated EnerGuide Fuel Economy L/100 km (mpg) (City/Hwy)	 MTX – 7.4 L/100 km (38 mpg) city / 4.9 L/100 km (58 mpg) highway
 DDCT – 7.4 L/100 km (38 mpg) city / 5.3 L/100 km (53 mpg) highway	
Engine Assembly Plant 	Dundee Engine Plant, Dundee, Mich.	
	
ENGINE: 2.4-LITRE DOHC 16-VALVE MULTIAIR® II TIGERSHARK INLINE FOUR-CYLINDER	
Availability	Standard — R/T	
Type and Description	Inline four-cylinder, 16-valve MultiAir with multiport fuel injection	
Displacement, cu cm	2,360	
Bore x Stroke	88 X 97	
Valve System	SOHC, 4 valves per cylinder (16 total)	
Fuel Injection	Sequential, Multi-port, electronic, returnless	
Construction	Aluminum block, aluminum cylinder head	
Compression Ratio	10:1	
Power 	184 bhp @ 6,250 rpm	
Torque 	171 lb.-ft. @ 4,800 rpm	
Max. Engine Speed	6,500 rpm	
Fuel Requirement	Unleaded regular, 87 octane	
Oil Capacity L (qt.)	4.7 (5.0)	
Coolant Capacity L (qt.)	6.7 (7.1)	
Emission Controls	Single catalytic converter, Heated Wide Band Lambda Sensor upstream and mid-catalyst heated oxygen sensor	
Estimated EnerGuide Fuel Economy L/100 km (mpg) (City/Hwy)	TBD	
Engine Assembly Plant 	Dundee Engine Plant, Dundee, Mich.	
		
TRANSAXLE: c635 SIx-speed manual	
Availability	Standard with 2.0L (except Limited), 1.4L (except Limited) and 2.4L engines 	
Description	6-speed, fully synchronized, FWD, manual transmission	
Gear Ratios		
1st	3.90	
2nd	2.11	
3rd	1.36	
4th	0.97	
5th	0.75	
6th	0.62	
Reverse	4.0	
Final-drive Ratio	4.11 with 1.4L engine	
Overall Top-gear	2.54 with 1.4L engine	
	
TRANSAXLE: 6F24 six-Speed Automatic Overdrive	
Availability	Optional with 2.0L (standard on Limited) and 2.4L engines	
Description	6-speed, FWD, electronically controlled, automatic overdrive	
Gear Ratios		
1st	4.21	
2nd	2.64	
3rd	1.80	
4th	1.39	
5th	1.00	
6th	0.77	
Reverse	3.29	
Final-drive Ratio	3.20 with 2.0L engine and 2.4L engine	
Overall Top-gear	2.46 with 2.0L engine and 2.4L engine	
	
TRANSAXLE: C635 six-Speed Dual Dry Clutch Tranmission (DDCT)	
Availability	Optional with 1.4L engine	
Description	Six-speed, FWD, electronically controlled, automatic overdrive with dual dry clutch technology	
Gear Ratios		
1st	4.15	
2nd	2.26	
3rd	1.44	
4th	0.97	
5th	0.75	
6th	0.62	
Reverse	4.0	
Final-drive Ratio	4.43 with 1.4L engine	
Overall Top-gear	2.75 with 1.4L engine	
		
Drivetrain	
Front-wheel Drive		
Availability	Standard with all engines	
	
Dimensions and Capacities		
Dimensions		
Wheelbase	2703 (106.4)	
Track, Front	1568 (61.7) 	
Track, Rear	1565 (61.6) 	
Overall Length	4672 (183.9) 	
Overall Width	1830 (72.0) 	
Overall Height	1465 (57.7) 	
Aero Cd	0.285	
Fuel Tank Capacity, L (gal.)	60 (13.2) 	
Towing Capabilities, kg (lb.)		
2.0L automatic transmission	454  (1000) 	
2.4L automatic transmission	454 (1000) 	
Curb Weight, (with fuel) kg (lb.) 		
2.0L gasoline engine	1445 (3186) (MTX)
1471 (3242) (ATX)	
1.4L gasoline engine	1447 (3191) (MTX)
1471 (3242) (DDCT)	
2.4L gasoline engine	1495 (3297) (MTX)
1519 (3348) (ATX)	
		
accommodations		
Seating Capacity - F/R	2/3	
Total Interior Passenger Volume, 
L (cu. ft.) 	2752 (97.2) 	
Front, mm (in.)		
Head Room w/o Sunroof	980 (38.6) 	
Head Room w/Sunroof	950 (37.4) 	
Leg Room	1071 (42.2) 	
Shoulder Room	1477 (58.2) 	
Hip Room	1393 (54.8) 	
Seat Travel	260 (10.32) 	
Front Compartment Volume, 
L (cu. ft.) 	1552 (54.8) 	
Rear, mm (in.)		
Head Room w/o Sunroof 	940 (37.0) 	
Leg Room	895 (35.2) 	
Shoulder Room	1425 (56.1) 	
Hip Room	1337 (52.6) 	
Knee Clearance	30.2 (1.2) 	
Rear Compartment Volume, L (cu. ft.)	1201 (42.4) 	
Cargo		
Trunk Lift-over Height	710 (29.7) 	
Luggage Compartment Volume, L (cu. ft.) 	371 (13.1) 	
	
Body/Chassis		
Layout	Transverse front engine, front-wheel drive	
Construction	High-strength steel unibody	
	
Suspension		
Front	Independent MacPherson strut, coil spring over gas-charged shock absorbers, stabilizer bar 	
Rear	Multi-link independent with coil springs, link-type stabilizer bar, gas-charged shock absorbers 	
	
Steering		
Type	Electric, Dual Pinion	
Overall Ratio	15:1 (12.76:1 R/T Model)	
Turning Diameter (curb-to-curb), m (ft.)	11.1 (36.5) (17-in. wheels)
11.5 (37.7) (18-in. wheels)	
Steering Turns (lock-to-lock)	3.3 (17-in. wheels)
3.0 (18-in. wheels)	
		
Brakes	
Availability	Standard	
Power-assist Type	Single 11-in. Diaphragm vacuum	
Front		
Size and Type (mm)	305 X 28 vented rotors with 60mm single piston floating caliper	
Swept Area (Total Front), sq. cm (sq. in.)	413.2 (64.0) 	
Rear		
Size and Type (mm)	264 X 10 solid rotors with 38mm single piston floating caliper	
Swept Area (Total Rear), sq. cm (sq. in.)	254.6 (39.5) 	
Parking Brake Type	Rear caliper integrated park brake system	
Antilock Brake System (ABS)	Standard	
Electronic Stability Control (ESC)	Standard	
Traction Control	Standard	
Brake Assist	Standard	
		
Wheels		
Availability	Standard on SE	
Type and Material	Steel Wheel with Tech Silver Painted wheel cover	
Size (in.)	16 x 7	
		
Availability	Standard on SXT	
Type and Material	Steel Wheel with Tech Silver Painted wheel cover	
Size (in.)	17 x 7	
		
Availability	Optional on SXT, Standard on Rallye & Limited	
Type and Material	Cast Aluminum, Tech Silver painted  	
Size (in.)	17 x 7.5	
		
Availability	Optional on Rallye	
Type and Material	Cast Aluminum, Hyper Black 	
Size (in.)	17 x 7.5	
	
Availability 	Optional on Limited	
Type and Material	Cast Aluminum, Polished	
Size (in.)	17 x 7.5	
	
Availability	Standard on R/T	
Type and Material	Cast Aluminum, Satin Silver painted	
Size (in.)	18 x 7.5	
		
Availability	Optional on R/T	
Type and Material	Cast Aluminum, Hyper Black	
Size (in.)	18 x 7.5	
	
Tires		
Availability 	Standard on SE	
Size and Type	205/55 R16, All Season	
Model	Continental ContiProContact 	
Revs per km (mile)	1300 (808)	
		
Availability	Standard on SE	
Size and Type	205/55 R16, All Season	
Model	Kumho Solus KH25	
Revs per km (mile)	1300 (808)	
	
Availability	Standard on SXT, Rallye, Limited	
Size and Type	225/45 R17, All Season	
Model	Continental ContiProContact	
Revs per km (mile)	1300 (808)	
		
Availability	Standard on SXT, Rallye, Limited	
Size and Type	225/45 R17, All Season	
Model	Kumho Solus KH25	
Revs per km (mile)	1300 (808)	
		
Availability	Standard on SXT, Rallye, Limited	
Size and Type	225/45 R17, All Season	
Model	Yokohama (late availability)	
Revs per km (mile)	1300 (808)	

Availability	Standard on R/T	
Size and Type	225/40 R18, All Season	
Model	Continental ContiProContact	
Revs per km (mile)	1294 (804)	
		
Availability	Standard on R/T	
Size and Type	225/40 R18, All season	
Model	Yokohama (late availability)	
Revs per km (mile)	1294 (804)	

• • •