2013 Dodge Durango
CANADIAN SPECIFICATIONS

All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions are measured at curb weight with standard wheels and tires unless otherwise noted.
NOTE: Information shown is correct at time of publication and is subject to change. 

GENERAL INFORMATION		
Body Style	Four-door sport-utility vehicle 	
Construction	Steel unibody	
Assembly Plant	Detroit, Michigan, USA	
EnerGuide Vehicle Class	Special Purpose	
Introduction Date	Fourth quarter of 2010 as a 2011 model	
		
Engine: 3.6-Litre PENTAStar™ DOHC 24-Valve VVT V6	
Availability	Standard on all models (not available on R/T)	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	3604 cu. cm (220 cu. in.) 	
Bore x Stroke	96.0 x 83.0 (3.78 x 3.27) 	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads	
Compression Ratio	10.2:1	
Power 	290 hp at 6,400 rpm 	
Torque 	260 lb.-ft. at 4,800 rpm	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R + M)/2	
Oil Capacity	5.7L (6.0 qt.) 	
Coolant Capacity	13.25L (14.0 qt.) 	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors 
and internal engine features	
2012 EnerGuide Fuel Economy L/100 km (mpg) - City/Hwy 	3.6 L Pentastar V6 with automatic 13.0 (22)/8.8 (32)
		 	
Assembly Plant	Trenton, Michigan, USA	

ENGINE: 5.7-LITRE HEMI® MDS VVT V8	
Availability	Standard on R/T and optional on Crew, Citadel 	
Type and Description	90-degree V-type, liquid-cooled	
Displacement	5654 cu. cm (345 cu. in.) 	
Bore x Stroke	99.5 x 90.9 (3.92 x 3.58) 	
Valve System	Variable valve timing (VVT), pushrod-operated overhead valves, 
16 valves, eight deactivating and eight conventional hydraulic lifters, 
all with roller followers	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, 
aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.5:1	
Power 	360 hp at 5,150 rpm	
Torque 	390 lb.-ft. at 4,250 rpm	
Max. Engine Speed	5,800 rpm (electronically limited)	
Fuel Requirement	Unleaded mid-grade, 89 octane (R+M)/2—recommended;
unleaded regular, 87 octane (R+M)/2—acceptable	
Oil Capacity	6.6L (7 qt.) 	
Coolant Capacity	13.72L (14.5 qt.) 	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad heated oxygen sensors and internal engine features	
2012 EnerGuide Fuel Economy L/100 km (mpg) - City/Hwy 	5.7L HEMI VVT V8 with automatic 16.6 (17)/10.1(28)			
Assembly Plant	Saltillo, Mexico	
		
TRANSFER CASE: MP 3010		
Availability	Optional with 3.6-litre engine	
Type	Single-speed	
Operating Mode	Full-time AWD	
Low Range Ratio	None	
Torque Split, Front/Rear	50/50	
		
TRANSFER CASE: MP 3022		
Availability	Optional with 5.7-litre engine	
Type	Two-speed, electronically shifted	
Operating Modes	AWD Low (Lock), Neutral; full-time active AWD	
Low Range Ratio	2.72	
Torque Split, Front/Rear	Variable	

FRONT AXLES		
Differential Type	Conventional	
Availability	Standard on AWD models with 3.6-litre and 5.7-litre engines	
Ring Gear Diameter	195 mm (7.7 in.) 	
Axle Ratios	3.09:1 — 3.6-litre engine; 3.45:1 — 5.7-litre engine	
		
REAR AXLES		
Differential Type	Conventional	
Availability	Standard on all engines	
Ring Gear Diameter	215 mm (8.4 in.)– 3.6-litre engine, 
225 mm (8.9 in.)– 5.7 litre engine	
Axle Ratios	3.09:1 — 3.6-litre engine; 3.45:1 — 5.7-litre engine		
Differential Type	Electronic Limited Slip Differential	
Axle Ratios	3.47—5.7-litre engine		
		
ELECTRICAL SYSTEM		
Alternator	160-amp; 180-amp or 220-amp depending on option content	
Battery	Group 65 maintenance-free 750CCA	
		
DIMENSIONS AND CAPACITIES		
Wheelbase	3042 (119.8) 	
Track, Front	1623 (63.9) 	
Track, Rear	1627 (64.1) 	
Overall Length	5075 (199.8) 	
Overall Width (Width at Mirrors)	2172 (85.5) 	
Body Width	1924 (75.8) 	
Overall Height (at Roof Rail / at Antenna)	1801 (70.9) / 1819 (71.6) 	
Load Floor Height	817 (32.2) 	
Sill Step Height	522 (20.5) / 523 (20.6) 	
Ground Clearance 
(with P265/60R18 Tire and 3.6L Engine)	
207 (8.1) 	
Chassis (Fuel Tank) 	250 (9.8) 	
Front Axle	243 (9.6) 	
Rear Axle	241 (9.5) 	
Approach Angle	16.3 degrees	
Ramp Breakover Angle	17.8 degrees 	
Departure Angle	21.4 degrees	
Frontal Area	2.88 sq. m (31.0 sq. ft.) 	
Drag Coefficient 	Approximately 0.35	
Fuel Tank Capacity L (imp. gal.)	93.1L (20.5) 	
		
ACCOMMODATIONS		
Seating Capacity, front/second/third rows	2/3/2, 2/2/2 with optional second-row captain’s chairs	
Front Row		
Head Room	1013 (39.9) 	
Legroom	1025 (40.3) 	
Shoulder Room	1486 (58.5) 	
Hip Room	1449 (57.0) 	
Seat Travel	280 (11.0) 	
Volume L (cu. ft.)	1540 (54.4)	
Second Row		
Head Room	1011 (39.8) 	
Legroom	981 (38.6) 	
Shoulder Room	1481 (58.3) 	
Hip Room	1423 (56.0) 	
Volume L (cu. ft.)	1269 (48.8)	
Third Row		
Head Room	960 (37.8) 	
Legroom	800 (31.5) 	
Shoulder Room	1281 (50.4) 	
Hip Room 	1088 (42.8) 	
Volume L (cu ft.)	982 (34.7) 	
Cargo Volume		
Behind Third Row L (cu. ft.)	487 (17.2) 	
Behind Second Row L (cu. ft.)	1351 (47.7) 	
Behind Front-row Seats with 
Rear Seats Folded L (cu. ft.)	2393 (84.5) 	

WEIGHTS (Estimates)	
	MODEL	ENGINE	GVWR(a) kg (lb.) 	CURB WEIGHT(b) kg (lb.)	PAYLOAD(c) kg (lb.)	
AWD	SXT	3.6-litre	2948 (6500) 	2229 (4913) 	640 (1410) 	
	Crew	3.6-litre
5.7-litre	2948 (6500) 
3221 (7100) 	2262 (4987) 
2418 (5330) 	645 (1420) 
650 (1430) 	
	Citadel	3.6-litre
5.7-litre	3221 (7100) 
3221 (7100) 	2312 (5097) 
2448 (5397) 	615 (1360) 
620 (1370) 	
	R/T	5.7-litre	3221 (7100) 	2418 (5331) 	605 (1340) 	
(a) Gross Vehicle Weight Rating. 
(b) Curb weight includes standard equipment and full quantities of fuel, lubricant and coolant.
(c) Payload is the maximum allowable weight of driver, passengers, cargo, and options, rounded to the nearest 5kg (10 lb.). 	

SUSPENSION		
Front	Short- and long-arm independent (SLA), coil springs, 
gas-charged, twin-tube coil-over shock absorbers, 
upper- and lower-control arms (“A” arms), stabilizer bar	
Rear	Multi-link rear suspension, coil spring, twin tube shocks (including load leveling for towing), aluminum lower control arm, independent upper links (tension and camber) plus a separate toe link.	
		
STEERING		
Type	Power rack and pinion	
Steering Ratio	19:1	
Turn Circle metres (feet)	11.3 (37.1)	
Lock-to-Lock Steering Wheel Rotations	3.67	
Power Steering Pump	Electro-hydraulic on V6, Hydraulic on V8	
		
BRAKES 	
Type  	Power-assisted, Anti-Lock Braking System (ABS)	
Front	
Size and Type in. (mm)	13.0 x 1.26 (330 x 32) vented disc (Standard duty) or 13.8 x 1.26 (350 x 32) vented disc (Heavy duty) with 1.89 (48) 
two-piston pin-slider caliper and ABS	
Swept Area		1969 sq. cm (305 sq. in.) - Standard Duty 324 2088 sq. cm (sq. in.) - Heavy Duty	
Rear	
Size and Type in. (mm)	13.0 x 0.55  (330 x 14) solid disc (Standard Duty) or 13.0 x 0.87 (330 x 22 mm) vented disc (Heavy Duty) with 1.89 (48) single-piston floating caliper and ABS	
Swept Area	1523 sq. cm (232 sq. in.) 	
(a) Turning diameter is measured at the outside of the tires at curb height. Turning diameters and steering wheel turns, 
lock-to-lock, may differ with optional tires and wheels. 
(b) Four-channel ABS standard 	
	
TIRES 	
Availability		
Standard — SXT and Crew 		
Size and Type	P265/60R18	
Mfr. and Model	Michelin Latitude Tour Black Sidewall All-Season	
Standard — R/T and Citadel, optional on SXT and Crew	
Size and Type	P265/50R20	
Mfr. and Model	Goodyear Fortera HL Black Sidewall All-Season	
	
WHEELS 	
Type and Material	Cast-aluminum 	
Size	SXT 18-in. x 8-in, Crew, R/T, Citadel: 20-in x 8-in.  SXT:  20-in x 8-in. (available)	

TRAILER TOWING(a)	
	Engine	Axle Ratio	Maximum Trailer 
Weight (b) kg (lb.) 	
			 	
AWD 		3.6-litre V6
5.7-litre V8	3.06 
3.47	2812 (6200) 
3265 (7200) 	
(a) All models can tow trailers up to 2,268 kilograms ( 5,000 pounds) with the addition of a trailer hitch. For towing heavier trailers up to the Maximum Trailer Weight Ratings shown in the Trailer Towing chart, the vehicle must be equipped with the Trailer Tow Group Class IV for the 5.7-litre engines for North America.
(b) Maximum Trailer Weight = GCWR - Curb Wt. with hitch – 136 kg (300 lb.) (allowance for driver and passenger) and must be decreased by the weight of optional equipment, cargo and additional passengers. Maximum trailer weights shown are rounded to the nearest 23 kg (50 lb.) Tongue weight should be 10-15% of loaded trailer weight but may not cause vehicle to exceed GVWR or GAWR. Load equalizing hitch recommended for trailers over 907 kilograms (2,000 pounds.)	

		• • •