2013 Dodge Journey
cANADIAN Specifications 

All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions are measured at curb weight with standard wheels and tires unless otherwise noted.
NOTE: Information shown is correct at time of publication and is subject to change. 

General Information		
Body Style	Four-door; five- or seven-passenger	
Assembly Plant	Toluca, Mexico	
EnerGuide Vehicle Class	Special Purpose	
Introduction date	Early 2008	
	
BODY/CHASSIS	
Layout	Transverse front engine, front-wheel drive or all-wheel drive	
Construction	Steel unibody	
	
ENGINE: 2.4-LITRE DOHC 16-VALVE, VVT, SMPI I-4	
Availability	CVP, SE Plus and SXT	
Type and Description	Four cylinders in-line, tuned intake manifold with dual counter-rotating balance shafts and dual variable-valve timing	
Displacement, cu. cm (cu. in.)	2360 (144) 	
Bore x Stroke	88 x 97 (3.46 x 3.82) 	
Compression Ratio	10.5:1	
Power 	173 bhp @ 6,000 rpm 	
Torque 	166 lb.-ft. @ 4,000 rpm	
Maximum Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity, L (qt.)	4.26 (4.5) w/filter SAE 5W-20	
Coolant Capacity, L (qt.)	7.5 (7.9) — single-zone climate control 	
Emission Controls	Single catalytic converter, dual heated oxygen sensors and internal engine features	
EnerGuide Fuel Economy 
L/100 km (mpg) - City/Hwy 	10.8 (26) / 7.5 (38)	
Engine Assembly Plant	Dundee, Michigan, U.S.A.	
	
ENGINE: 3.6-LITRE SOHC, 24-VALVE SMPI V6	
Availability	Available on SXT. Standard on Crew, R/T AWD and R/T Rallye AWD	
Type and Description	60-degree bank angle, liquid-cooled, three-plenum intake manifold with electronically controlled manifold tuning valve and short-runner valves 	
Displacement, cu. cm (cu. in.)	3,605 (220) 	
Bore x Stroke	96 x 81 (3.78 x 3.19) 	
Compression Ratio	10.0:1	
Valve System	DOHC, 24 valves, hydraulic, centre-pivot roller 
rocker arms 	
Fuel Injection	Sequential, multi-port, electronic 	
Power 	283 bhp @ 6,350 rpm 	
Torque 	260 lb.-ft. @ 4,400 rpm 	
Maximum Engine Speed	6,800 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2 
Ethanol E85	
Oil Capacity, L (qt.)	5.2  (5.5) w/filter 10W-30 MAF 	
Coolant Capacity, L (qt.)	10 (10.6) — single- or dual-zone climate control 
11 (11.6) — tri-zone climate control 	
Emission Controls	Three-way catalytic converter, electronic EGR, and internal engine features	
2012 EnerGuide Fuel Economy 
L/100 km (mpg) - City/Hwy 	12.6 (22)/7.8 (36) FWD; 13.0 (22)/ 8.4 (34) AWD	
	
TRANSAXLE: 40TES AUTOMATIC FOUR-SPEED OVERDRIVE	
Availability	CVP, SE Plus and SXT with 2.4L engine	
Description	Four-speed overdrive, adaptive electronic control, electronically modulated converter clutch	
Gear Ratios		
1st	2.842	
2nd	1.57	
3rd	1.0	
4th	0.69	
Reverse	2.21	
Final-drive Ratio	4.28	
Overall Top-gear	2.95	
	
TRANSAXLE: 62TE/62TEA AUTOMATIC SIX-SPEED OVERDRIVE	
Availability	SXT, Crew, R/T AWD and R/T Rallye AWD with 3.6 L engine	
Description	Six-speed, adaptive electronic control and electronically modulated torque converter clutch	
Gear Ratios		
1st	4.127	
2nd	2.842	
3rd	2.283	
4th	1.452 — Upshift 
1.570 — WOT kickdown	
5th	1.00	
6th	0.690	
Reverse	3.214	
Transfer Ratio	0.95	
Final-drive Ratio	3.16	
Overall Top-gear	2.06	
		
Drivetrain	
Front-wheel Drive		
Availability	CVP, SE Plus, SXT, and Crew	
All-wheel Drive		
Availability	R/T AWD and R/T Rallye AWD	
Type	Electronically-controlled coupling (ECC) with variable torque output	
Rear Differential	Open	
	
Body/Chassis	
Layout	Transverse front engine, front-wheel drive or 
all-wheel drive	
Construction	Steel unibody	
	
Suspension	
Front	Independent MacPherson strut, coil spring over gas-charged shock absorbers, stabilizer bar with isolated suspension cradle	
Rear	Multi-link independent with coil springs, link-type stabilizer bar, gas-charged shock absorbers and isolated rear suspension cradle	
	
Steering	
Type	Power rack and pinion	
Overall Ratio	16.45	
Turning Diameter (curb-to-curb), m (ft.)	11.7  (38.5) — 17-in. wheels and tires 
11.9  (39.0) —19-in. wheels and tires 	
Steering Turns (lock-to-lock)	2.92	
	
Electrical	
Battery	525-amp maintenance-free 	
Alternator	160-amp — Standard on all Journey models 	
	
Brakes	
Four-wheel anti-lock brakes	Standard on all Journey models	
Front		
Size and Type, in. (mm)	11.9 x 1.1 (302 x 28) vented rotors with 2.6 (66.0) single-piston floating caliper	
Swept Area (total front), sq. cm (sq. in.)	1494  (231.6) 	
Rear		
Size and Type, in. (mm)	12.0 x 0.47 (305 x 12) solid rotors with 1.7 (43.0) single-piston floating caliper	
Swept Area (total rear), sq. cm (sq. in.)	1395 (216.3) 	
Power-assist Type	204 x 230 (8 x 9) tandem-diaphragm vacuum	
Parking Brake Type	Foot lever with integral parking brake	
		
Electronic Chassis Control Features	
Four-wheel anti-lock brakes	Standard	
Electronic Stability Control	Standard	
All-speed traction control	Standard	
Trailer Sway Control	Standard	
Electronic Roll Mitigation	Standard 	
	
Dimensions and Capacities	
General		
Wheelbase	2890 (113.8) 	
Track, Front	1571 (61.8) 	
Track, Rear	1582 (62.3) 	
Overall Length	4888 (192.4) 	
Overhang, Front	989 (38.9) 	
Overhang, Rear	1009 (39.7) 	
Overall Width	1835 (72.2) 	
Body Width, including Mirrors	2127 (83.7) 	
Overall Height (with P225/65R17 tires)	1693 (66.6) 	
Vehicle Height including Roof Rack Assembly Complete (with P225/65R17 tires)	1765 (69.5) 	
Aero Coefficient of Drag (CD)	0.368	
Fuel Tank Capacity, L (gal.) 	2.4L and 3.6L FWD — 78 (17) 
3.6L AWD — 80 (17.6) 	
Towing Capabilities, kg  (lb.) 		
2.4L I4 with Automatic Transaxle	454 (1000) 	
3.6L V6 with Automatic Transaxle, FWD or AWD	1134 (2500) 	
Gross Vehicle Weight Rating (GVWR), kg (lb.) 		
Five-passenger Vehicle, FWD 2.4L	2270 (5005) 	
Seven-passenger Vehicle, FWD 2.4L	2381 (5250) 	
Five-passenger Vehicle, AWD 3.6L	2540 (5600) 	
Seven-passenger Vehicle, FWD 3.6L	2483 (5475) 	
Seven-passenger Vehicle, AWD 3.6L	2540 (5600) 	
Gross Axle Weight Rating (GAWR), kg (lb.) 		
Front Five- and seven-passenger vehicles	1247 (2750) 	
Rear Five- and seven-passenger vehicles	1315 (2900) 	
Curb Weight, Five-passenger Vehicle, Automatic Transaxle, kg (lb.) 		
2.4L I-4 Engine	FWD — 1735 (3818) 	
3.6L V6 Engine	FWD — 1843 (4054) 
AWD — 1926 (4238) 	
	
Accommodations	
Seating Capacity — F/R	2/3 or 2/3/2	
 Volume Index, L (cu. ft.) 	3793.7 (134) – 7-passenger / 3,810.1 (134.6) 5-passenger	
Total Interior Passenger Compartment Volume, L (cu. ft.) 	3502.8 (123.7) – 7-passenger / 2820.8 (99.6) 
5-passenger	
First-Row		
Head Room without Sunroof	1036 (40.8) 	
Head Room with Sunroof	995 (39.2) 	
Leg Room	1036 (40.8) 	
Shoulder Room	1460 (57.5) 	
Hip Room	1367 (53.8) 	
Seat Travel	260 (10.23) 	
Front Compartment Volume, L (cu. ft.) 	1568.4 (55.39) 	
Second-Row		
Head Room without Sunroof	1013 (39.9) 	
Head Room with Sunroof	995 (39.2) 	
Leg Room	854 (33.6) 	
Leg Room, Maximum	917 (36.1) 	
Shoulder Room	1444 (56.9) 	
Hip Room	1382 (54.4) 	
Couple, First to Second Row	774 (30.5) 	
Second Row Compartment Volume, L (cu. ft.) 	1248.8 (44.1) 	
Third-Row		
Head Room	957 (37.7) 	
Legroom	596 (23.4) 	
Shoulder Room	1105 (43.5) 	
Hip Room	1016 (40.0) 	
Couple, Second to Third Row	765 (30.1) 	
Rear Compartment Volume, L (cu. ft.) 	628.6 (22.2) 	
Cargo Area		
Liftover Height @ Curb Load	782 (30.8) 	
Cargo Width @ Wheelhouse	1051 (41.4) 	
Maximum Cargo Height	 842 (33.1) 	
Cargo Volumes		
Behind First Row Seat, L (cu. ft.) 	1914.2 (67.6) 	
Behind Second Row Seat, L (cu. ft.)
(5-passenger vehicles)	1121.6 (39.61) 	
Behind Second Row Seat, L (cu. ft.)
(7-passenger vehicles)	1047.7 (37.0) 	
Behind Third Row Seat, L (cu. ft.) 	303 (10.7) 	
	
Wheels	
Availability	Standard on CVP, SE Plus 	
Type and Material	Cast-aluminum, 5-spoke	
Size (in.)	17 x 6.5	
		
Availability	Available on CVP	
Type and Material	Steel wheel with twin 5-spoke wheel cover	
Size (in.)	17 x 6.5	
		
Availability	Standard on SXT	
Type and Material	Cast-aluminum, twin 5-spoke 	
Size (in.)	17 x 6.5	
		
Availability	Standard on Crew and R/T AWD, optional on SXT	
Type and Material	Cast-aluminum	
Size (in.)	19 x 7.0	
		
Availability	Optional on Crew and R/T AWD	
Type and Material	Chrome-clad aluminum, 6-spoke	
Size (in.)	19 x 7.0	
		
Availability	Standard on R/T Rallye AWD	
Type and Material	Cast-aluminum, satin carbon finish	
Size (in.)	19 x 7.0	
		
Availability	Standard on all models 	
Type and Material	Temporary spare steel wheel	
Size (in.)	16 x 4.0 x 46	
	
Tires 	
Availability	Standard on CVP, SE Plus and SXT	
Size and Type	P225/65R17, All-season Touring	
Model	Kumho Solus KH16	
Revs per km (mile)	471 (725) 	
		
Availability	Standard on Crew, R/T AWD and R/T Rallye AWD, optional on SXT	
Size and Type	225/55R19, All-season Touring	
Model	Kumho Solus KH16	
Revs per km (mile)	444 (711)	
		
Availability	Standard on all Journey models 	
Size and Type	T145/80 R16 temporary spare tire	

		• • •