2013 Ram 1500 
CANADIAN SPECIFICATIONS

All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions are measured at curb weight with standard wheels and tires unless otherwise noted.
NOTE: Information shown is correct at time of publication and is subject to change. 

GENERAL INFORMATION		
Vehicle Type	Regular Cab, Quad Cab, and Crew Cab, 2WD, 4WD	
Assembly Plant	Regular Cab: Saltillo, Mexico
Quad Cab: Warren, Michigan, U.S.A.
Crew Cab: Warren, Michigan, U.S.A.	
Vehicle Class	Standard Pickup	

BODY/CHASSIS		
Layout	2WD — Longitudinal, front engine
4WD — Longitudinal, front engine, transfer case	
Construction	2WD — Ladder-type frame, steel cab, double-wall steel pickup box
4WD — Ladder-type frame, steel cab, double-wall steel pickup box	
		
ENGINE: 3.6-LITRE 24-VALVE DOHC V6 	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	3604 cu. cm (220 cu. in.) 	
Bore x Stroke	96.0 mm x 83.0 mm (3.78 in. x 3.27 in.)  	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads	
Compression Ratio	10.2:1	
Power 	305 hp at 6,400 rpm	
Torque 	269 lb.-ft. at 4,175 rpm	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2, 
E85-compatible for non-feet applications	
Oil Capacity	5.7L (6.0 qt.) 	
Coolant Capacity	13.25L (14.0 qt.) 	
Emission Controls	Dual three-way catalytic converters, heated oxygen sensors	
Estimated EnerGuide Fuel Economy 
L/100 km (mpg) (City/Hwy)	TBA	
		
ENGINE: 4.7-LITRE SOHC 16-VALVE SMPI V8 E85	
Type and Description	90-degree V8, liquid-cooled	
Displacement	4701 cu. cm (287 cu. in.) 	
Bore x Stroke	93.0 mm x 86.5 mm (3.66 in. x 3.40 in.)	
Valve System	Chain-driven SOHC, 16 valves	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	Cast-iron block, aluminum alloy heads	
Compression Ratio	9.0:1	
Power 	310 hp @ 5,650 rpm	
Torque 	330 lb.-ft. @ 3,950 rpm	
Max. Engine Speed	6,000 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2, E85-compatible	
Oil Capacity	5.7L (6.0 qt.) 	
Coolant Capacity	10.23L (10.8 qt.) 	
Emission Controls	Three-way catalytic converters, heated oxygen sensors 
and internal engine features	
Estimated EnerGuide Fuel Economy 
L/100 km (mpg) (City/Hwy)	TBA	
		
ENGINE: 5.7-LITRE HEMI® 16-VALVE V8		
Type and Description	90-degree V8, liquid-cooled	
Displacement	5654 cu. cm (345 cu. in.) 	
Bore x Stroke	99.5 mm x 90.9 mm (3.92 in. x 3.58 in.) 	
Valve System	Variable cam timing, pushrod-operated overhead valves, 16 valves, hydraulic lifters with roller followers	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.5:1	
Power 	395 hp @ 5,600 rpm	
Torque 	407 lb.-ft. @ 3,950 rpm	
Max. Engine Speed	5,800 rpm	
Fuel Requirement	Unleaded mid-grade, 89 octane (R+M)/2 — recommended 
Unleaded regular, 87 octane (R+M)/2 — acceptable	
Oil Capacity	6.6L (7.0 qt.) 	
Coolant Capacity	13.33L (14.0 qt.) 	
Emission Controls	Three-way catalytic converters, heated oxygen sensors 
and internal engine features	
Estimated EnerGuide Fuel Economy 
L/100 km (mpg) (City/Hwy) 8-speed automatic	TBA	
Estimated EnerGuide Fuel Economy 
L/100 km (mpg) (City/Hwy) 6-speed automatic	TBA	
TRANSMISSION: 65RFE AUTOMATIC SIX-SPEED	
Availability	Standard with 4.7-litre V8, available with 5.7-litre V8 equipped trucks	
Description	Three planetary gear sets, one overrunning clutch, full electronic control, electronically controlled converter clutch	
Gear Ratios		
1st	3.00	
2nd	1.67 	
    3rd   	1.50	
4th	1.00	
    5th	0.75	
6th	0.67	
Reverse	3.00	
Final Drive and Overall Top Gear Ratios	2.15 with 3.21 axle; 2.38 with 3.55 axle; 2.63 with 3.92 axle; 
and 2.75 with 4.10 axle	
Max Torque	410 lb.-ft. 	
	
TRANSMISSION: ZF 8HP45 AUTOMATIC EIGHT-SPEED WITH ELECTRONIC RANGE SELECT (ERS)	
Availability	Standard with 3.6-litre V6 equipped trucks	
Description	Adaptive electronic control, automatic or Electronic Range Select (ERS) manual control. Five clutch-pack design with only two open clutches in any gear. Torque converter lock with turbine torsional damper for low lock-up speeds in 1st through 8th gear	
Gear Ratios		
1st	4.71	
2nd 	3.14	
3rd 	2.10	
4th 	1.67	
5th 	1.29	
6th 	1.00	
7th 	0.84	
8th 	0.67	
Reverse 	3.30	
Final Drive and Overall Top Gear Ratios	2.15 with 3.21 axle; 2.38 with 3.55 axle	
Max Torque	332 lb.-ft. 	
		
TRANSMISSION: ZF 8HP70 AUTOMATIC EIGHT-SPEED WITH ELECTRONIC RANGE SELECT (ERS)	
Availability	Available with select 5.7-litre V8 equipped trucks (late availability)	
Description	Adaptive electronic control, automatic or ERS manual control. Five clutch-pack design with only two open clutches in any gear. Torque converter lock with turbine torsional damper for low lock-up speeds in 1st through 8th gear	

Gear Ratios		
1st	4.71	
2nd	3.14	
3rd	2.10	
4th	1.67	
5th	1.29	
6th	1.00	
7th	0.84	
8th	0.67	
Reverse	3.30	
Final Drive and Overall Top Gear Ratios	2.15 with 3.21 axle; 2.38 with 3.55 axle; 2.63 with 3.92 axle	
Max Torque	516 lb.-ft. 	
		
TRANSFER CASE: BW 44-45 PART-TIME		
Availability	3.6-litre V6 4x4, 4.7-litre V8 4x4 and 5.7-litre V8 4x4	
Shift Mechanism	Electric	
Available Speeds	2-speed	
Operating Modes	2WD High; 4WD High, Locked; Neutral; 4WD Low, Locked	
Low-range Ratio	2.64	
Centre Differential Type	None	
		
TRANSFER CASE: BW 44-44 ON-DEMAND		
Availability	5.7-litre V8 4x4 	
Shift Mechanism	Electric	
Available Speeds	2-speed	
Operating Modes	2WD High; 4WD Auto; 4WD High, Locked; Neutral; 4WD Low, Locked	
Low-range Ratio	2.64	
Centre Differential Type	None	
		
AXLES		
Front	ZF 215MM 	
Rear	C235MM (available limited slip)	
Available Ratios	3.21, 3.55, 3.92, 4.10	
		
ELECTRICAL SYSTEM		
Architecture	Powernet	
Alternator	160-amp, 180-amp, 220-amp (Stop-start only)	
Battery	Group 65, low-maintenance 730 CCA (Stop-start features 800 CCA Absorbed Glass Mat)	
SUSPENSION		
Front
	Upper and lower “A” arms, coil springs, twin-tube shock absorbers, stabilizer bar. Optional air suspension replaces twin-tube shock absorbers and coil springs	
Rear
	Five-link with track bar, coil springs, stabilizer bar, twin-tube shock absorbers, solid axle. Optional air suspension replaces twin-tube shock absorbers and coil springs	
		
STEERING		
Power-assist	Electric power steering	

Regular Cab	2WD	2WD	4WD	4WD	
Box Length	Short box	Long Box	Short Box	Long Box	
Wheelbase (nominal) 	3061 (120.5) 	3569.2 (140.5) 	3569.2 (140.5) 	3569.2 (140.5) 	
Overall Steering Ratio 	19.1:1	17.9:1	19.1:1	17.9:1	
Steering Wheel Turns (lock-to-lock)	3.5	3.3	3.5	3.3	
Turning Diameter – 17-in. Tire –m (ft.)(a)	12.0 (39.5) 	13.7 (45.1) 	12.1 (39.8) 	13.8 (45.4) 	
Turning Diameter – 20-in. Tire - m (ft.)(a)	12.0 (39.3) 	13.7 (44.9) 	12.1 (39.8) 	13.9 (45.5) 	
Turning Diameter – 17-in. Outdoorsman
Tire – m (ft.)(a)	N/A	N/A	12.0 (39.4) 	13.7 (45.0) 	
					
Quad Cab		2WD		4WD	
Box Length		Long Box		Long Box	
Wheelbase (nominal)		3569.2 (140.5) 		3569.2 (140.5) 	
Overall Steering Ratio 		17.9:1		17.9:1	
Steering Wheel Turns (lock-to-lock)		3.3		3.3	
Turning Diameter – 17-in. Tire –m (ft.)(a)		13.7 (45.1) 		13.8 (45.4) 	
Turning Diameter – 20-in. Tire - m (ft.)(a)		13.7 (44.9) 		13.9 (45.5) 	
Turning Diameter – 17-in. Outdoorsman
Tire – m (ft.)(a)		13.7 (44.8) 		13.7 (45.0) 	
					
Crew Cab	2WD	2WD	4WD	4WD	
Box Length	Short box	Long Box (1)	Short Box	Long Box (1)	
Wheelbase (nominal)	3061 (140.5) 	3569.2 (149.5) 	3569.2 (140.5) 	3569.2 (149.5) 	
Overall Steering Ratio 	19.1:1	17.9:1	19.1:1	17.9:1	
Steering Wheel Turns (lock-to-lock)	3.5	3.3	3.5	3.3	
Turning Diameter – 17-in. Tire –m (ft.)(a)	12.0 (39.5) 	13.7 (45.1) 	12.1 (39.8) 	13.8 (45.4) 	
Turning Diameter – 20-in. Tire - m (ft.)(a)	12.0 (39.3) 	13.7 (44.9) 	12.1 (39.8) 	13.9 (45.5) 	
Turning Diameter – 17-in. Outdoorsman
Tire – m (ft.)(a)	N/A	N/A	12.0 (39.4) 	13.7 (45.0) 	
(1) Late Availability					

CHASSIS		
Layout	Longitudinal, front engine (optional transfer case)	
Construction	Ladder-type frame, steel cab, double-wall steel pickup box	
		
BRAKES		
Front
	Size and Type 13.2 in. x 1.1 in. (336 mm x 28 mm) vented disc 
with 2.13 in. (54 mm) two-piston pin-slider caliper and ABS
Swept Area 292 sq. in. (1884 sq. cm)	
Rear	Size and Type 13.8 in. x 0.87 in. (352 mm x 22 mm) disc 
with 2.13 in. (54 mm) single-piston pin-slider caliper and ABS
Swept Area 274 sq. in. (1768 sq. cm)	
Power-assist	Dual-rate, tandem diaphragm vacuum	

DIMENSIONS AND CAPACITIES

Regular Cab Pickup	
Model – Tire Size 	2WD –265/70R17	4WD –265/70R17	
Box Length 	6ft. 4in.	8ft.	6ft. 4in.	8ft.	
Wheelbase (nominal)	3061.2 (120.5) 	3569.2 (140.5) 	3062.5 (120.5) 	3570.2 (140.5) 	
Track, Front 	1728.2 (68.0) 	1728.2 (68.0) 	1732.3 (68.2) 	1732.3 (68.2) 	
Track, Rear 	1714.7 (67.5) 	1714.7 (67.5) 	1714.7 (67.5) 	1714.7 (67.5)	
Overall Length 	5308.5 (209.0) 	5866.5 (231.0) 	5308.5 (209.0)	5866.5 (231.0)	
Overall Width 	2017.4 (79.4) 	2017.4 (79.4)	2017.4 (79.4)	2017.4 (79.4)	
Overall Height 	1894.2 (74.6) 	1889.2 (74.4) 	1910.4 (75.2) 	1906.2 (75.0) 	
Ground Clearance	
Front Axle 	229.3 (9.0)  	229.3 (9.0)	232.6 (9.2) 	232.7 (9.2) 	
Rear Axle 	221.2 (8.7)  	221.5 (8.7) 	219.2 (8.6) 	219.5 (8.6) 	
Open Tailgate to Ground 	883.4 (34.8) 	878.3 (34.6) 	889.6 (35.0) 	885.3 (34.9) 	
Pickup Body Height 	511.1 (20.1) 	513.0 (20.2) 	511.1 (20.1) 	513.0 (20.2) 	
Approach Angle (degrees) 	15.6	15.7	17.7	17.8	
Departure Angle (degrees)	25.2	24.1	25.6	24.4	
Ramp Breakover Angle (degrees) 	21.5	19.2	22.9	20.5	
Fuel-Tank Capacity 	98-litre 
(Standard)	121-litre
(Standard)	98-litre
(Standard)	121-litre
(Standard)	

Quad Cab 6-ft. 4-in. Box Pickup	
Model – Tire Size 	2WD –265/70R17	4WD –265/70R17	
Wheelbase (nominal)	3569.2 (140.5) 	3570.2 (140.5) 	
Track, Front 	1728.2 (68.0) 	1732.3 (68.2) 	
Track, Rear 	1714.7 (67.5) 	1714.7 (67.5) 	
Overall Length 	5816.5 (229.0) 	5816.5 (229.0) 	
Overall Width 	2017.4 (79.4) 	2017.4 (79.4) 	
Overall Height 	1960.2 (77.2) 	1974.8 (77.7) 	
Ground Clearance	
Front Axle 	229.2 (9.0) 	232.7 (9.2) 	
Rear Axle 	221.5 (8.7) 	219.5 (8.6) 	
Open tailgate to ground 	878.3 (34.6) 	885.3 (34.9) 	
Pickup Body Height 	511.1 (20.1) 	511.1 (20.1) 	
Approach Angle (degrees)	15.7	17.8	
Departure Angle (degrees)	25.1	25.4	
Ramp Breakover Angle (degrees)	19.2	20.5	
Fuel-Tank Capacity	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	

Quad Cab 6ft. 4in. Box Pickup – Outdoorsman	
Model – Tire Size 	2WD –275/60R20	4WD –275/60R20	
Wheelbase (nominal)	3569.4 (140.5) 	3573.5 (140.7) 	
Track, Front	1742.2 (68.6) 	1743.2 (68.6) 	
Track, Rear 	1727.4 (68.0) 	1727.4 (68.0) 	
Overall Length	5816.5 (229.0) 	5816.5 (229.0) 	
Overall Width 	2017.4 (79.4) 	2017.4 (79.4) 	
Overall Height	1979.4 (77.9) 	2001.6 (78.8) 	
Ground Clearance	
Front Axle 	244.8 (9.6) 	248.6 (9.8) 	
Rear Axle 	237.0 (9.3) 	233.2 (9.2) 	
Open tailgate to ground 	887.7	903.5	
Pickup Body Height 	511.1 (20.1) 	511.1 (20.1)	
Approach Angle (degrees)	21.3	23.9	
Departure Angle, (degrees)	21.4 	22.1	
Ramp Breakover Angle (degrees)	20.9	18.8	
Ground Clearance without Skid Plate	261.5 (10.3) 	NA	
Ground Clearance with Skid Plate	NA	252.2 (9.9) 	
Fuel-Tank Capacity	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre Optional)	

Quad Cab 6ft. 4in. Box Pickup - Air Suspension 4x2 and 4x4	
Tire Size 	265/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal) 	3569.4 (140.5) 	3569.4 (140.5) 	3569.4 (140.5) 	3569.4 (140.5) 	
Track, Front 	1728.2 (68.0) 	1728.2 (68.0) 	1728.2 (68.0) 	1728.2 (68.0)	
Track, Rear 	1714.7 (67.5) 	1714.7 (67.5) 	1714.7 (67.5) 	1714.7 (67.5)	
Overall Length 	5816.5 (229.0) 	5816.5 (229.0)	5816.5 (229.0)	5816.5 (229.0)	
Overall Width 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4) 	
Overall Height 	1909.0 (75.2) 	1962.0 (77.2) 	1986.6 (78.2) 	2013.0 (79.2) 	
Ground Clearance	
Front Axle 	232.3 (9.1) 	232.3 (9.1)	232.3 (9.1)	232.3 (9.1)	
Rear Axle 	220.0 (8.7) 	220.0 (8.7) 	220.0 (8.7)	220.0 (8.7)	
Open Tailgate to Ground 	832.8 (32.8) 	871.2 (34.3) 	889.6 (35.0) 	922.2 (36.3) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0)	
Approach Angle (degrees) 	13.8	18.3	20.9	22.5	
Departure Angle (degrees)	23.0	24.8	25.6	27.1	
Ramp Breakover Angle (degrees) 	15.9	19.4	21.4	23.0	
Ground Clearance without Skid Plate	171.0 (6.7) 	223.5 (8.8) 	254 (10.0) 	274.3 (10.8) 	
Ground Clearance with Skid Plate	153.1 (6.0) 	205.7 (8.1) 	236.2 (9.3) 	256.5 (10.1) 	
Fuel-Tank Capacity 	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre  (Standard)
121-litre (Optional)	98-litre  (Standard)
121-litre  (Optional)	

Quad Cab 6ft. 4in. Box Pickup - Air Suspension 4x2 and 4x4	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)	3569.4 (140.5) 	3569.4 (140.5) 	3569.4 (140.5) 	3569.4 (140.5) 	
Track, Front 	1742.2 (68.6) 	1742.2 (68.6) 	1742.2 (68.6) 	1742.2 (68.6)	
Track, Rear 	1727.4 (68.0) 	1727.4 (68.0)	1727.4 (68.0)	1727.4 (68.0)	
Overall Length 	5816.5 (229.0) 	5816.5 (229.0) 	5816.5 (229.0) 	5816.5 (229.0) 	
Overall Width 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4) 	
Overall Height 	1924.4 (75.8) 	1977.4 (77.8) 	2002.0 (78.8) 	2028.4 (79.9) 	
Ground Clearance	
Front Axle 	248.5 (9.8) 	248.5 (9.8) 	248.5 (9.8) 	248.5 (9.8) 	
Rear Axle 	235.0 (9.3) 	235.0 (9.3) 	235.0 (9.3) 	235.0 (9.3) 	
Open Tailgate to Ground 	847.2 (33.4) 	885.7 (34.9) 	904.1 (35.6) 	936.7 (36.9) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	
Approach Angle (degrees) 	15.2	19.8	22.4	23.9	
Departure Angle (degrees)	23.7	25.5	26.4	27.8	
Ramp Breakover Angle (degrees) 	17.1	20.6	22.5	24.2	
Ground Clearance without Skid Plate	187.2 (7.4)	239.8 (9.4) 	269.5 (10.6) 	290.8 (11.4) 	
Ground Clearance with Skid Plate	169.3 (6.7)	222.8 (8.8) 	252.8 (9.9) 	273.7 (10.8) 	
Fuel-Tank Capacity 	98-litre  (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	

Quad Cab 6ft. 4in. Box Pickup - Air Suspension 4x2 and 4x4 Outdoorsman	
Tire Size 	265/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal) 	3569.4 (140.5) 	3569.4 (140.5) 	3569.4 (140.5) 	3569.4 (140.5) 	
Track, Front 	1728.2 (68.0) 	1728.2 (68.0)	1728.2 (68.0)	1728.2 (68.0)	
Track, Rear 	1714.7 (67.5) 	1714.7 (67.5)	1714.7 (67.5)	1714.7 (67.5)	
Overall Length 	5816.5 (229.0) 	5816.5 (229.0)	5816.5 (229.0)	5816.5 (229.0)	
Overall Width 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4)	2017.4 (79.4)	
Overall Height 	1909.0 (75.2) 	1962.0 (77.2) 	1986.6 (78.2) 	2013.0 (79.2) 	
Ground Clearance	
Front Axle 	232.3 (9.1) 	232.3 (9.1)	232.3 (9.1)	232.3 (9.1)	
Rear Axle 	220.0 (8.7) 	220.0 (8.7) 	220.0 (8.7)	220.0 (8.7)	
Open Tailgate to Ground 	832.8 (32.8) 	871.2 (34.3) 	889.6 (35.0) 	922.2 (36.3) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0)	508.6 (20.0)	508.6 (20.0)	
Approach Angle (degrees) 	15.2	19.7	21.8	22.9	
Departure Angle (degrees)	18.7	20.6	21.4	22.9	
Ramp Breakover Angle without Skid Plate 	15.9	19.4	21.4	23.0	
Ramp Breakover Angle, with Skid Plate 	12.7	15.9	17.6	19.2	
Ground Clearance without Skid Plate	171.0 (6.7) 	223.5 (8.8) 	254 (10.0) 	274.3 (10.8) 	
Ground Clearance with Skid Plate	153.1 (6.0) 	205.7 (8.1) 	236.2 (9.3) 	256.5 (10.1) 	
Fuel-Tank Capacity 	98-litre (Standard)
121litre (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	

Quad Cab 6ft. 4in. Box Pickup - Air Suspension 4x2 and 4x4 Outdoorsman	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal) 	3569.4 (140.5) 	3569.4 (140.5)	3569.4 (140.5)	3569.4 (140.5)	
Track, Front 	1742.2 (68.6) 	1742.2 (68.6)	1742.2 (68.6)	1742.2 (68.6)	
Track, Rear 	1727.4 (68.0) 	1727.4 (68.0)	1727.4 (68.0)	1727.4 (68.0)	
Overall Length 	5816.5 (229.0) 	5816.5 (229.0)	5816.5 (229.0)	5816.5 (229.0)	
Overall Width 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4)	2017.4 (79.4)	
Overall Height 	1924.4 (75.8) 	1977.4 (77.8) 	2002.0 (78.8) 	2028.4 (79.9) 	
Ground Clearance	
Front Axle 	248.5 (9.8) 	248.5 (9.8)	248.5 (9.8)	248.5 (9.8)	
Rear Axle 	235.0 (9.3) 	235.0 (9.3) 	235.0 (9.3)	235.0 (9.3)	
Open Tailgate to Ground 	847.2 (33.4) 	885.7 (34.9) 	904.1 (35.6) 	936.7 (36.9) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0)	508.6 (20.0)	508.6 (20.0)	
Approach Angle (degrees) 	16.6	20.9	22.9	24.0	
Departure Angle (degrees)	19.4	21.3	22.2	23.6	
Ramp Breakover Angle without Skid Plate	17.1	20.6	22.5	24.2	
Ramp Breakover Angle with Skid Plate	13.8	17.0	18.7	20.3	
Ground Clearance without Skid Plate	187.2 (7.4)	239.8 (9.4) 	269.5 (10.6) 	290.8 (11.4) 	
Ground Clearance with Skid Plate	169.3 (6.7)	222.8 (8.8) 	252.8 (9.9) 	273.7 (10.8) 	
Fuel-Tank Capacity 	98-litre (Standard)
121-litre (Optional)	(98-litre) (Standard)
121-litre (Optional)	98-litre (Standard)
(121-litre) (Optional)	98-litre (Standard)
121-litre  (Optional)	

Crew Cab Pickup	
Model – Tire Size 	2WD –265/70R17	4WD –265/70R17	
Box Length 	5ft. 7in.	6ft. 4in.	5ft. 7in.	6ft. 4in.	
Wheelbase (nominal)	3569.2 (140.5) 	3795.3 (149.4) 	3570.2 (140.5) 	3795.2 (149.4) 	
Track, Front 	1728.2 (68.0) 	1728.2 (68.0)	1732.3 (68.2) 	1732.3 (68.2) 	
Track, Rear 	1714.7 (67.5) 	1714.7 (67.5)	1714.7 (67.5)	1714.7 (67.5)	
Overall Length 	5816.5 (229.0)	6042.6 (237.9) 	5816.5 (229.0)	6042.6 (237.9) 	
Overall Width 	2017.4 (79.4) 	2016.6 (79.4) 	2017.4 (79.4)	2016.6 (79.4)	
Overall Height 	1953.8 (76.9) 	1950.6 (76.8) 	1967.9 (77.5) 	1965.1 (77.4) 	
Ground Clearance	
Front Axle 	229.2 (9.0) 	231.1 (9.1) 	232.7 (9.2) 	235.2 (9.2) 	
Rear Axle 	221.5 (8.7) 	220.5 (8.7) 	219.5 (8.6) 	218.3 (8.6) 	
Open Tailgate to Ground 	878.3 (34.6) 	874.0 (34.4) 	885.3 (34.9) 	880.8 (34.7)  	
Pickup Body Height 	508.6 (20.0) 	511.1 (20.1) 	508.6 (20.0)	511.1 (20.1)	
Approach Angle (degrees) 	15.7	16.0	17.8	18.0	
Departure Angle (degrees)	25.1	24.9	24.7	25.2	
Ramp Breakover Angle (degrees) 	19.2	18.5	20.5	19.7	
Fuel-Tank Capacity 	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	

Crew Cab Pickup - Outdoorsman	
Model – Tire Size 	2WD –275/60R20	4WD –275/60R20	
Box Length 	5ft. 7in.	6ft. 4in.	5ft. 7in.	6ft. 4in.	
Wheelbase (nominal)	3569.4 (140.5) 	3795.8 (149.4) 	3573.5 (140.7) 	3799.6 (149.6) 	
Track, Front 	1742.2 (68.6) 	1742.2 (68.6)	1742.2 (68.6)	1742.2 (68.6)	
Track, Rear 	1727.4 (68.0) 	1727.4 (68.0)	1727.4 (68.0)	1727.4 (68.0)	
Overall Length 	5816.5 (229.0) 	6042.6 (237.9) 	5816.5 (229.0)	6042.6 (237.9)	
Overall Width 	2017.4 (79.4) 	2016.6 (79.4) 	2017.4 (79.4)	2016.6 (79.4)	
Overall Height 	1972.3 (77.6) 	1968.1 (77.5) 	1994.1 (78.5) 	1991.7 (78.4) 	
Ground Clearance	
Front Axle 	244.8 (9.6) 	243.6 (9.6) 	248.6 (9.8) 	248.0 (9.8) 	
Rear Axle 	237.0 (9.3) 	235.0 (9.3) 	233.2 (9.2) 	233.1 (9.2) 	
Open Tailgate to Ground 	887.7 (34.9) 	883.9 (34.8) 	903.5 (35.6) 	902.3 (35.5) 	
Pickup Body Height 	508.6 (20.0) 	511.1 (20.1) 	508.6 (20.0) 	511.1 (20.1) 	
Approach Angle (degrees) 	21.3	21.0	23.9	22.9	
Departure Angle (degrees)	21.4	21.2	22.1	22.1	
Ramp Breakover Angle (degrees) 	20.9	19.9	18.8	17.6	
Ground Clearance without Skid Plate	261.5 (10.3) 	261.0 (10.3) 	NA	NA	
Ground Clearance with Skid Plate	NA	NA	252.2 (9.9) 	251.6 (9.9) 	
Fuel-Tank Capacity 	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	

Crew Cab 5ft. 7in. Box Pickup - Air Suspension 4x2 and 4x4	
Tire Size 	265/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal) 	3569.4 (140.5) 	3569.4 (140.5)	3569.4 (140.5)	3569.4 (140.5)	
Track, Front 	1728.2 (68.0) 	1728.2 (68.0)	1728.2 (68.0)	1728.2 (68.0)	
Track, Rear 	1714.7 (67.5) 	1714.7 (67.5)	1714.7 (67.5)	1714.7 (67.5)	
Overall Length 	5816.5 (229.0) 	5816.5 (229.0)	5816.5 (229.0)	5816.5 (229.0)	
Overall Width 	2017.4 (79.4) 	2017.4 (79.4)	2017.4 (79.4)	2017.4 (79.4)	
Overall Height 	1902.1 (74.9) 	1955.1 (77.0) 	1979.2 (77.9) 	2006.1 (79.0) 	
Ground Clearance	
Front Axle 	232.3 (9.1) 	232.3 (9.1)	232.3 (9.1)	232.3 (9.1)	
Rear Axle 	220.0 (8.7) 	220.0 (8.7)	220.0 (8.7)	220.0 (8.7)	
Open Tailgate to Ground 	832.8 (32.8) 	871.2 (34.3) 	889.6 (35.0) 	922.2 (36.3) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0)	508.6 (20.0)	
Approach Angle (degrees) 	13.8	18.3	20.9	22.5	
Departure Angle (degrees)	23.0	24.8	25.6	27.1	
Ramp Breakover Angle (degrees) 	15.9	19.4	21.4	23.0	
Ground Clearance without Skid Plate	171.0 (6.7) 	223.5 (8.8) 	254 (10.0) 	274.3 (10.8) 	
Ground Clearance with Skid Plate	153.1 (6.0) 	205.7 (8.1) 	236.2 (9.3) 	256.5 (10.1) 	
Fuel-Tank Capacity 	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (32-gal.) (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	

Crew Cab 5ft. 7in. Box Pickup - Air Suspension 4x2 and 4x4	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)	3569.4 (140.5) 	3569.4 (140.5) 	3569.4 (140.5) 	3569.4 (140.5)	
Track, Front 	1742.2 (68.6) 	1742.2 (68.6) 	1742.2 (68.6) 	1742.2 (68.6) 	
Track, Rear 	1727.4 (68.0) 	1727.4 (68.0)	1727.4 (68.0)	1727.4 (68.0)	
Overall Length 	5816.5 (229.0) 	5816.5 (229.0)	5816.5 (229.0)	5816.5 (229.0)	
Overall Width 	2017.4 (79.4) 	2017.4 (79.4)	2017.4 (79.4)	2017.4 (79.4)	
Overall Height 	1917.4 (75.5) 	1970.4 (77.6) 	1994.5 (78.5) 	2021.4 (79.6) 	
Ground Clearance	
Front Axle 	248.5 (9.8) 	248.5 (9.8)	248.5 (9.8)	248.5 (9.8)	
Rear Axle 	235.0 (9.3) 	235.0 (9.3)	235.0 (9.3)	235.0 (9.3)	
Open Tailgate to Ground 	847.2 (33.4) 	885.7 (34.9) 	904.1 (35.6) 	936.7 (36.9) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0)	508.6 (20.0)	508.6 (20.0)	
Approach Angle (degrees) 	15.2	19.8	22.4	23.9	
Departure Angle (degrees)	23.7	25.5	26.4	27.8	
Ramp Breakover Angle (degrees) 	17.1	20.6	22.5	24.2	
Ground Clearance without Skid Plate	187.2 (7.4)	239.8 (9.4) 	269.5 (10.6) 	290.8 (11.4) 	
Ground Clearance with Skid Plate	169.3 (6.7)	222.8 (8.8) 	252.8 (9.9) 	273.7 (10.8) 	
Fuel-Tank Capacity 	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	

Crew Cab 5ft. 7in. Box Pickup - Air Suspension 4x2 and 4x4 Outdoorsman	
Tire Size 	265/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal) 	3569.4 (140.5) 	3569.4 (140.5) 	3569.4 (140.5) 	3569.4 (140.5) 	
Track, Front 	1728.2 (68.0) 	1728.2 (68.0) 	1728.2 (68.0) 	1728.2 (68.0) 	
Track, Rear 	1714.7 (67.5) 	1714.7 (67.5) 	1714.7 (67.5) 	1714.7 (67.5) 	
Overall Length 	5816.5 (229.0) 	5816.5 (229.0) 	5816.5 (229.0) 	5816.5 (229.0) 	
Overall Width 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4) 	
Overall Height 	1902.1 (74.9) 	1955.1 (77.0) 	1979.2 (77.9) 	2006.1 (79.0) 	
Ground Clearance	
Front Axle 	232.3 (9.1) 	232.3 (9.1) 	232.3 (9.1) 	232.3 (9.1) 	
Rear Axle 	220.0 (8.7) 	220.0 (8.7) 	220.0 (8.7) 	220.0 (8.7) 	
Open Tailgate to Ground 	832.8 (32.8) 	871.2 (34.3) 	889.6 (35.0) 	922.2 (36.3) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0)	508.6 (20.0)	508.6 (20.0)	
Approach Angle (degrees) 	15.2	19.7	21.8	22.9	
Departure Angle (degrees)	18.7	20.6	21.4	22.9	
Ramp Breakover Angle without Skid Plate	15.9	19.4	21.4	23.0	
Ramp Breakover Angle with Skid Plate	12.7	15.9	17.6	19.2	
Ground Clearance without Skid Plate	171.0 (6.7) 	 223.5 (8.8) 	254 (10.0) 	274.3 (10.8) 	
Ground Clearance with Skid Plate	153.1 (6.0) 	205.7 (8.1) 	236.2 (9.3) 	256.5 (10.1) 	
Fuel-Tank Capacity 	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	

Crew Cab 5ft. 7in. Box Pickup - Air Suspension 4x2 and 4x4 Outdoorsman	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal) 	3569.4 (140.5) 	3569.4 (140.5) 	3569.4 (140.5) 	3569.4 (140.5) 	
Track, Front 	1742.2 (68.6) 	1742.2 (68.6) 	1742.2 (68.6) 	1742.2 (68.6) 	
Track, Rear 	1727.4 (68.0) 	1727.4 (68.0) 	1727.4 (68.0) 	1727.4 (68.0) 	
Overall Length 	5816.5 (229.0) 	5816.5 (229.0) 	5816.5 (229.0) 	5816.5 (229.0) 	
Overall Width 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4) 	
Overall Height 	1917.4 (75.5) 	1970.4 (77.6) 	1994.5 (78.5) 	2021.4 (79.6) 	
Ground Clearance	
Front Axle 	248.5 (9.8) 	248.5 (9.8) 	248.5 (9.8) 	248.5 (9.8) 	
Rear Axle 	235.0 (9.3) 	235.0 (9.3) 	235.0 (9.3) 	235.0 (9.3) 	
Open Tailgate to Ground 	847.2 (33.4) 	885.7 (34.9) 	904.1 (35.6) 	936.7 (36.9) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0)	508.6 (20.0)	508.6 (20.0)	
Approach Angle (degrees) 	16.6	20.9	22.9	24.0	
Departure Angle (degrees)	19.4	21.3	22.2	23.6	
Ramp Breakover Angle without Skid Plate	17.1	20.6	22.5	24.2	
Ramp Breakover Angle with Skid Plate	13.8	17.0	18.7	20.3	
Ground Clearance without Skid Plate	187.2 (7.4)	239.8 (9.4) 	269.5 (10.6) 	290.8 (11.4) 	
Ground Clearance with Skid Plate	169.3 (6.7)	222.8 (8.8) 	252.8 (9.9) 	273.7 (10.8) 	
Fuel-Tank Capacity 	98-litre (Standard)
121-litre (Optional)	98-litre  (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	

Crew Cab 6ft. 4in. Box Pickup - Air Suspension 4x2 and 4x4	
Tire Size 	265/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal) 	3798.0 (149.50 	3798.0 (149.50 	3798.0 (149.50 	3798.0 (149.50 	
Track, Front 	1728.2 (68.0) 	1728.2 (68.0) 	1728.2 (68.0) 	1728.2 (68.0) 	
Track, Rear 	1714.7 (67.5) 	1714.7 (67.5) 	1714.7 (67.5) 	1714.7 (67.5) 	
Overall Length 	6042.6 (237.9) 	6042.6 (237.9) 	6042.6 (237.9) 	6042.6 (237.9) 	
Overall Width 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4) 	
Overall Height 	1897.7 (74.7) 	1950.7 (76.8) 	1975.2 (77.8) 	2001.7 (78.8) 	
Ground Clearance	
Front Axle 	231.6 (9.1)	 231.6 (9.1) 	 231.6 (9.1) 	 231.6 (9.1) 	
Rear Axle 	217.7 (8.6) 	217.7 (8.6) 	217.7 (8.6) 	217.7 (8.6) 	
Open Tailgate to Ground 	827.9 (32.6) 	866.6 (34.1) 	885.2 (34.8) 	917.6 (36.1) 	
Pickup Body Height 	511.1 (20.1) 	511.1 (20.1)	511.1 (20.1)	511.1 (20.1)	
Approach Angle (degrees) 	13.8	18.3	20.9	22.5	
Departure Angle (degrees)	22.8	24.6	25.5	26.9	
Ramp Breakover Angle (degrees) 	15.3	18.7	20.5	22.2	
Ground Clearance without Skid Plate	170.0 (6.7) 	222.7 (8.8) 	252.4 (9.9) 	273.7 (10.8) 	
Ground Clearance with Skid Plate	152.3 (6.0) 	205.4 (8.1) 	235.4 (9.3) 	256.4 (10.1) 	
Fuel-Tank Capacity 	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre  (Optional)	98-litre  (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	

Crew Cab 6ft. 4in. Box Pickup - Air Suspension 4x2 and 4x4 	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)	3798.0 (149.5) 	3798.0 (149.5) 	3798.0 (149.5) 	3798.0 (149.5) 	
Track, Front 	1742.2 (68.6) 	1742.2 (68.6) 	1742.2 (68.6) 	1742.2 (68.6) 	
Track, Rear 	1727.4 (68.0) 	1727.4 (68.0) 	1727.4 (68.0) 	1727.4 (68.0) 	
Overall Length 	6042.6 (237.9) 	6042.6 (237.9) 	6042.6 (237.9) 	6042.6 (237.9) 	
Overall Width 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4) 	
Overall Height 	1914.5 (75.4) 	1967.5 (77.5) 	1991.9 (78.4) 	2018.5 (79.5) 	
Ground Clearance	
Front Axle 	247.9 (9.8) 	247.9 (9.8)	247.9 (9.8)	247.9 (9.8)	
Rear Axle 	234.7 (9.2) 	234.7 (9.2)	234.7 (9.2)	234.7 (9.2)	
Open Tailgate to Ground 	819.5 (32.3) 	883.9 (34.8) 	902.5 (35.5) 	934.9 (36.8) 	
Pickup Body Height 	511.1 (20.1) 	511.1 (20.1) 	511.1 (20.1)	511.1 (20.1)	
Approach Angle (degrees) 	15.5	19.7	22.3	23.9	
Departure Angle (degrees)	22.5	25.5	26.4	27.8	
Ramp Breakover Angle (degrees) 	16.4	19.8	21.7	23.3	
Ground Clearance without Skid Plate	185.8 (7.3) 	239.0 (9.4) 	268.7 (10.6) 	290.0 (11.4) 	
Ground Clearance with Skid Plate	168.8 (6.6) 	221.7 (8.7) 	251.7 (9.9) 	272.7 (10.7) 	
Fuel-Tank Capacity 	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre  (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	

Crew Cab 6ft. 4in. Box Pickup - Air Suspension 4x2 and 4x4 Outdoorsman	
Tire Size 	265/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal) 	3798.0 (149.5)	3798.0 (149.5)	3798.0 (149.5)	3798.0 (149.5)	
Track, Front 	1728.2 (68.0) 	1728.2 (68.0) 	1728.2 (68.0) 	1728.2 (68.0) 	
Track, Rear 	1714.7 (67.5) 	1714.7 (67.5) 	1714.7 (67.5) 	1714.7 (67.5) 	
Overall Length 	6042.6 (237.9) 	6042.6 (237.9) 	6042.6 (237.9) 	6042.6 (237.9) 	
Overall Width 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4) 	
Overall Height 	1897.7 (74.7) 	1950.7 (76.8) 	1975.2 (77.8) 	2001.7 (78.8) 	
Ground Clearance	
Front Axle 	231.6 (9.1) 	231.6 (9.1) 	231.6 (9.1) 	231.6 (9.1) 	
Rear Axle 	217.7 (8.6) 	217.7 (8.6) 	217.7 (8.6) 	217.7 (8.6) 	
Open Tailgate to Ground 	827.9 (32.6) 	866.6 (34.1) 	885.2 (34.8) 	917.6 (36.1) 	
Pickup Body Height 	511.1 (20.1) 	511.1 (20.1)	511.1 (20.1)	511.1 (20.1)	
Approach Angle (degrees) 	15.3	19.7	21.8	22.9	
Departure Angle (degrees)	18.6	20.4	21.3	22.7	
Ramp Breakover Angle without Skid Plate	15.3	18.7	20.5	22.2	
Ramp Breakover Angle with Skid Plate	12.0	15.0	16.6	18.2	
Ground Clearance without Skid Plate	170.0 (6.7) 	222.7 (8.8) 	252.4 (9.9) 	273.7 (10.8) 	
Ground Clearance with Skid Plate	152.3 (6.0) 	205.4 (8.1) 	235.4 (9.3) 	256.4 (10.1) 	
Fuel-Tank Capacity 	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	98-litre (Standard)
121-litre (Optional)	

Crew Cab 6ft. 4in. Box Pickup - Air Suspension 4x2 and 4x4 Outdoorsman 	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal) 	3798.0 (149.5) 	3798.0 (149.5) 	3798.0 (149.5) 	3798.0 (149.5) 	
Track, Front 	1742.2 (68.6) 	1742.2 (68.6) 	1742.2 (68.6) 	1742.2 (68.6) 	
Track, Rear 	1727.4 (68.0) 	1727.4 (68.0) 	1727.4 (68.0) 	1727.4 (68.0) 	
Overall Length 	6042.6 (237.9) 	6042.6 (237.9) 	6042.6 (237.9) 	6042.6 (237.9) 	
Overall Width 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4) 	2017.4 (79.4) 	
Overall Height 	1914.5 (75.4) 	1967.5 (77.5) 	1991.9 (78.4) 	2018.5 (79.5) 	
Ground Clearance	
Front Axle 	247.9 (9.8) 	247.9 (9.8) 	247.9 (9.8) 	247.9 (9.8) 	
Rear Axle 	234.7 (9.2) 	234.7 (9.2) 	234.7 (9.2) 	234.7 (9.2) 	
Open Tailgate to Ground 	819.5 (32.3) 	883.9 (34.8) 	902.5 (35.5) 	934.9 (36.8) 	
Pickup Body Height 	511.1 (20.1) 	511.1 (20.1)	511.1 (20.1)	511.1 (20.1)	
Approach Angle (degrees) 	16.6	20.9	22.9	24.0	
Departure Angle (degrees)	19.4	21.3	22.1	23.6	
Ramp Breakover Angle without Skid Plate	16.4	19.8	21.7	23.3	
Ramp Breakover Angle with Skid Plate	13.0	16.0	17.7	19.2	
Ground Clearance without Skid Plate	185.8 (7.3) 	239.0 (9.4) 	268.7 (10.6) 	290.0 (11.4) 	
Ground Clearance with Skid Plate	168.8 (6.6) 	221.7 (8.7) 	251.7 (9.9) 	272.7 (10.7) 	
Fuel-Tank Capacity 	98-litre (Standard)
121-litre (Optional)	98-litre  (Standard)
121-litre (Optional)	98-litre  (Standard)
121-litre (Optional)	98-litre  (Standard)
121-litre (Optional)	

Cargo Box	
Nominal Box Size 	5 ft 7 in 
(Crew)	6 ft 4 in 
(Regular, Quad, or Crew)	8 ft 
(Regular)	
Volume, L (cu. ft.) 	1424.3 (50.3) 	1628.3 (57.5) 	2015.6 (74.7) 	
Length at Floor, Tailgate Closed 	1712.4 (67.4) 	1938.5 (76.3) 	2496.5 (98.3) 	
Cargo Width 	1686.9 (66.4) 	1686.9 (66.4) 	1686.9 (66.4) 	
Distance Between Wheelhouses 	1295.4 (51) 	1295.4 (51) 	1295.4 (51) 	
Depth  	508.6 (20.0) 	511.1 (20.1) 	513.0 (20.2) 	
Tailgate Opening Width mm (in.) 	1535.3 (60.4) 	1535.3 (60.4) 	1535.3 (60.4) 	

ACCOMMODATIONS	
Model 	Regular Cab	Quad Cab	Crew Cab	
Seating Capacity, F/R 	3/0 or 2/0	3/3 or 2/3	3/3 or 2/3	
Front	
Head Room 	1013.5 (39.9) 	1041.4 (41.0)	1041.4 (41.0)	
Legroom  	1041.4 (41.0) 	1041.4 (41.0)	1041.4 (41.0)	
Shoulder Room 	1676.4 (66.0) 	1676.4 (66.0)	1676.4 (66.0)	
Hip Room 	1598.7 (62.9) 	1605.3 (63.2) 	1605.3 (63.2)	
Seat Travel 	230.0 (9.0) 	230.0 (9.0)	230.0 (9.0)	
Recliner Range (degrees) 	85 (38 rwd, 47 fwd)	56 (38 rwd, 18 fwd)	56 (38 rwd, 18 fwd)	

Rear	
Head Room 	N/A	1008.4 (39.7) 	1013.5 (39.9) 	
Legroom  	N/A	880.9 (34.7)	1023.3 (40.3) 	
Shoulder Room 	N/A	1668.8 (65.7) 	1668.8 (65.7) 	
Hip Room 	N/A	1598.3 (62.9) 	1605.3 (63.2) 	
Interior Volume	
Front – L (cu. ft.) 	1769.8 (62.5) 	1817.9  (64.2) 	1817.9 (64.2) 	
Rear – L (cu. ft.)	N/A	1483.8 (52.4)	1730.2 (61.1) 	

• • •