2013 Ram C/V (Cargo Van)
CANADIAN SPECIFICATIONS

All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions are measured at curb weight with standard wheels and tires unless otherwise noted.
NOTE: Information shown is correct at time of publication and is subject to change. 

GENERAL INFORMATION		
Body Style	Multipurpose vehicle 	
Assembly Plant	Windsor, Ontario	
EnerGuide Vehicle Class	Multipurpose vehicle	
Introduction date	August 2011 as a 2012 model year	
	
ENGINE: 3.6-LITRE, GASOLINE, DOHC, 24-VALVE, V6	
Availability	Standard	
Type and Description	60° bank angle, liquid-cooled, with three-plenum intake manifold, electronically controlled manifold tuning valve and short-runner valves	
Displacement Displacement, cu. cm	3605 	
Bore x Stroke	96 x 83	
Valve System	DOHC, 24 valves, hydraulic, roller finger followers	
Fuel Injection	Sequential, multi-port, electronic	
Construction	High-pressure die-cast A380 aluminum block with iron liners and semi-permanent mould A319 aluminum heads	
Compression Ratio	10.2:1 	
Power 	283 bhp @ 6,400 rpm	
Torque 	260 lb.-ft. @ 4,400 rpm	
Max. Engine Speed	6,800 rpm (electronically limited)	
Fuel Requirement	Unleaded mid-grade, 89 octane (R+M)/2—preferred, 
Unleaded regular, 87 octane (R+M)/2—acceptable	
Oil Capacity, L (qt.)	5.68 (6) with dry filter	
Coolant Capacity, L (qt.)	9.75 (10.3)	
Emission Controls 	Dual catalytic converter, four heated oxygen sensors, electronic EGR, and internal engine features	
2012 EnerGuide Fuel Economy L/100 km (mpg) - City/Hwy	12.2 (23) / 7.9 (36)
	
Assembly Plant	Trenton South Engine Plant, Trenton, Michigan, USA	

TRANSAXLE: 62TE, Automatic Six-Speed Overdrive	
Availability	Standard	
Description	6-speed, adaptive electronic control, electronically modulated torque converter clutch	
Gear Ratios		
1st	4.127	
2nd	2.842	
3rd	2.283	
4th	Upshift – 1.452 WOT kickdown – 1.570 	
5th 	1.0	
6th 	0.690	
Reverse	3.214	
Transfer Ratio	0.95	
Final Drive Ratio	3.16	
Overall Top Gear	2.24	
	
DRIVETRAIN		
Front-wheel Drive	Standard 	
	
ELECTRICAL SYSTEM		
Alternator	160A	
Battery	730 CCA, maintenance-free	
	
DIMENSIONS AND CAPACITIES		
Wheelbase	3078 (121.2) 	
Overhang — Front	961 (37.8) 	
Overhang — Rear	1112 (43.8) 	
Track—Front	1666 (65.6) 	
Track—Rear	1647 (64.8) 	
Overall Length	5151 (202.8) 	
Overall Width	1998 (78.7) 	
Overall Width with Mirrors	2273 (89.5) 	
Overall Height 	1752 (69.0) 	
Liftover Height 	665 (26.2) 	
Cargo Width at Wheelhouse 	1236 (48.7)	
Maximum Cargo Height 	1224 (48.2) 	
Angle of Approach (curb load) (degrees)	13.9°	
Angle of Departure (curb load) (degrees)	20.6°	
Breakover Angle (curb load) (degrees)	14.2°	
Minimum Running Ground Clearance 
(curb load)	163 (6.4)	
Fuel Tank Capacity, L (imp. gal.)	76 (17)	
Gross Vehicle Weight Rating (GVWR), lb. (kg)	2744 (6050)	
Towing Capacity, kg (lb.) (when properly equipped)	1633 (3600)	
Curb Weight, kg (lb.)	2050 (4510)	
Payload, kg (lb.)	818 (1800) 	
Weight Distribution % F/R	56/44	
	
ACCOMMODATIONS		
Seating Capacity — F/I/R	2	
Front		
Head Room	1012 (39.8) 	
Head Room with Sunroof 	946 (37.2) 	
Legroom	1034 (40.7) 	
Shoulder Room	1619 (63.7) 	
Hip Room	485 (58.4) 	
Seat Travel	220 (8.7) 	
Cargo Volume 		
Maximum Cargo Volume, L (cu. ft.)	4089 (144.4) 	
Total Passenger plus Cargo Volume, L (cu. ft.)	5544 (195.8) 	
		
BODY/CHASSIS		
Layout	Transverse front engine, front-wheel drive	
Construction	Unitized steel with hinged front doors; sliding left and right side doors—power available; rear liftgate with gas props—power available	
	
SUSPENSION		
Front	Independent MacPherson strut, coil over gas-charged shock absorbers, stabilizer bar with isolated suspension cradle	
Rear	Twist-beam axle with coil springs, track bar, heavy-duty shock absorbers	
		
STEERING		
Type	Power rack and pinion	
Overall Ratio	14.3:1	
Turning Diameter (curb-to-curb), m (ft.)	11.92  (39.1) 	
Steering Turns (lock-to-lock)	2.90	

BRAKES		
Power Assist Type	All — 204 x 320 (8 x 9) tandem-diaphragm vacuum	
Availability	Standard on all models	
Front		
Size and Type, in. (mm)	11.9 x 1.1 (302 x 28) vented rotors with 66 mm single-piston caliper	
Swept Area (total front), sq. cm (sq. in.)	355 (55.0) 	
Rear		
Size and Type, in. (mm)	12.0 x 0.47 (305 x 12) solid rotors with 42 mm single-piston IPB caliper	
Swept Area (total rear), sq. cm (sq. in.)	350 (54.3)	
Parking Brake Type	Integral parking brake	
Four-wheel Anti-lock brakes	Standard	
Electronic Stability Control 	Standard	
All-speed traction control	Standard	
	
WHEELS	
Availability	Standard	
Type and Material	Steel with painted bolt-on wheelcover	
Size (in.)	16 x 6.5	
	
TIRES		
Availability	Standard	
Size and Type	225/65R16 BSW, All Season	
Model	Yokohama Avid C33	
Revs per km (mile)	473 (762) 	

• • •