2013 Ram 3500, 4500 and 5500 Chassis Cab
CANADIAN SPECIFICATIONS

All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions are measured at curb weight with standard wheels and tires unless otherwise noted.
NOTE: Information shown is correct at time of publication and is subject to change. 
Typical 2013 Ram 3500 Crew Cab Chassis Cab.
Some unique exceptions showing 4500 and 5500 complexity are included.

GENERAL INFORMATION	
Vehicle Type	Chassis Cab: Regular Cab and Crew Cab	
Assembly Plant	Saltillo, Mexico	
Vehicle Class 	Medium Heavy Duty	
Introduction 	2007/2008 Model Year	
	
ENGINE: 5.7-LITRE HEMI® V8	
Availability  	Standard on 3500 	
Type and Description 	Eight-cylinder, 90-degree V-type, liquid-cooled, with variable-valve timing (VVT)	
Displacement — cu.cm (cu.in.)	5654 (343) 	
Bore x Stroke — mm (in.)	99.5 x 90.9 (3.92 x 3.58) 	
Valve System 	Pushrod-operated overhead valves, 16 valves, hydraulic lifters with roller followers	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction 	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio 	9.6:1	
Power 	383 hp @ 5,600 rpm 	
Torque 	400 lb.-ft. @ 4,000 rpm	
Maximum Engine Speed 	5,800 rpm	
Fuel Requirement 	Unleaded mid-grade, 89 octane (R+M)/2 — recommended 
Unleaded regular, 87 octane (R+M)/2 — acceptable	
Oil Capacity — L (qt.)	6.6 (7.0) 	
Coolant Capacity — L (qt.)	17.7 (18.7) 	
Emission Control 	Dual three-way catalytic converters, internal engine features with knock sensors	
	
ENGINE: 6.7-LITRE CUMMINS TURBO DIESEL I-6	
Availability	Optional on 3500, Standard on 4500 and 5500	
Type and Description	Six-cylinder, inline, liquid-cooled, turbocharged, intercooled	
Displacement — cu.cm (cu.in.)	6690 (408)  	
Bore x Stroke — mm (in.)	107 x 124 (4.21 x 4.88) 	
Valve System	OHV, 24 valves, solid lifters	
Fuel Injection	Electronic high-pressure common rail	
Construction	Cast-iron block and head	
Compression Ratio	17.3:1	
Power 	320 hp @ 2,900 rpm	
Torque 	650 lb.-ft. @ 1,600 rpm	
Maximum Engine Speed	3,000 rpm	
Fuel Requirement	Ultra-low sulfur diesel	
Oil Capacity — L(qt.)	(Low ash req.) 11.3 (12) with filter	
Coolant Capacity — L(qt.)	30.9 (32.7) 	
Emission Controls	Selective Catalytic Reduction (SCR)		
	
ENGINE: 6.7-LITRE HIGH OUTPUT CUMMINS TURBO DIESEL I-6 	
Availability	Optional on 3500, Standard on 4500 and 5500	
Type and Description	Six-cylinder, inline, liquid-cooled, turbocharged, intercooled	
Displacement — cu.cm (cu.in.)	6690 (408)  	
Bore x Stroke — mm. (in.)	107 x 124 (4.21 x 4.88) 	
Valve System	OHV, 24 valves, solid lifters	
Fuel Injection	Electronic high-pressure common rail	
Construction	Cast-iron block and head	
Compression Ratio	17.3:1	
Power 	325 hp @ 2,900 rpm	
Torque 	750 lb.-ft. @ 1,600 rpm	
Maximum Engine Speed	3,500 rpm	
Fuel Requirement	Ultra-low sulfur diesel	
Oil Capacity — L (qt.)	(Low ash req.) 11.3 (12) with filter	
Coolant Capacity — L (qt.)	30.9 (32.7) 	
Emission Controls	Selective Catalytic Reduction (SCR)		
	
TRANSMISSION: G56 — MANUAL SIX-SPEED OVERDRIVE	
Availability	6.7-litre diesel	
Description	Synchronized in all gears	
Gear Ratios 		
1st	5.94	
2nd	3.28	
3rd	1.98	
4th	1.31	
5th	1.0	
6th	0.74	
Reverse	5.42	
	
TRANSMISSION: 66RFE — AUTOMATIC SIX-SPEED	
Availability	5.7-litre gas	
Description	Three planetary gear sets, one overrunning clutch, full electronic control, electronically controlled converter clutch	
Gear Ratios		
1st	3.23	
2nd	1.84	
3rd	1.41	
4th	1.00	
5th	0.82	
6th	0.63	
Reverse	4.44	
Overall Top Gear 	2.35 with 3.73 axle ratio; 2.58 with 4.10 axle ratio; 2.87 with 4.56 axle ratio	
	
TRANSMISSION: AS69RC — AUTOMATIC Six-SPEED	
Availability	6.7-litre diesel 	
Description	Three planetary gear-sets, one overrunning clutch, full electronic control, electronically controlled converter clutch	
Gear Ratios		
1st	3.75	
2nd	2.0	
3rd	1.34	
4th	1.0	
5th	0.77	
6th	0.63	
Reverse	3.54	
Overall Top Gear 	2.15 with 3.42 axle ratio; 2.35 with 3.73 axle ratio; 2.58 with 4.10 axle ratio	
	
TRANSFER CASES: BW 44-46, BW 44-47	
Availability	Optional on 6.7-litre diesel and 5.7-litre gas	
Type	Part-time - BW 44-47 manual shift and BW 44-46 electric shift	
Operating Modes	2WD; 4WD High; Neutral; 4WD Low	
Low-range Ratio	2.64	
Centre Differential	None	
	
ELECTRICAL SYSTEM	
Alternator		
Rating	160-amp standard with 5.7-litre	
Rating	180-amp included with Snow Plow Prep Package standard with 6.7-litre, optional on 5.7-litre	
Rating	220-amp (optional on 6.7-litre)	
Rating	Dual 220-amp (optional on 6.7-litre)	
		
Battery		
Availability	Standard — gas 3500	
Description	Group 65, maintenance-free, 750 CCA	
Availability	Optional — diesel 3500, standard — 4500 and 5500 	
Description	Dual, Group 65, maintenance-free, 750 CCA	

• • •