2013 Chrysler 300 SRT8®
CANADIAN SPECIFICATIONS 

All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions are measured at curb weight with standard wheels and tires unless otherwise noted.
NOTE: Information shown is correct at time of publication and is subject to change. 

GENERAL INFORMATION	
Body Style	Full-size 	
Assembly Plant	Brampton, Ontario	
EnerGuide Vehicle Class	Full Size	
Introduction Date	Summer 2011 as 2012 model	
		
ENGINE: 6.4-LITRE HEMI® V8 WITH FUELSAVER MDS TECHNOLOGY	
Availability	Standard 	
Type and Description	90-degree V-type, liquid-cooled	
Displacement, cu. cm (cu. in.) 	6,424 (392) 	
Bore x Stroke	103.9 x 94.5 (4.09 x 3.72)	
Valve System	Pushrod-operated overhead valves, 16 valves with sodium-filled exhaust valves and hollow stem intake valves, 
16 conventional hydraulic lifters, all with roller tips	
Fuel Injection	Sequential, multi-port, electronic, returnless; automatic features FuelSaver mode	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.9:1	
Power 	470 bhp at 6,000 rpm	
Torque 	470 lb.-ft. at 4,300 rpm	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Premium 91 octane (R+M)/2 — recommended	
Oil Capacity, L (qt.) 	6.6 (7) 	
Factory Oil Fill 	0W-40 Full Synthetic	
Coolant Capacity, L (qt.) 	13.25 (14) 	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad-heated oxygen sensors and internal engine features	
EnerGuide Fuel Economy
L/100 km (mpg) - City/Hwy	15.0 (19) / 8.7 (32)	
Assembly Plant	Saltillo, Mexico	

TRANSMISSION: W5A580 FIVE-SPEED AUTOMATIC	
Availability	Standard 	
Description	Adaptive electronic control or driver-interactive manual control with Auto/StickTM or paddle controls; with “Track” mode (features performance shifting and gear holding feature combined with “Sport” mode suspension damping rates)	
Gear Ratios		
1st	3.59	
2nd	2.19	
3rd	1.41	
4th	1.00	
5th	0.83	
Reverse	3.16	
Final Drive Ratio	3.06 – Getrag limited-slip differential	
Overall Top Gear	2.54	
		
ELECTRICAL SYSTEM		
Alternator	220-amp	
Battery	H7 case, 730 CCA, maintenance free	
		
DIMENSIONS AND CAPACITIES(a)		
Wheelbase	3052 (120.2) 	
Track, Front	1611 (63.4) 	
Track, Rear	1604 (63.1) 	
Overall Length	5088 (200.33) 	
Overall Width	1886 ( 74.24) 	
Overall Height	1480 (58.26) 	
Frontal Area, L (cu. ft.)	2430 (26.2)	
Ground Clearance (Minimum) 	111 (4.37)–Front 	
Drag Coefficient (Cd)	0.334 	
Curb Weight, kg (lb.)	1980 (4365) 	
Weight Distribution, per cent F/R	54/46	
Fuel Tank Capacity, L (gal.)	72.2 (15.8)	
 (a)All dimensions measured at curb weight with standard tires.	
	
ACCOMMODATIONS		
Seating Capacity, F/R	2/3	
Front		
Head room	981 (38.6) 
938 (36.9) with dual-pane sunroof 	
Legroom	1061 (41.8) 	
Shoulder room	1510 (59.5) 	
Hip room	1428 (56.2) 	
Seat travel	Driver — 270 (10.6) 
Passenger —  220 (8.66)	
Recliner angle range, deg.	Power — 70.7
Manual — 70	
Front row interior volume, L (cu. ft.) 	1573 (55.6) 	
 Rear Seat		
Head room	963 (37.9) 
937 (36.9) with dual-pane sunroof 	
Legroom	1019  (40.1) 	
Knee clearance	99 (3.9) 	
Shoulder room	1465  (57.7)	
Hip room	142 (56.1) 	
Second row interior volume, L (cu. ft.) 	1436  (50.7) 	
Total Interior Volume, L (cu. ft.) 	3010  (106.3) 	
Luggage Compartment Volume, L (cu. ft.) 	462 (16.3) 	
Interior Volume Index, L (cu. ft.) 	3472  (122.6)	
Trunk Liftover Height	30 (768.9) 	
		
BODY		
Layout	Longitudinal front engine, RWD	
Construction	Unitized steel body and aluminum hood	
		
EXHAUST		
Type 	Dual 70mm (2.75-in.) active exhaust with dual 102mm (4-in.) round tips 	
		
SUSPENSION 		
Type	SRT tuned three-mode adaptive damping system: “Auto” mode = sporty but compliant ride; “Sport” mode = firm, maximum handling; “Track” mode = firm, maximum handling plus performance shifting and gear holding feature	
Front 	Independent SLA with high upper “A” arm, coil spring over ADS Bilstein shock absorber, 30 mm. stabilizer bar, lateral and diagonal lower links	
Rear	Five-link independent with coil spring, ADS Bilstein shock absorber and isolated suspension cradle, link type 18 mm. stabilizer bar	
		
STEERING		
Type	SRT tuned rack and pinion with hydraulic power assist	
Overall Ratio	14.4:1	
Steering Turns (lock-to-lock)	2.75	
		
TIRES		
Front and Rear	Standard on 300 SRT8	
Size and type	245/45R20 All-season 	
Mfr. and model	Goodyear Eagle RS-A 2	
Revs per km (mile)	456 (731) 	
		
Front and Rear	Optional on 300 SRT8 	
Size and type	245/45R20 Three-season	
Mfr. and model	Goodyear F1 Supercar	
Revs per km (mile) 	450 (726) 	
		
WHEELS		
Availability 	Standard on 300 SRT8	
Type and material	Fully forged aluminum	
Size (in.)	20 x 9.0	
		
Availability	Optional on 300 SRT8	
Type and material	Fully forged aluminum with Black Vapour chrome finish	
Size (in.)	20 x 9.0	
		
BRAKES		
Front		
Rotor size and type, in. (mm)	14.2 x 1.26 (360 x 32) vented and slotted	
Caliper size and type	44 (1.73) Brembo four-piston fixed with aluminum housing	
Swept area, sq. cm (sq. in.) 	2261 (351)	
Rear		
Rotor size and type, in. (mm)	13.8 x 1.10 (350 x 28) vented and slotted	
Caliper size and type	32 (1.26) Brembo four-piston fixed with aluminum housing	
Swept area, sq. cm (sq. in.) 	2036 (316)	

		• • •