2013 Fiat 500 Abarth
CANADIAN SPECIFICATIONS

All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions are measured at curb weight with standard wheels and tires unless otherwise noted.
NOTE: Information shown is correct at time of publication and is subject to change. 

General Information		
Vehicle Type	Hatchback	
EnerGuide Vehicle Class 	Subcompact	
Assembly Plant	Toluca, Mexico	
Introduction Date	First half of 2012 as a 2012 model	

Engine:  1.4 -LITRE SOHC 16 -VALVE TURBOCHARGED MULTIAIR® INLINE FOUR-CYLINDER	
Availability	Standard —Fiat 500 Abarth	
Type and Description	Inline four-cylinder, liquid-cooled	
Displacement, cu. cm (cu. in.)	1368 (83.48)	
Bore x Stroke 	72.0 x 84.0 (2.83x3.31)	
Valve System	Belt-driven, MultiAir SOHC, 16 valves, hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	Cast-iron block with aluminum-alloy head and aluminum-alloy bedplate	
Compression Ratio	9.8:1	
Maximum Turbo Boost (psi/bar)	18 psi/1.24 bar	
Power 	160 bhp @ 5,500 rpm (117 bhp/L)	
Torque 	170 lb.-ft. @ 2,500-4,000 rpm	
Max. Engine Speed (rpm)	6,500 rpm (electronically limited)	
Fuel Requirement	87 octane (R+M)/2 acceptable 91 octane recommended	
Oil Capacity, L (qt.)	3.8 (4.0) with dry filter	
Coolant Capacity, L (qt.)	4.4 (4.6)	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors and internal engine features 	
Max. Gross Trailer Weight	Not rated for trailer tow	
2012 EnerGuide Fuel Economy
L/100 km (mpg) (City/Hwy) 	7.1 (40 mpg)/5.7 (50 mpg)	
Engine Assembly Plant	Dundee, Michigan, U.S.A.	

Transmission: C510 PERFORMANCE FIVE-SPEED MANUAL	
Availability	Standard on Fiat 500 Abarth	
Description	1st, 2nd gear: Double Cone 3rd, 4th, 5th, gear: Single Cone	
Gear Ratios		
1st	3.909	
2nd	2.238
	
3rd	1.520	
4th	1.156	
5th	0.872	
Reverse	3.909	
Final Drive Ratio	3.353	

Electrical System		
Alternator	120-amp	
Battery	500 CCA, maintenance free	

Dimensions and Capacities(a)		
Wheelbase	2300 (90.6)	
Track — Front	1406.8 (55.4)	
Track — Rear	1397.0 (55.0)	
Overall Length	3667.3 (144.4)	
Overall Width	1627.0 (64.1)
1866.0 (73.5) with side mirrors	
Overall Height	1502.4 (59.2) to antenna base
 1490.3 (58.7) to roof	
Ground Clearance	103.7(4.1)	
Drag Coefficient  (cd.)	0.352 – with 16-inch wheels
0.365 – with 17-inch wheels	
Curb Weight, kg (lb.)	1139 (2512) – 5-MTX	
Weight Distribution, per cent F/R	64/36 – 5-MTX	
Fuel Tank Capacity, L (gal.)	40 (8.8)	
(a) All dimensions measured at curb weight with standard tires.	

Accommodations (Estimated)		
Seating Capacity, F/R	2/2	
Front Seat		
Head Room	989 (38.9)
956 (37.6) with sunroof	
Legroom	1035 (40.7)	
Shoulder Room	1255 (49.4)	
Hip Room	1215 (47.8)	
Seat Travel	Driver—210 (8.2)
Passenger—210 (8.2)	
Front row interior volume, L (cu. ft.)	1282 (45.3)	

Rear Seat		
Head Room	903 (35.5)	
Legroom	805 (31.7)	
Knee Clearance	97 (3.8)	
Shoulder Room	1178 (46.4)	
Hip Room	1083 (42.6)	
Second row interior volume, L (cu. ft.)	855 (30.2) 	
Total Interior Volume, L (cu. ft.)	2404 (84.9) 	
Luggage Compartment Volume, L (cu. ft.)	269 (9.5) 
759 (26.8) with rear seats folded	
Interior Volume Index, L (cu. ft.)	2138 (75.5) 	
Trunk Liftover Height	690.2 (27.2)	
		
BODY		
Layout	Transverse-mounted front engine, front-wheel drive	
Construction	Unitized steel body	
		
SUSPENSION		
Front	MacPherson suspension, coil spring with KONI® Frequency Selective Damping (FSD) twin-tube shock absorbers and stabilizer bar	
Rear	Rear twist-beam axle with coil springs and twin-tube shock absorbers with stabilizer bar	
		
STEERING		
Type	Power rack and pinion with electric power steering (EPS) column	
Overall Ratio	15.5:1	
Turning Diameter (curb-to-curb), m (ft.)	11.45 (37.6)	
Steering Turns (lock-to-lock)	2.3	
		
Tires		
Availability	Standard on Fiat 500 Abarth	
Size and type	195/45R16XL BSW all-season	
Mfr. and model	Pirelli Cinturato P7 A/S	
Revs per km (mile)	560 (901)	
		
Availability	Optional on Fiat 500 Abarth	
Size and type	205/40R17 BSW Three – season	
Mfr. and model	Pirelli P-Zero Nero Three – season	
Revs per km (mile)	545 (877)	
		
Wheels		
Availability	Standard on Fiat 500 Abarth	
Type and material	Cast-aluminum, polished face with dark mineral grey painted pockets	
Size (in.)	16 x 6.5	
		
Availability	Optional on Fiat 500 Abarth	
Type and material	Forged-aluminum painted Hyper Black or optional Gloss White 	
Size (in.)	17 x 7.0	

BRAKES		
Front		
  Rotor size and type	282 x 22 (11.1 x 0.86) vented	
  Caliper size and type	54 (2.12) single-piston with aluminum housing
	
  Swept area, sq. cm (sq. in.)	1244 (193)	
Rear		
  Rotor size and type	240 x 11 (9.4 x 0.4) solid	
  Caliper size and type	34 (1.33) single-piston with aluminum housing	
  Swept area, sq. cm (sq. in.)	984 (153)	

• • •