2014 Chrysler 200
CANADIAN SPECIFICATIONS

Specifications are based on the latest product information available at the time of publication. 
All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Body Style	Four-door sedan 	
Assembly Plant 	Sterling Heights Assembly, Michigan (U.S.A.)	
Vehicle Class 	Mid-size sedan 	
Introduction Date	December 2010	
		
BODY/CHASSIS		
Layout 	Transverse front engine with front-wheel drive 	
Construction 	Steel unibody 	
		
ENGINE: 2.4-LITRE, GASOLINE, DOHC, 16-VALVE, VVT, SMPI I-4    	
Availability	Standard on 200 LX,Touring, Limited models	
Type and Description	Four-cylinder inline, tuned intake manifold with electronic active charge motion control valves with dual counter-rotating balance shafts	
Displacement	2,360 cu. cm (144 cu. in.) 	
Bore x Stroke	88 x 97 (3.46 x 3.82) 	
Valve System	Chain-driven DOHC, 16 valves, electronically controlled dual variable-valve timing (VVT), direct-acting shimless mechanical bucket tappets	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	High-pressure die-cast aluminum block with dry iron liners, cast-aluminum cylinder heads, cast-aluminum ladder frame, forged-steel crankshaft	
Compression 	10.5:1	
Power 	173 bhp  @ 6,000 rpm 	
Torque 	166 lb.-ft. @ 4,400 rpm	
Max. Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity	4.23 litres (4.5 qt.)  	
Coolant Capacity	6.8 litres (7.2 qt.)	
Emission Controls	Single catalytic converter dual heated oxygen sensors and engine features	

2013 EnerGuide Fuel Economy L/100 km (mpg) City/Hwy	10.0 (28)/6.9 (41) with 4-speed automatic
10.6 (27)/6.5 (43) with 6-speed automatic	
		
ENGINE: 3.6-LITRE, GASOLINE, DOHC, 24-VALVE, SMPI V-6	
Availability	Available on 200 Touring,Limited and S models	
Type and Description	60-degree bank angle, liquid-cooled, three-plenum intake manifold with electronically controlled manifold tuning valve and short-runner valves	
Displacement	3605 cu. cm (220 cu. in.)	
Bore x Stroke	96 x 83 mm (3.78 x 3.28) 	
Valve System	DOHC, 24 valves, hydraulic, roller finger followers	
Fuel Injection	Sequential, multiport, electronic	
Construction	High-pressure die-cast A380 aluminum block with iron liners and semi-permanent mould A319 aluminum heads	
Compression Ratio	10.2:1	
Power 	283 bhp @ 6,400 rpm	
Torque 	260 lb.-ft. @ 4,400 rpm	
Max. Engine Speed	6,800 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity	5.7 litres (6 qt.) with dry filter	
Coolant Capacity	9.75 litres (10.3 qt.) 	
Emission Controls	Dual catalytic converters, four heated oxygen sensors, electronic EGR, and internal engine features	
2013 EnerGuide Fuel Economy L/100km (mpg) City/Hwy	11 (26)/6.8(42)	

TRANSAXLE: 40TES, AUTOMATIC FOUR-SPEED OVERDRIVE	
Availability	Standard on 200 LX and touring model	
Description	Four-speed overdrive, adaptive electronic control, electronically modulated converter clutch	
Gear Ratios		
1st 	2.842   	
2nd	1.57    	
3rd	1.00	
4th 	0.69  	
Reverse 	2.21    	
Final Drive Ratio 	3.91 with 2.4-liter engine	
Overall Top Gear	2.69 with 2.4-liter engine	
		
TRANSAXLE: 62TE, AUTOMATIC SIX-SPEED OVERDRIVE	
Availability	Standard on 200 Limited and S models; Available on LX and Touring models 	
Description	Six-speed, adaptive electronic control or Auto Stick driver-interactive manual control and electronically modulated torque converter clutch	
Gear Ratios		
1st	4.127  	
2nd	2.842   	
3rd	2.283     	
4th	1.452   	
5th	1   	
6th 	0.69    	
Reverse	3.214	
Transfer Ratio 	0.95	
Final Drive Ratio	3.16 with 3.6-litre engine, 3.43 with 2.4-litre engine	
Overall Top Gear 	2.06 with 3.6-litre engine, 2.24 with 2.4-litre engine	
		
SUSPENSION		
Front	Independent MacPherson strut, coil spring over gas-charged shock absorbers, stabilizer bar 	
Rear 	Multi-link independent with coil springs, link-type stabilizer bar, gas-charged shock absorbers and isolated rear suspension cradle	
		
STEERING		
Type	Power rack and pinion 	
Overall Ratio	16.65:1	
Turning Diameter (curb-to-curb)	11.1 m (36.5 ft.) (17-in. wheels), 11.5 m (37.7 ft.) (18-in. wheels)	
Steering Turns (lock-to-lock)	2.98 (17-in. wheels), 2.89 (18-in. wheels)	
		
BRAKES mm (in.) unless otherwise noted	
Power-assist Type	204 x 230 (8 x 9) tandem-diaphragm vacuum	
Availability	Standard on LX, Touring, Limited and S models 	
Front		
Size and Type	294 x 26 (11.5 x 1.0) vented rotors with 57.0 (2.2) single-piston floating caliper	
Swept Area (Total Front)	1,442.1 sq. cm (223.5 sq. in.) 	
Rear		
Size and Type	262 x 10 (10.3 x 0.4) solid rotor with 35.0 (1.4) single-piston floating caliper	
Swept Area (Total Rear)	894.6 sq. cm (138.6 sq. in.) 	
Parking Brake Type	Drum-in-hat  	
Anti-lock Brake System (ABS)	Standard    	
Electronic Stability Control (ESC) 	Standard	
Traction Control	Standard	
Brake Assist	Standard	
		
DIMENSIONS AND CAPACITIES mm (in.) unless otherwise noted	
Wheelbase	2,765 (108.9) 	
Track, Front	1,567 (61.7) 	
Track, Rear	1,594 (62.7) 	
Overall Length	4,870 (191.7) 	
Overall Width	1,843 (72.5) without side mirrors / 2,121 (83.5) with side mirrors	
Overall Height	1,482 (58.4) (For P225/55R17)	
Aero	 	
Cd	0.34	
Fuel Tank Capacity	64.0 litre (14.1 gal.) standard and FFV
18.5 PZEV	
Towing Capabilities, NAFTA Markets kg (lb.) (a)	
2.4-litre Automatic Transmission	450 (1,000) 	
3.6-litre Automatic Transmission	450 (1,000) 	
(a) Maximum frontal area of trailer or boat: 2.04 square metre (22 square feet) 3.6L engine and 1.02 square metre (11 square feet) 2.4L engine.	
		
Curb Weight, Base Vehicle, kg (lb.)	 	
2.4-litre Gasoline Engine	200 Touring — 1,544 (3,402.8) 	
3.6-litre Gasoline Engine	200 Touring — 1,622 (3,575.8) 	

ACCOMMODATIONS mm (in.) unless otherwise noted	
Seating Capacity - F/R	2/3	
Total Interior Passenger Volume	2,840 litres (100.3 cu. ft.)	
Front		
Head Room w/o Sunroof	1,017 (40.1) 	
Head Room w/Sunroof	963 (37.9) 	
Legroom	1,077 (42.4) 	
Shoulder Room	1,431 (56.3) 	
Hip Room	1,336 (52.6) 	
Seat Travel 	260 (10.2) 	
Front Compartment Volume	1,566 litres (55.3 cu. ft.) 	
Rear		
Head Room 	975 (38.4) 	
Legroom	919 (36.2) 	
Shoulder Room 	1,422 (56.0) 	
Hip Room	1,341 (52.8) 	
Knee Clearance	50 (2.0) 	
 Rear Compartment Volume	1,274 litres (45.0 cu. ft.) 	
Cargo		
Trunk Lift-over Height	799 (31.5) (For P225/55R17)	
Luggage Compartment Volume 	385 litres (13.6 cu. ft.) 	
		
WHEELS (in.)		
Availability	Standard on 200 LX model	
Type and Material	Steel with Sparkle Silver wheel cover 	
Size 	17 in. x 6.5 in.    	
		
Availability	Standard on 200 Touring model, available onLX model	
Type and Material	Machined cast-aluminum, Sparkle Silver	
Size	17 in. x 6.5 in.	
		
Availability	Standard on 200 Limited model, available on Touring model	
Type and Material	Polished aluminum	
Size	18 x 7.0 in. 	
		
Availability	Standard on 200 S model	
Type and Material	Polished Aluminum with Black Painted Pockets	
Size	18 x 7.0 in.	
		
Availability	Available on Touring model	
Type and Material	Cast Aluminum, Satin Silver	
Size	18 x 7.0 in.	
		
TIRES		
Availability	Available on 200 LX 	
Size and Type	P225/55R17, All-season	
Model	Michelin Primacy MXV4 Touring	
Revs per km (mile)	483 (778)	
		
Availability	Available on 200 Limited model, optional on Touring model	
Size and Type	P225/50R18, All-season Touring	
Model 	Goodyear Eagle LS-2 Touring	
Revs per km (mile)	483 (777) 	
		
Availability	Standard on 200 LX and Touring models	
Size and Type	225/55R17, All-season	
Model 	Nexen CP671	
Revs per km (mile)	484 (779)