2014 Fiat® 500 & 500c
CANADIAN SPECIFICATIONS

Specifications are based on the latest product information available at the time of publication. 
All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Vehicle Type	Hatchback or cabrio	
EnerGuide Vehicle Class	Micro car (hatchback) / Standard Specialty (Cabrio)	
Assembly Plant	Toluca (Mexico)	
Introduction Date	Spring 2011 as a 2012 model	
	
BODY/CHASSIS	
Layout	Transverse-mounted front engine, front-wheel-drive (FWD)	
Construction	Unitized steel body 	
	
ENGINE: 1.4-LITRE SOHC 16-VALVE MULTIAIR® INLINE FOUR-CYLINDER	
Availability	Standard — Fiat® 500 and 500c Pop, Sport and Lounge	
Type and Description	Inline four-cylinder, liquid-cooled	
Displacement	1,368 cu. cm (83.48 cu. in.) 	
Bore x Stroke	72.0 x 84.0 (2.83 x 3.31) 	
Valve System	Belt-driven, MultiAir, SOHC, 16 valves, hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Cast iron block with aluminum-alloy heads and aluminum-alloy bedplate	
Compression Ratio	10.8:1	
Power 	101 bhp  @ 6,500 rpm (73.8 bhp/litre)	
Torque 	98 lb.-ft. @ 4,000 rpm	
Max. Engine Speed	6,900 rpm (electronically limited)	
Fuel Requirement	87 octane (R+M)/2 acceptable 
91 octane recommended	
Oil Capacity	3.8 litres (4.0 qt.)  with dry filter	
Coolant Capacity	4.4 litres (4.6 qt.) 	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors 
and internal engine features	
Max. Gross Trailer Weight	Not rated for trailer tow	
2013 EnerGuide Fuel Economy L/100km (mpg) City/Hwy	6.4 (44) / 4.9 (58) with 5-speed manual (Hatchback)
6.7 (42) / 5.2 (54) with 5-speed manual (Cabrio)
7.4 (38) / 5.7 (50) with 6-speed automatic	
Engine Assembly Plant	Dundee, Mich.(U.S.A.)	
	
ENGINE: 1.4-LITRE SOHC 16-VALVE TURBOCHARGED MULTIAIR® INLINE FOUR-CYLINDER	
Availability	Standard — Fiat 500 Turbo	
Type and Description	Inline four-cylinder, liquid-cooled, turbocharged	
Displacement	1368 cu. cm (83.48 cu. in.)	
Bore x Stroke	72.0 x 84.0 (2.83 x 3.31 in.) 	
Valve System	Belt-driven, MultiAir, SOHC, 16 valves, hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Cast-iron block with aluminum-alloy head and aluminum-alloy bedplate	
Compression Ratio	9.8:1		
Maximum Turbo Boost (psi / bar)	18 psi / 1.24 bar	
Power 	135 bhp @ 5,500 rpm (98.7 bhp/litre)	
Torque 	150 lb.-ft.  @ 2,500-4,000 rpm	
Max. Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	87 octane (R+M)/2 acceptable 
91 octane recommended	
Oil Capacity	3.8 litres (4.0 qt.)  with dry filter	
Coolant Capacity	4.4 litres (4.6 qt.) 	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors 
and internal engine features	
Max. Gross Trailer Weight	Not rated for trailer tow	
2013 EnerGuide Fuel Economy 
L/100 km (mpg) City/Hwy	7.1 (40) / 5.7 (50)	
Engine Assembly Plant	Dundee, Mich. (U.S.A.)	
	
TRANSMISSION: C514 FIVE-SPEED MANUAL	
Availability	Standard on 500 and 500c Pop, Sport and Lounge models	
Description	1st, 2nd gear: Double Cone 3rd, 4th, 5th, gear: Single Cone	
Gear Ratios		
1st	3.909	
2nd	2.174	
3rd	1.345	
4th	0.974	
5th	0.766	
Reverse	3.818	
Final-drive Ratio	3.44 (500 and 500c Pop and Lounge)
3.73 (500 Sport)	
Overall Top Gear	2.63 (500 and 500c Pop and Lounge)
2.85 (500 Sport)	
		
TRANSMISSION: AISIN AUTOMATIC SIX-SPEED OVERDRIVE WITH AUTO STICK	
Availability	Optional on 500 and 500c Pop, Sport and Lounge models	
Description	Auto Stick driver-interactive manual control and electronically modulated torque converter clutch	
Gear Ratios		
1st	4.044	
2nd	2.371	
3rd	1.556	
4th	1.159	
5th	0.852	
6th	0.672	
Reverse	3.193	
Final Drive Ratio	4.103	
Overall Top Gear	6.01	
	
TRANSMISSION: C510 PERFORMANCE FIVE-SPEED MANUAL	
Availability	Standard on Fiat 500 Turbo	
Description	1st, 2nd gear: Double Cone
3rd, 4th, 5th, gear: Single Cone	
Gear Ratios		
1st	3.909	
2nd	2.238 	
3rd	1.520 	
4th	1.156	
5th	0.872 	
Reverse	3.909	
Final-drive Ratio	3.353	
Overall Top Gear	2.92	
		
ELECTRICAL SYSTEM		
Alternator	105-amp — Standard on 500 Pop (with automatic transmission) and 500c Pop, Sport and Lounge models	
	120-amp — Standard on 500 Pop (with manual transmission) and 500 Turbo	
Battery	500 CCA, maintenance free	
		
SUSPENSION		
Front 	MacPherson suspension, coil spring with twin-tube shock absorbers and stabilizer bar — included with 500 and 500c Pop and Lounge 	
	Sport-tuned shock absorbers and springs — included with 500 Sport	
	Sport-tuned shock absorbers, springs and performance-designed lower-control arm — included with 500 Turbo	
Rear	Rear twist-beam axle with coil springs and twin-tube shock absorbers — included with 500 and 500c Pop and Lounge	
	Sport-tuned shock absorbers and springs — included with 500 Sport and 500 Turbo	
		
STEERING		
Type	Power rack and pinion with electric power steering (EPS) column	
Overall Ratio	16.3:1	
Turning Diameter (curb-to-curb)	9.32 m (30.6 ft.) 	
Steering Turns (lock-to-lock)	3.0	
		
BRAKES mm (in.) unless otherwise noted		
Availability	Standard on 500 and 500c Pop and Lounge, 500 Sport	
Front		
Rotor size and type	257 x 22 (10.1 x 0.86)  vented	
Caliper size and type	54 (2.12)  single-piston with aluminum housing	
Swept area	1,244 sq. cm (193 sq. in.) 	
Rear		
Rotor size and type	240 x 11 (9.4 x 0.4)  solid	
Caliper size and type	34 (1.33)  single-piston with aluminum housing	
Swept area	984 sq. cm (153 sq. in.) 	

Availability	Standard on 500 Turbo	
Front		
Rotor size and type	282 x 22 (11.1 x 0.86)  vented	
Caliper size and type	54 (2.12) single-piston with aluminum housing	
Swept area	1,244 sq. cm (193 sq. in.) 	
Rear		
Rotor size and type	240 x 11 (9.4 x 0.4)  solid	
Caliper size and type	34 (1.33)  single-piston with aluminum housing	
Swept area	984 sq. cm (153 sq. in.) 	
		
DIMENSIONS AND CAPACITIES(a) mm (in.) unless otherwise noted	
Wheelbase	2,300 (90.6) 	
Track, Front	1,407 (55.4) 	
Track, Rear	1,397 (55.0) 	
Overall Length	500/500c — 3,547 (139.6) 
500 Turbo — 3667 (144.4) 	
Overall Width	1,627 (64.1) 	
Overall Height	1,519 (59.8) 	
Ground Clearance	500 — 104 (4.1)
500c — 118 (4.6)	
Drag Coefficient (Cd)	500 Pop — 0.332
500 Sport and Turbo — 0.362
500 Lounge — 0.359
500c  Pop and Lounge — 0.364	
Curb Weight	500 with 5-speed manual — 1,074 kg (2,363 lb.) 
500 with 6-speed automatic — 1,106 kg (2,434 lb.) 
500c with 5-speed manual — 1,094 kg (2,411 lb.) 
500c with 6-speed automatic — 1,130 kg (2,486 lb.) 
500 Turbo — 1,124 kg (2,477 lb.) 	
Weight Distribution, per cent Front/Rear	500 with 5-speed manual — 64/36 
500 with 6-speed automatic — 66/34 
500c with 5-speed manual — 62/38
500c with 6-speed automatice — 63/37
500 Turbo — 65/35	
Fuel Tank Capacity	40 litres (8.8 gal.)	
(a) All dimensions measured at curb weight with standard tires.	
	
ACCOMMODATIONS mm (in.) unless otherwise noted	
Seating Capacity, F/R	2/2	
Front Seat		
Head room	500 – 989 (38.9)
500 – 956 (37.6) with sunroof
500c – 980 (38.6)	
Legroom	1,035 (40.7)	
Shoulder room	1,255 (49.4)	
Hip room	1,215 (47.9) 	
Total seat travel	Driver — 210 (8.2)
Passenger — 210 (8.2)	
Front row interior volume	500 – 1,240 litres (43.8 cu. ft.) 
500c – 1,271 litres (44.9 cu. ft.)	
Rear Seat		
Head room	500 – 903 (35.6)
500c – 934 (36.8)	
Legroom	805 (31.7) 	
Knee clearance	97 (3.8)	
Shoulder room	1,178 (46.4)	
Hip room	43 (1083.1) 	
Second row interior volume	500 – 855.2 litres (30.2 cu. ft.)
500c – 886 litres (31.3 cu. ft.)	
Total Interior Volume	500 – 2,409.8 litres (85.1 cu. ft.) 
500c – 2,311 litres (81.6 cu. ft.)	
Luggage Compartment Volume	500 – 269 litres (9.5 cu. ft.)
500c – 153 litres (5.4 cu. ft.) 	
Interior Volume Index	500 – 2,140.8 litres (75.6 cu. ft.)
500c – 2,158 litres (76.7 cu. ft.) 	
Trunk Liftover Height	703.6 (27.7) 	
		
TIRES		
Availability 	Standard on 500 and 500c Pop and Lounge	
Size and type	185/55R15 BSW All-season 	
Mfr. and model	Continental ContiProContact or Firestone Firehawk GTH 
or Pirelli Cinturato P7 A/S	
Revs per km (mile)	563 (906) 	

Availability	Standard on 500 Sport and 500 Turbo	
Size and type	195/45R16XL BSW All-season 	
Mfr. and model	Pirelli Cinturato P7 A/S or Continental ContiProContact	
Revs per km (mile)	560 (901) or 566 (911) 	
		
WHEELS (in.)		
Availability	Standard on 500 and 500c Pop	
Type and material	Steel wheels with tech silver painted wheel covers	
Size	15 x 6.0	
		
Availability	Standard on 500c Lounge	
Type and material	Cast-aluminum, five oval spoke design, fully painted tech silver	
Size	15 x 6.0	
		
Availability	Standard on 500 Lounge	
Type and material	Cast-aluminum, nine split-spoke design, fully painted tech silver	
Size	15 x 6.0	
		
Availability	Standard on 500c Lounge	
Type and material	Cast-aluminum, seven split-spoke design, fully painted tech silver	
Size	15 x 6.0	
		
Availability	Optional on 500 and 500c Lounge	
Type and material	Cast-aluminum premium finish, radial design, fully painted premium silver	
Size	15 x 6.0	
		
Availability	Standard on 500 Sport	
Type and material	Cast-aluminum, polished face with dark mineral grey painted pockets	
Size	16 x 6.5	
		
Availability	Standard on 500 Turbo	
Type and material	Cast-aluminum, polished face with gloss black painted pockets	
Size	16 x 6.5	

Availability	Optional on 500 Sport	
Type and material	Cast-aluminum, five split-spoke design with polished face with dark mineral grey painted pockets and Rosso accented centre cap	
Size	16 x 6.5	
		
Availability	Optonal on 500 Turbo	
Type and material	Cast-aluminum, five split-spoke design with Hyper Nero face and Rosso accented centre cap	
Size	16 x 6.5