2014 Jeep® Cherokee
CANADIAN SPECIFICATIONS

Specifications are based on the latest product information available at the time of publication. 
All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Body Style 	Sport-utility vehicle (SUV)	
Assembly Plant	Toledo North Assembly Plant, Toledo, Ohio (U.S.A.)	
EnerGuide Vehicle Class 	Multipurpose vehicle	
Introduction Date	Initial introduction mid-2013 as a 2014 model	
	
BODY AND CHASSIS	
Layout	Transverse front engine, 4x2 and 4x4	
Construction 	Steel uniframe	
	
ENGINE: 3.2-LITRE DOHC 24-VALVE V6	
Availability 	Optional on Sport, North and Trailhawk 	
Type and Description 	60-degree V-type, liquid-cooled	
Displacement 	3,239 cu. cm (197.7 cu. in.) 	
Bore x Stroke 	91.0 x 83.0 (3.58 x 3.27) 	
Valve System 	Chain-driven, DOHC, 24 valves, with hydraulic roller finger followers	
Fuel Injection 	Sequential, multiport, electronic, return-less 	
Construction 	Die cast aluminum block, aluminum alloy heads 	
Compression Ratio 	10.7:1	
Power 	271 hp @ 6,500 rpm (82.4 hp/litre)	
Torque 	239 lb.-ft. @ 4,400 rpm 	
Max. Engine Speed	6,500 rpm, electronically limited	
Fuel Requirement	Regular unleaded, 87 octane (R+M)/2	
Oil Capacity 	5.7 litres (6.0 qt.) 	
Coolant Capacity 	9.2 litres (9.7 qt.) 	
Emission Controls	Two mini-oxidation three-way catalytic converters; four heated oxygen sensors; and internal engine features	
EnerGuide Fuel Economy L/100 km (mpg), City/Hwy 	TBD — 4x2 with automatic transmission
TBD — 4x4 with automatic transmission	
Engine Assembly Plant	Trenton Engine, Trenton, Mich. (U.S.A.)	
	
ENGINE: 2.4-LITRE 16-VALVE MULTIAIR® TIGERSHARK™ INLINE FOUR-CYLINDER	
Availability	Standard on Sport, North and Limited	
Type and Description	Inline four-cylinder, 16-valve MultiAir with multiport fuel injection	
Displacement	2,360 cu. cm (144 cu. in.) 	
Bore x Stroke	88 X 97	
Valve System	SOHC, 4 valves per cylinder (16 total)	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum block, aluminum cylinder head	
Compression Ratio	10:1	
Power 	184 hp @ 6,250 rpm	
Torque 	171 lb.-ft. @ 4,800 rpm	
Max. Engine Speed	6,500 rpm	
Fuel Requirement	Unleaded regular, 87 octane	
Oil Capacity 	5.2 litres (5.5 qt.) 	
Coolant Capacity 	6.7 litres (7.1 qt.) 	
Emission Controls	Single catalytic converter, heated wide band lambda sensor upstream and mid-catalyst heated oxygen sensor	
Estimated EnerGuide Fuel Economy 
L/100km (mpg) (city/hwy) 	TBD	
Engine Assembly Plant 	Dundee Engine Plant, Dundee, Mich. (U.S.A.)	
	
TRANSMISSION: 948TE NINE-SPEED AUTOMATIC 	
Availability	Standard on all models	
Description 	Planetary gear train, transverse layout	
Ratio Spread	9.79	
Gear Ratios		
1st	4.70	
2nd	2.84	
3rd	1.91	
4th	1.38	
5th	1.00	
6th	0.81	
7th	0.70	
8th	0.58	
9th	0.48	
Rev	3.81	
Spread	9.79	
Axle Ratios	3.2-litre 4x2 — 3.251
3.2-litre 4x4 (non-trailer tow) — 3.251
3.2-litre 4x4 (trailer tow) — 3.517
2.4-litre 4x2 — 3.734
2.4-litre 4x4 (non-trailer tow) — 3.734
2.4-litre 4x4 (trailer tow) — 4.048	
	
4X4 SYSTEMS: JEEP ACTIVE DRIVE I, JEEP ACTIVE DRIVE II, JEEP ACTIVE DRIVE LOCK	
Availability 	Jeep Active Drive I is standard on Sport, North and Limited and Jeep Active Drive II is optional on North and Limited; Jeep Active Drive Lock is standard on Trailhawk	
Type	Fully disconnecting 4x2 mode with automatic 4x4 engagement	
	Electronic 4x4 Low and Neutral range shifting	
	Full-time 4x4 mode with active on demand clutch	
Operating Modes	Auto 4x2/4x4, 4x4 Low, Neutral	
Centre Differential Type	None	
Terrain Response	Unique tuning in all terrain modes	
Low-range Ratio	2.92:1	
	
ELECTRICAL SYSTEM	
Alternator 	160-amp, 180-amp optional	
Battery	600-amp maintenance-free, 730-amp optional	
	
SUSPENSION	
Front 	McPherson strut, long travel coil springs, one-piece aluminum 
sub-frame, aluminum lower control arms, stabilizer bar	
Rear	Four link rear suspension with trailing arm, aluminum lateral links, isolated high-strength steel rear cradle, coil springs, and stabilizer bar	
	
STEERING	
Type 	Electric Power rack and pinion	
Overall Ratio 	15.15 4x2 and 4x4, 15.36 4x4 Lock	
Turning Diameter (curb-to-curb) 	4x2: 11.5 m (37.6 ft.) 
4x4: 11.5 m (37.7 ft.) 
4x4 Lifted: 11.6 m (38.0 ft.) 
Off-road: 11.6 m (38.1 ft.) 	
Steering Turns (lock-to-lock)	2.56 4x2 and 4x4, 2.67 4x4 Lock	
BRAKES	
Front		
Size and Type 	330 x 28 (13 x 1.1)  vented rotor with 
60 (2.36)  single-piston floating caliper	
	330 x 28 (13 x 1.1) vented rotor with
48 (1.89) twin piston floating caliper (Available)	
Swept Area (per caliper)	651.1 sq. cm (100.9 sq. in.), 1 x 60; 839.4 sq. cm.(130.1 sq. in.) 
2 x 48 	
Rear		
Size and Type	278 x 12 (10.95 x 0.47) solid rotor with 
38 (1.5)  single-piston floating caliper	
	320 x 12 (12.6 x 0.47)  solid rotor with
43 (1.69)  single piston floating caliper (Available)	
Swept Area (per caliper)	638.6 sq. cm (99.0 sq. in.) 1 x 38; 754.8 sq. cm (117.0 sq. in.)  
1 x 43 	
Power-assist Type 	230 x 230 (9 x 9)  tandem diaphragm, vacuum assist 	
Four-wheel anti-lock brake system (ABS)	Standard	
Electronic stability control (ESC)	Standard	
Parking Brake Type	Electric motor on caliper	
	
DIMENSIONS AND CAPACITIES(a) mm (in.) unless otherwise noted	
Wheelbase	2,700 (106.3)  4x4 I, 2,699.1 (106.26) 4x2, 2,718.8 (107.0) 4x4 Lock	
Track, Front	1,574.9 (62)  4x4 and 4x2, 1,593.5 (62.7)  4x4 II, 
and 1,613.5 (63.5)  4x4 Lock	
Track, Rear	1,573.2 (61.9)  4x4 and 4x2, 1,593.5 (62.7)  4x4 II, 
and 1613.5 (63.5)  4x4 Lock	
Overall Length (NAFTA vehicles)	4,624 (182) 	
Overall Width	1,858.8 (73.2)  4x2 and 4x4, 1,903.6 (74.9)  4x4 Lock	
Overall Height (with roof rack)	1,682.9 (66.2)  4x4, 1,670.2 (65.7)  4x2, 1,710 (67.3)  4x4 II, 
and 1,723.3 (67.8)  4x4 Lock	
Load-floor height	785.6 (30.9)  4x4	
Sill-step height	453.8 (17.9)  front step height, 460.8 (18.1) rear step height, 4x4	
Ground Clearances 
(4x4 with P245/65R17 tires)	219.1 (8.7)  minimum running ground clearance	
Chassis	247.8 (9.7)  cradle bolt head / 222.9 (8.8)  front underbody skid plate 	
Fuel Tank	271.3 (10.7)  (bolt under fuel tank) / 255.3 (10) brush guard	
Front Axle	265.4 (10.4)  two-speed PTU heat shield	
Rear Axle	246.4 (9.7)  two-speed RDM with locker	
Approach Angle, (with air dam) (degrees)	29.9 4x4 Lock; 18.9 4x4 I, 16.7 4x2	
Breakover Angle (degrees)	22.9 4x4 Lock; 19.5 4x4 I; 17.7 4x2	
Departure Angle (degrees)	32.2 4x4 Lock; 25.0 4x4 I; 24.6 4x2	
Frontal Area	TBD	
Aero CdA	TBD  (Cd x cross-sectional area)	
Aero Cd	TBD 	
Fuel-tank Capacity 	60 L (13.1 gal.) 	
Payload	454 kg (1,000 lb.) 	
Towing
All models without Trailer-tow Group and equipped with aftermarket Class II type hitch	907 kg (2,000 lb.) 	
3.2-litre engine automatic transmission with Trailer Tow Package (Class III)	2,041 kg (4,500 lb.) 	
Curb Weight 		
3.2-litre 4x2	1,729 kg (3,811 lb.) 	
3.2-litre 4x4 	1,834 kg (4,044 lb.) 	
3.2-litre 4x4 Lock	1,862 kg (4,106 lb.) 	
Weight Distribution, 4x4, F/R	57/43 	
(a) All dimensions measured with two passengers.	
	
ACCOMMODATIONS mm (in.) unless otherwise noted	
Seating Capacity — F/R 	2/3	
Front Row		
Head Room without Sunroof	999.9 (39.4) 	
Head Room with Sunroof	964.5 (37.9) 	
Legroom 	1,045 (41.1) 	
Shoulder Room 	1,462.3 (57.6) 	
Hip Room	1,366.6 (53.8) 	
Seat Travel 	210 (8.3) 	
Recliner Range (degrees)	6 to 84 (manual) / 6 to 61.25 (automatic)	
Volume (standard roof) 	1,585.2 litres (55.98 cu. ft.) 	
Second Row		
Head Room 	978.2 (38.5) 	
Legroom 	1,023.2 (40.3) 	
Knee Clearance	90.1 (3.5) 	
Shoulder Room 	1,399.8 (55.1) 	
Hip Room	1,268.1 (49.9) 	
Recliner Range (degrees)	19.25 to 27.25	
Cargo Volume 	1,400.8 litres (49.47 cu. ft.) 	
Cargo Access		
Liftover Height	785.6 (30.9)  4x4	
Maximum Cargo Width at Liftgate Opening	1,051 (41.4)  without subwoofer	
Minimum Cargo Width at Liftgate Opening 	916.9 (36.1)  at top of opening	
Maximum Cargo Height at Liftgate Opening	825.0 (32.5)  4x4 Lock	
Minimum Cargo Height at Liftgate Opening	780.0 (30.7)  4x2	
Distance Between Wheelhouse Interior Trim	1,000.5 (39.4) 	
Cargo Volume 		
Behind Rear Seat 	702.3 litres (24.8 cu. ft.) rear seat at design position
770.2 litres (27.2 cu. ft.) rear seat at mid travel 
841 litres (29.7 cu. ft.) rear seat at full forward	
Behind Front-row Seats 
with Rear Seats Folded	1,554.6 litres (54.9 cu. ft.) 	
	
WHEELS (in.)	
Availability	Standard on Sport 	
Type and Material	Painted Silver Full Face Steel 	
Size 	17 x 7	
		
Availability	Standard on North 	
Type and Material 	Painted Silver cast aluminum 	
Size 	17 x 7	
		
Availability	Standard on Limited 	
Type and Material 	Polished aluminum with painted pockets 	
Size 	18 x 7	
		
Availability	Standard on Trailhawk 	
Type and Material	Polished aluminum with painted pockets	
Size	17 x 7.5	
	
TIRES	
Availability	Standard on Sport / North 4x2	
Size and Type 	225/60R17 BSW, all-season 	
Mfr. and Model 	Firestone Destination LE2	
Revs per km (mile)	470 (757)	
		
Availability	Standard on Limited 4x2	
Size and Type 	225/55R18 BSW, all-season 	
Mfr. and Model	Continental ProContact TX 	
Revs per km (mile)	467 (752) 	
		
Availability	Standard on Sport / North 	
Size and Type	225/65R17 BSW all-season 	
Mfr. and Model	Firestone Destination LE2	
Revs per km (mile)	456 (734) 	
		
Availability	Standard on Limited 4x4	
Size and Type	225/60R18 BSW, all-season 	
Mfr. and Model 	Continental ProContact TX 	
Revs per km (mile)	452 (727)	
		
Availability	Standard on Trailhawk 	
Size and Type	P245/65R17 OWL all-terrain	
Mfr. and Model 	Firestone Destination A/T 	
Revs per km (mile)	443 (713) 	
		
Parking Brake Type	Electronic Park Brake	
Four-wheel anti-lock brakes	Standard 	
All-speed traction control	Standard