2014 Jeep® Compass
CANADIAN SPECIFICATIONS

Specifications are based on the latest product information available at the time of publication. 
All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Body Style	Sport-utility vehicle (SUV)	
Assembly Plant	Belvidere, Ill. (U.S.A.)	
EnerGuide Vehicle Class	Compact SUV	
Introduction Date	August 2006 	
		
BODY AND CHASSIS		
Layout	Transverse front-engine, front-wheel drive or four-wheel drive	
Construction	Unitized steel body	
		
ENGINE: 2.0-LITRE DOHC 16-VALVE I-4 WITH DUAL VVT	
Availability	Standard on Sport and North 4x2 models	
Type and Description 	Four-cylinder inline, tuned intake manifold with electronic active charge motion control valves, dual counter-rotating balance shafts	
Displacement	1,998 cu. cm (121.9 cu. in.) 	
Bore x Stroke	86 x 86 (3.39 x 3.39) 	
Valve System	Chain-driven DOHC, 16 valves, electronically controlled dual variable-valve timing (VVT), direct-acting shimless mechanical bucket tappets	
Fuel Injection 	Sequential, multiport, electronic, returnless	
Construction 	High-pressure die-cast aluminum block with dry iron liners, cast-aluminum cylinder head, cast-aluminum ladder frame, forged steel crankshaft	
Compression Ratio	10.5:1	
Power 	158 bhp @ 6,400 rpm 	
Torque 	141 lb.-ft. @ 5,000 rpm 	
Maximum Engine Speed	6,750 rpm (electronically limited)	
Fuel Requirement 	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity 	4.7 litres (5.0 qt.) 	
Coolant Capacity 	6.8 litres (7.2 qt.) 	
Emission Controls	Single catalytic converter, dual heated oxygen sensors 
and engine features 0.56g/km (0.9 g/mile) 	
2013 EnerGuide Fuel Economy 
L/100km (mpg) City/Hwy
	8.9 (32)/6.6 (43) — 4x2 with five-speed manual transaxle
9.7 (29)/7.0 (40) — 4x2 with six-speed automatic transmission 	
		
ENGINE: 2.4-LITRE DOHC 16-VALVE I-4 WITH DUAL VVT	
Availability	Standard on Limited models, Sport and North 4x4 models, 
Available on Sport and North 4x2 models	
Type and Description	Four-cylinder inline, tuned intake manifold with electronic active charge motion control valves dual counter-rotating balance shafts	
Displacement	2360 cu. cm (144 cu. in.) 	
Bore x Stroke	88 x 97 (3.46 x 3.82) 	
Valve System	Chain-driven DOHC, 16 valves, electronically controlled dual VVT, direct-acting shimless mechanical bucket tappets	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	High-pressure die-cast aluminum block with dry iron liners, 
cast-aluminum cylinder head, cast-aluminum ladder frame, 
forged steel crankshaft	
Compression Ratio	10.5:1	
Power 	172 bhp @ 6,000 rpm 	
Torque 	165 lb.-ft. @ 4,400 rpm	
Maximum Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity 	4.7 litres (5.0 qt.) 	
Coolant Capacity 	6.8 litres (7.2 qt.) 	
Emission Controls	Single catalytic converter, 4x2, dual catalytic converter, 
4x4 dual heated oxygen sensors and engine features	
Smog-forming Pollution	0.56 g/km (0.9 g/mile) (a)	
Maximum Gross Trailer Weight	450 kg (1000 lb.)  
900 kg  (2000 lb.) — with Trailer-tow Prep Group	
EnerGuide Fuel Economy L/100km (mpg) (city/hwy) 
	9.0 (31)/7.0 (40) — 4x2 with five-speed manual transaxle	
	9.8 (29)/7.0 (40) — 4x2 with six-speed automatic transmission 	
	9.0 (31)/7.0 (40) — 4x4 with five-speed manual transaxle	
	10.0 (28)/7.4 (38) — Freedom Drive I® 4x4 with six-speed automatic transmission 	
	10.3 (27)/8.7 (32) — Trail Rated® 4x4 with CVT2	
(a) NMOG + NOX emission limits under ULEV II and Tier 2, Bin 5 emission requirements.	
		
TRANSAXLE: MANUAL MAGNA DRIVELINE T355 FIVE-SPEED	
Availability	Standard — 2.0-litre engine
Standard — 2.4-litre engine	
Description	Five-speed, overdrive, synchronized in all forward ratios, 
cable-operated, three-plane shifter	
Gear Ratios		
1st	3.77	
2nd	2.16	
3rd	1.41	
4th	1.026	
5th	0.72 	
Reverse	3.417	
Final-drive Ratio	4.12	
Overall Top-gear	2.97	
		
TRANSAXLE: AUTOMATIC 6F24 SIX-SPEED POWERTECH WITH AUTO STICK 	
Availability	Optional — 2.0-litre engine 
Optional — 2.4-litre engine Optional — 2.4-litre engine 	
Description	Six-speed automatic transmission, lockup torque converter, 
electronic controls	
Gear Ratios		
1st	4.212	
2nd	2.637	
3rd	1.800	
4th	1.386	
5th	1.000	
6th	0.772	
Reverse	3.285	
Final-drive Ratio	3.648:1 (2.0-litre engine), 3.367:1 (2.4-litre engine)	
Overall Top-gear Ratio	2.817 (2.0-litre engine); 2.600 (2.4-litre engine)	
Auto Stick	Standard with 6F24	
		
TRANSAXLE: AUTOMATIC JATCO MODEL CVT2L (Freedom Drive II)	
Availability	Optional on Sport, North and Limited 4x4 with 2.4-litre engine and Freedom Drive II®	
Description	Continuously variable ratio, lockup torque converter, electronic controls	
Gear Ratios		
Forward	2.349:1 to 0.394:1 continuously variable	
Reverse	1.75:1	
Final-drive Ratio	8.135:1	
Overall Top-gear Ratio	3.21:1	
Effective Maximum Low-gear Ratio	19.11:1	
		
DRIVETRAIN		
Front-wheel-Drive		
Availability	Standard	
Front Differential	Open	
Four-wheel-Drive		
Availability	Optional	
Type	Electronically-controlled coupling (ECC) with four-wheel-drive lock	
Rear Differential	Open	
		
ELECTRICAL SYSTEM		
Alternator	120-amp; 140-amp with CVT2L (Freedom Drive II)	
Battery	525 CCA, maintenance-free	
		
SUSPENSION		
Front	Independent MacPherson strut, coil spring over gas-charged shock absorbers and stabilizer bar
	
Rear	Multi-link independent with coil springs, link-type stabilizer bar, 
gas-charged shock absorbers	
		
STEERING		
Type	Rack and pinion with hydraulic power assist	
Overall Ratio	16.4:1	
Turning Diameter (curb-to-curb)	17-in. wheels and tires — 10.8 m (35.6 ft.) 
18-in. wheels and tires — 11.3 m (37.2 ft.)  	
Steering Turns (lock-to-lock)	17-in. wheels and tires — 2.88
18-in. wheels and tires — 2.76	
		
BRAKES		
Availability	Standard on 4x2 Sport and North	
Front		
Size and Type 	294 x 26 (11.5 x 1.0) vented disc with 57 (2.2) 
single-piston floating caliper	
Swept Area	1,442.12 sq. cm (223.52 sq. in.) 	
Rear		
Size and Type 	229 x 35 (9.0 x 1.38) drums 	
Swept Area	503 sq. cm (78.1 sq. in.) 	
Power-assist Type	254 (10)  single-diaphragm vacuum	
Anti-lock Brake System (ABS)	Standard	
Electronic Stability Control (ESC)	Standard	
Hill-start Assist (HSA)	Standard with manual transmission	
		
Availability	Standard on 4x4 Sport, North and Limited, and 4x2 Limited	
Front		
Size and Type 	294 x 26 (11.5 x 1.0) vented disc 
with 57 (2.2) single-piston floating caliper	
Swept Area	1442.12 sq. cm (223.52 sq. in.) 	
Rear		
Size and Type 	262 x 10 (10.3 x 0.39) solid disc 
with 35 (1.4) single-piston floating caliper	
Swept Area	894.6 sq. cm (138.64 sq. in.) 	
Power-assist Type	254 (10)  single-diaphragm vacuum	
Anti-lock Brake System (ABS)	Standard	
Electronic Stability Control (ESC)	Standard	
Hill-start Assist (HSA)	Standard with manual transmission and 
Freedom Drive II Off-road Package	
Off-road brake-traction Control System (BTCS)	Included with Freedom Drive II Off-road Package 	
Hill-descent Control (HDC)	Included with Freedom Drive II Off-road Package 	
DIMENSIONS AND CAPACITIES(d) mm (in.) unless otherwise noted	
Wheelbase	2,634 (103.7) 	
Track, Front	1,520 (59.8) 	
Track, Rear	1,520 (59.8) 	
Overall Length	4,448 (175.1) 	
Overall Width	1,814 (71.4) 	
Overall Height	1,651 (65.0) 	
Overhang, Front	916 (36.1) 	
Overhang, Rear	897 (35.3) 	
Approach Angle with P215/60/R17 Tire (degrees)	19.5	
Breakover Angle with P215/60/R17 Tire (degrees)	20.6	
Departure Angle with P215/60/R17 Tire (degrees)	28.5	
Ground Clearance with P215/60/R17 Tire	206 (8.1) 	
Approach Angle with Freedom Drive II Off-road Package P215/65/R17 Tire (degrees)	29.6	
Breakover Angle with Freedom Drive II Off-road Package P215/65/R17 Tire (degrees)	23.6	
Departure Angle with Freedom Drive II Off-road Package P215/65/R17 Tire (degrees)	31.2	
Ground Clearance with Freedom Drive II Off-road Package P215/65/R17 Tire	231 (9.1) 	
Aero (CdA)	10.5 — 4x2	
	10.6 — 4x4	
Curb Weight 	Sport 4x2 — 1,404 kg (3,097 lb.)   2.0-litre MTX
Sport 4x2 — 1,438 kg (3,171 lb.)   2.0-litre ATX
Sport 4x2 — 1,410 kg (3,108 lb.)   2.4-litre MTX 
Sport 4x2 — 1,448 kg (3,192 lb.)   2.4-litre ATX	
	Sport 4x4 — 1,479 kg (3,260 lb.)   2.4-litre MTX
Sport 4x4 — 1,517 kg (3,345 lb.)   2.4-litre ATX 
Sport 4x4 — 1,521 kg (3,354 lb.)   2.4-litre ATX – CVT2	
Weight Distribution, per cent F/R	59/41 — 4x2	
	58/42 — 4x4	
Fuel Tank Capacity	51.5 litre (13.6 gal.) — 4x2; 51.1 (13.5)  — 4x4	
(d) All dimensions measured at curb weight with standard tires.	
		
ACCOMMODATIONS mm (in.) unless otherwise noted	
Seating Capacity, F/R	2/3	
Front		
Head Room without Sunroof	1,034 (40.7) 	
Legroom	1,031 (40.6) 	
Shoulder Room	1,387 (54.6) 	
Hip Room	1,328 (52.3) 	
Seat Travel	Driver — 10.2 (260); Passenger — 10.2 (260) 	
Recliner Angle Range (degrees)	Driver — up to 88; Passenger — 76 fold-flat/88 non-fold-flat	
Front Seat Volume Index	1,478 litres (52.2 cu. ft.) 	
Rear		
Head Room	1,013 (39.9) 	
Legroom	1,001 (39.4) 	
Knee Clearance	44.1 (1.7) 	
Shoulder Room	1,372 (54.0)  	
Hip Room	1,295 (51.0) 	
Rear Seat Volume Index	1,391 litres (49.1 cu. ft.) 	
Interior Volume	2,868 litres (101.3 cu. ft.) 	
Cargo Volume Indexes		
Rear Seats Up	643 litres (22.7 cu. ft.) 	
Rear Seats Folded	1,518 litres (53.6 cu. ft.) 	
Interior Volume Index	3,511 litres (124 cu. ft.) 	
Trunk Lift-over Height	775 (30.5) 	
Cargo Volume with Front Passenger Seat 
and Rear Seat Folded 	1,776 litres (62.7 cu. ft.) 	
Minimum Cargo Width at Liftgate Opening	976 (38.5) 	
Minimum Cargo Height at Liftgate Opening	634 (25.0) 	
Maximum Cargo Width at Liftgate Opening	1,150 (45.3) 	
Maximum Cargo Height at Liftgate Opening	681 (26.7) 	
Distance Between Wheelhouse Interior Trim	966 (38.0) 	
		
WHEELS (in.)		
Availability	Standard on Sport, and North with 2.0-litre engine	
Type and Material	Full painted aluminum	
Size	16 x 6.5	
		
Availability	Standard on Sport, North with 2.4-litre engine, optional with 2.0-litre	
Type and Material	Full painted aluminum	
Size	17 x 6.5	
		
Availability	Standard on Limited	
Type and Material	Full painted aluminum 	
Size	18 x 7.0	
		
Availability	Optional on Limited	
Type and Material	Chrome-clad aluminum	
Size	18 x 7.0	
		
Availability	Optional on Limited	
Type and Material	Full painted aluminum 	
Size	18 x 7.0	
		
TIRES		
Availability	Standard on Sport, North with 2.0-litre engine	
Size and Type	P205/70R16 BSW All-season Touring	
Manufacturer and Model	Goodyear Eagle LS	
Revs per km (mile)	763 (475)	
		
Availability	Optional on the Latitude	
Size and Type	P225/60R17 BSW All-season Touring	
Manufacturer and Model	Kumho Solus KL21	
Revs per km (mile)	756 (470)	

Availability	Standard on Sport, North with 2.4-litre engine	
Size and Type	P215/60R17 BSW All-season Touring	
Manufacturer and Model	Firestone Affinity S3	
Revs per km (mile) 	771 (479)	
		
Availability	Optional on Sport, North and Limited with Off-Road Group	
Size and Type	P215/65R17 outlined white letter (OWL) All-terrain	
Manufacturer and Model	Goodyear Wrangler GTA 03	
Revs per km (mile) 	743 (462)	
		
Availability	Standard on Limited	
Size and Type	P215/55R18 All-season Performance	
Manufacturer and Model	Firestone Firehawk GTA 03	
Revs per km (mile) 	765 (476)