2014 Ram 1500
CANADIAN SPECIFICATIONS

Specifications are based on the latest product information available at the time of publication. 
All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Vehicle Type	Regular Cab, Quad Cab, and Crew Cab, 2WD, 4WD	
Assembly Plant	Regular Cab: Saltillo Truck Assembly, Saltillo (Mexico)	
	Quad Cab: Warren Truck Assembly Plant, Warren, Mich. (U.S.A.)	
	Crew Cab: Warren Truck Assembly Plant, Warren, Mich. (U.S.A.)	
Vehicle Class	Standard Pickup	
		
BODY/CHASSIS		
Layout	2WD — Longitudinal, front engine	
	4WD — Longitudinal, front engine, transfer case	
Construction	2WD — Ladder-type frame, steel cab, double-wall steel pickup box	
	4WD — Ladder-type frame, steel cab, double-wall steel pickup box	
		
ENGINE: 3.6-LITRE 24-VALVE DOHC V6 E85	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	3,604 cu. cm  (220 cu. in.) 	
Bore x Stroke	96.0 mm x 83.0 mm (3.78 in. x 3.27 in.) 	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads	
Compression Ratio	10.2:1	
Power 	305 hp at 6,400 rpm	
Torque 	269 lb.-ft. at 4,175 rpm	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2, E85-compatible	
Oil Capacity	5.7 litres (6.0 qt.) 	
Coolant Capacity	13.25 litres (14.0 qt.) 	
Emission Controls	Dual three-way catalytic converters, heated oxygen sensors	
2014 EnerGuide Fuel Economy 
L/100 km (mpg) (City/Hwy)  	11.4 (25) / 7.8 (36)	
		
ENGINE: 3.0-LITRE DOHC ECODIESEL V6	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	2988 cu. cm (182 cu. in.) 	
Bore x Stroke	83 x 92 (3.27 x 3.60) 	
Valve System	Chain-driven DOHC, 24 valves	
Fuel Injection	Common-rail, 2000 bar, Solenoid Injectors	
Construction	Cast-iron block, aluminum alloy heads	
Compression Ratio	15.5:1	
Power 	240 hp at 3,600 rpm	
Torque 	420 lb.-ft. at 2,000 rpm	
Max. Engine Speed	4,800 rpm (electronically limited)	
Fuel Requirement	Ultra Low-sulfur diesel	
Oil Capacity	7.8 litres (8.2 qt.) 	
Coolant Capacity	11.4 litres (12 qt.) 	
Emission Controls	Cooled EGR, Oxidation catalyst, Diesel particulate filter, 
SCR w/urea injection	
Estimated Maximum Fuel Economy L/100 km (mpg) (city/hwy) (1)	TBA	
(1)	Ratings not available at time of printing		
		
ENGINE: 5.7-LITRE HEMI® 16-VALVE V8		
Type and Description	90-degree V8, liquid-cooled	
Displacement	5654 cu. cm (345 cu. in.) 	
Bore x Stroke	99.5 x 90.9 (3.92 x 3.58) 	
Valve System	Variable cam timing, pushrod-operated overhead valves, 16 valves, hydraulic lifters with roller followers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.5:1	
Power 	395 hp @ 5,600 rpm	
Torque 	410 lb.-ft. @ 3,950 rpm	
Max. Engine Speed	5,800 rpm	

Fuel Requirement	Unleaded mid-grade, 89 octane (R+M)/2 — recommended 	
	Unleaded regular, 87 octane (R+M)/2 — acceptable	
Oil Capacity	6.6 litres (7.0 qt.) 	
Coolant Capacity	13.33 litres (14.0 qt.) 	
Emission Controls	Three-way catalytic converters, heated oxygen sensors 
and internal engine features	
2014 EnerGuide Fuel Economy 
L/100 km (mpg) (city/hwy) 8-speed automatic 	14.1 (20) / 9.3 (30)	
2014 EnerGuide Fuel Economy 
L/100 km (mpg) (city/hwy) 6-speed automatic 	15.4 (18) / 10.2 (28)	
	
TRANSMISSION: 65RFE AUTOMATIC SIX-SPEED	
Availability	Available with 5.7-litre V8 equipped trucks	
Description	Three planetary gear sets, one overrunning clutch, full electronic control, electronically controlled converter clutch	
Gear Ratios		
1st	3.00	
2nd	1.67 	
3rd   	1.50	
4th	1.00	
5th	0.75	
6th	0.67	
Reverse	3.00	
Axle Gear Ratios	3.21,,3.55, 3.92, 4.10 	
	
TRANSMISSION: ZF 8HP45 AUTOMATIC EIGHT-SPEED WITH ELECTRONIC RANGE SELECT (ERS)	
Availability	Standard with 3.6-litre Pentastar 
	
Description	Adaptive electronic control, automatic or Electronic Range Select (ERS) manual control. Five clutch-pack design with only two open clutches in any gear. Torque converter lock with turbine torsional damper for low lock-up speeds in 1st through 8th gear	
Gear Ratios		
1st	4.71	
2nd 	3.14	
3rd 	2.10	
4th 	1.67	
5th 	1.29	
6th 	1.00	
7th 	0.84	
8th 	0.67	
Reverse 	3.30	
Axle Gear Ratios	3.21, 3.55	
		
TRANSMISSION: ZF 8HP70 AUTOMATIC EIGHT-SPEED WITH ELECTRONIC RANGE SELECT (ERS)	
Availability	Available with select 5.7-litre V8 equipped trucks	
Description	Adaptive electronic control, automatic or ERS manual control. Five clutch-pack design with only two open clutches in any gear. Torque converter lock with turbine torsional damper for low lock-up speeds in 1st through 8th gear	
Gear Ratios		
1st	4.71	
2nd	3.14	
3rd	2.10	
4th	1.67	
5th	1.29	
6th	1.00	
7th	0.84	
8th	0.67	
Reverse	3.30	
Final Drive and Overall Top Gear Ratios	2.15 with 3.21 axle; 2.38 with 3.55 axle; 2.63 with 3.92 axle	
		
TRANSFER CASE: BW 44-45 PART-TIME		
Availability	3.6-litre V6 4x4 and 5.7-litre V8 4x4	
Shift Mechanism	Electric	
Available Speeds	2-speed	
Operating Modes	2WD High; 4WD High, Locked; Neutral; 4WD Low, Locked	
Low-range Ratio	2.64	
Centre Differential Type	None	

TRANSFER CASE: BW 44-44 ON-DEMAND		
Availability	3.0-litre V6 4x4, 5.7-litre V8 4x4 	
Shift Mechanism	Electric	
Available Speeds	2-speed	
Operating Modes	2WD High; 4WD Auto; 4WD High, Locked; Neutral; 4WD Low, Locked	
Low-range Ratio	2.64	
Centre Differential Type	None	
		
AXLES		
Front	ZF 215 mm	
Rear	C235 mm (available limited slip)	
Available Ratios	3.21, 3.55, 3.92	
		
ELECTRICAL SYSTEM		
Architecture	Powernet	
Alternator	160-amp, 180-amp, 220-amp (Stop-start and Special Services Package)	
Battery	Group 65, low-maintenance 730 CCA (Stop-start features 800 CCA Absorbed Glass Mat)	
		
SUSPENSION		
Front	Upper and lower “A” arms, coil springs, twin-tube shock absorbers, stabilizer bar. Optional air suspension replaces twin-tube shock absorbers and coil springs	
Rear	Five-link with track bar, coil springs, stabilizer bar, twin-tube shock absorbers, solid axle. Optional air suspension replaces twin-tube shock absorbers and coil springs	

BRAKES 		
Front		
Size and Type	336 x 28 (13.2 x 1.1)  vented disc with 54 (2.13) ()
two-piston pin-slider caliper and ABS	
Swept Area	1,884 sq. cm  (292 sq. in.) 	
Rear		
Size and Type	352 x 22 (13.8 x 0.87)  disc with 54 (2.13) 
single-piston pin-slider caliper and ABS	
Swept Area	1,768 sq. cm  (274 sq. in.) 	
Power-assist	Dual-rate, tandem diaphragm vacuum	
		
AIR BAGS		
Regular Cab	6	
Quad Cab	6	
Crew Cab	6	
	
STEERING	
Power-assist	
Regular Cab	2WD	2WD	4WD	4WD	
Box Length	Short Box
(6-ft. 4-in.)	Long Box
(8-ft.)	Short Box
(6-ft. 4-in.)	Long Box
(8-ft.)	
Wheelbase (nominal)  	3,061 (120.5) 	3,569.2 (140.5) 	3,569.2 (140.5) 	3,569.2 (140.5) 	
Overall Steering Ratio 	19.1:1	17.9:1	19.1:1	17.9:1	
Steering Wheel Turns (lock-to-lock)	3.5	3.3	3.5	3.3	
Turning Diameter – 17-in. Tire 	12.0 m (39.5 ft.) 	13.7 m (45.1 ft.) 	12.1 m (39.8 ft.) 	13.8 m (45.4 ft.) 	
Turning Diameter – 20-in. Tire 	12.0 m (39.3 ft.) 	13.7 m (44.9 ft.) 	12.1 m (39.8 ft.) 	13.9 m (45.5 ft.) 	
Turning Diameter – 17-in. Outdoorsman
Tire 	N/A	N/A	12.0 m (39.4 ft.) 	13.7 m (45.0 ft.)	
					
Quad Cab	2WD	4WD	
Box Length	Long Box
(6-ft. 4-in.)	Long Box
(6-ft. 4-in.)	
Wheelbase (nominal)  	3,569.2 (140.5) 	3,569.2 (140.5) 	
Overall Steering Ratio 	17.9:1	17.9:1	
Steering Wheel Turns (lock-to-lock)	3.3	3.3	
Turning Diameter – 17-in. Tire 	13.7 m (45.1 ft.) 	13.8 m (45.4 ft.) 	
Turning Diameter – 20-in. Tire 	13.7 m (44.9 ft.) 	13.9 m (45.5 ft.) 	
Turning Diameter – 17-in. Outdoorsman Tire 	13.7 m (44.8 ft.) 	13.7 m (45.0 ft.) 	
					
Crew Cab	2WD	2WD	4WD	4WD	
Box Length	Short Box
(5-ft. 7-in.)	Long Box
(6-ft. 4-in.)	Short Box
(5-ft. 7-in.)	Long Box
(6-ft. 4-in.)	
Wheelbase (nominal)  	3,061 (140.5) 	3,569.2 (149.5) 	3,569.2 (140.5) 	3,569.2 (149.5) 	
Overall Steering Ratio 	19.1:1	17.9:1	19.1:1	17.9:1	
Steering Wheel Turns (lock-to-lock)	3.5	3.3	3.5	3.3	
Turning Diameter – 17-in. Tire	12.0 m (39.5 ft.) 	13.7 m (45.1 ft.) 	12.1 m (39.8 ft.) 	13.8 m (45.4 ft.) 	
Turning Diameter – 20-in. Tire 	12.0 m (39.3 ft.) 	13.7 m (44.9 ft.) 	12.1 m (39.8 ft.) 	13.9 m (45.5 ft.) 	
Turning Diameter – 17-in. Outdoorsman Tire 	N/A	N/A	12.0 m (39.4 ft.) 	13.7 m (45.0) 	

DIMENSIONS AND CAPACITIES
mm (in.) unless otherwise noted	
Cargo Box	
Nominal Box Size 	5-ft. 7-in. 
(Crew)	6-ft. 4-in. 
(Regular, Quad, or Crew)	8-ft. 
(Regular)	
Volume, litres (cu. ft.)	1,424.3 (50.3) 	1,628.2 (57.5)	2,115.3 (74.7)	
Length at Floor, Tailgate Closed  	1,712.4 (67.4) 	1,938.5 (76.3) 	2,496.5 (98.3) 	
Cargo Width  	1,686.9 (66.4) 	1,686.9 (66.4) 	1,686.9 (66.4) 	
Distance Between Wheelhouses  	1,295.4 (51) 	1,295.4 (51) 	1,295.4 (51) 	
Depth  	508.6 (20.0) 	511.1 (20.1) 	513.0 (20.2) 	
Tailgate Opening Width 	1535.3 (60.4) 	1535.3 (60.4) 	1535.3 (60.4) 	

Regular Cab Pickup	
Model – Tire Size 	2WD –265/70R17	4WD –265/70R17	
Box Length 	6-ft. 4-in.	8-ft.	6-ft. 4-in.	8-ft.	
Wheelbase (nominal)  	3,061.2 (120.5) 	3,569.2  (140.5) 	3,062.5 (120.5) 	3,570.2 (140.5) 	
Track, Front 	1,728.2 (68.0) 	1,728.2 (68.0) 	1,732.3 (68.2) 	1,732.3  (68.2) 	
Track, Rear 	1,714.7 (67.5) 	1,714.7 (67.5) 	1,714.7 (67.5) 	1,714.7 (67.5) 	
Overall Length 	5,308.5 (209.0) 	5,866.5 (231.0)	5,308.5 (209.0) 	5,866.5 (231.0) 	
Overall Width 	2,017.4 (79.4)	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4)	
Overall Height 	1,894.2 (74.6) 	1,889.2 (74.4) 	1,910.4 (75.2) 	1,906.2 (75.0) 	
Ground Clearance	
Front Axle 	229.3 (9.0)  	229.2 (9.0) 	232.6 (9.2) 	232.7 (9.2) 	
Rear Axle 	221.2 (8.7)  	221.5 (8.7) 	219.2 (8.6) 	219.5 (8.6) 	
Open Tailgate to Ground 	883.4 (34.8) 	878.3 (34.6) 	889.6 (35.0) 	885.3 (34.9) 	
Pickup Body Height 	511.1 (20.1) 	513.0 (20.2) 	511.1 (20.1) 	513.0 (20.2) 	
Approach Angle (degrees) 	15.6	15.7	17.7	17.8	
Departure Angle (degrees)	25.2	24.1	25.6	24.4	
Ramp Breakover Angle (degrees) 	21.5	19.2	22.9	20.5	
Fuel-Tank Capacity 	98-litre (26-gal.)  (standard)	121-litre  (32-gal.)  (standard)	98-litre (26-gal.)  (standard)	121-litre  (32-gal.)  (standard)	

Quad Cab 6-ft. 4-in. Box Pickup	
Model – Tire Size 	2WD –265/70R17	4WD –265/70R17	
Wheelbase (nominal)	3,569.2 (140.5) 	3,570.2 (140.5) 	
Track, Front 	1,728.2 (68.0) 	1,732.3 (68.2) 	
Track, Rear 	1,714.7 (67.5)	1,714.7 (67.5) 	
Overall Length 	5,816.5 (229.0) 	5,816.5 (229.0) 	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4)	
Overall Height 	1,960.2 (77.2) 	1,974.8 (77.7) 	
Ground Clearance	
Front Axle 	229.2 (9.0) 	232.7 (9.2) 	
Rear Axle 	221.5 (8.7) 	219.5 (8.6) 	
Open tailgate to ground 	878.3 (34.6) 	885.3  (34.9) 	
Pickup Body Height 	511.1 (20.1) 	511.1 (20.1) 	
Approach Angle (degrees)	15.7	17.8	
Departure Angle (degrees)	25.1	25.4	
Ramp Breakover Angle (degrees)	19.2	20.5	
Fuel-Tank Capacity	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	

Model – Tire Size 	2WD –265/70R17	4WD –265/70R17	
Box Length 	6-ft. 4-in.	8-ft.	6-ft. 4-in.	8-ft.	
Ground Clearance	
Front Axle 	248.5 (9.8) 	248.5 (9.8) 	248.5 (9.8) 	248.5 (9.8) 	
Rear Axle 	235.0 (9.3) 	235.0 (9.3) 	235.0 (9.3) 	235.0 (9.3) 	
Open Tailgate to Ground 	847.2 (33.4) 	885.7 (34.9) 	904.1 (35.6) 	936.7 (36.9) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	
Approach Angle (degrees) 	16.6	20.9	22.9	24.0	
Departure Angle (degrees)	19.4	21.3	22.2	23.6	
Ramp Breakover Angle without Skid Plate	17.1	20.6	22.5	24.2	
Ramp Breakover Angle with Skid Plate	13.8	17.0	18.7	20.3	
Ground Clearance without Skid Plate	187.2 (7.4) 	239.8 (9.4) 	269.5 (10.6) 	290.8 (11.4) 	
Ground Clearance with Skid Plate	169.3 (6.7) 	222.8 (8.8) 	252.8 (9.9) 	273.7 (10.8) 	
Fuel-Tank Capacity 	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre  (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.) (optional)	98-litre (26-gal.) (standard)
121-litre (32-gal.)  (optional)	

Crew Cab Pickup	
Model – Tire Size 	2WD –265/70R17	4WD –265/70R17	
Box Length 	5-ft. 7-in.	6-ft. 4-in.	5-ft. 7-in.	6-ft. 4-in.	
Wheelbase (nominal) 	3,569.2 (140.5) 	3,795.3 (149.4) 	3,570.2 (140.5) 	3,795.2 (149.4) 	
Track, Front 	1,728.2 (68.0) 	1,728.2 (68.0) 	1,732.3 (68.2) 	1,732.3 (68.2) 	
Track, Rear 	1,714.7 (67.5) 	1,714.7 (67.5) 	1,714.7 (67.5)	1,714.7 (67.5) 	
Overall Length 	5,816.5 (229.0) 	6,042.6 (237.9) 	5,816.5 (229.0) 	6,042.6 (237.9) 	
Overall Width 	2,017.4 (79.4) 	2,016.6 (79.4) 	2,017.4 (79.4) 	2,016.6 (79.4) 	
Overall Height 	1,953.8 (76.9) 	1,950.6 (76.8) 	1,967.9 (77.5) 	1,965.1 (77.4) 	
Ground Clearance	
Front Axle 	229.2 (9.0) 	231.1 (9.1) 	232.7 (9.2) 	235.2 (9.2) 	
Rear Axle 	221.5 (8.7) 	220.5 (8.7) 	219.5 (8.6) 	218.3 (8.6) 	
Open Tailgate to Ground 	878.3 (34.6) 	874.0 (34.4) 	885.3 (34.9) 	880.8 (34.7)  	
Pickup Body Height 	508.6 (20.0) 	511.1 (20.1) 	508.6 (20.0) 	511.1 (20.1) 	
Approach Angle (degrees) 	15.7	16.0	17.8	18.0	
Departure Angle (degrees)	25.1	24.9	24.7	25.2	
Ramp Breakover Angle (degrees) 	19.2	18.5	20.5	19.7	
Fuel-Tank Capacity 	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	

Crew Cab Pickup - Outdoorsman	
Model – Tire Size 	2WD –275/60R20	4WD –275/60R20	
Box Length 	5-ft. 7-in.	6-ft. 4-in.	5-ft. 7-in.	6-ft. 4-in.	
Wheelbase (nominal)  	3,569.4 
(140.5) 	3,795.8 (149.4) 	3,573.5 (140.7) 	3,799.6 (149.6) 	
Track, Front 	1,742.2 (68.6) 	1,742.2 (68.6) 	1,743.2 (68.6) 	1,743.2 (68.6) 	
Track, Rear 	1,727.4 (68.0)	1,727.4 (68.0) 	1,727.4 (68.0) 	1,727.4 (68.0) 	
Overall Length 	5,816.5 (229.0) 	6,042.6 (237.9) 	5,816.5 (229.0) 	6,042.6 (237.9) 	
Overall Width 	2,017.4 (79.4) 	2,016.6 (79.4) 	2,017.4 (79.4) 	2,016.6 (79.4) 	
Overall Height 	1,972.3 (77.6) 	1,968.1 (77.5) 	1,994.1 (78.5) 	1,991.7 (78.4) 	
Ground Clearance	
Front Axle 	244.8 (9.6) 	243.6 (9.6) 	248.6 (9.8) 	248.0 (9.8) 	
Rear Axle 	237.0 (9.3) 	235.0 (9.3) 	233.2 (9.2) 	233.1 (9.2) 	
Open Tailgate to Ground 	887.7 (34.9) 	883.9 (34.8) 	903.5 (35.6) 	902.3 (35.5) 	
Pickup Body Height 	508.6 (20.0) 	511.1 (20.1) 	508.6 (20.0) 	511.1 (20.1) 	
Approach Angle (degrees) 	21.3	21.0	23.9	22.9	
Departure Angle (degrees)	21.4	21.2	22.1	22.1	
Ramp Breakover Angle (degrees) 	20.9	19.9	18.8	17.6	
Ground Clearance without Skid Plate	261.5 (10.3) 	261.0 (10.3) 	NA	NA	
Ground Clearance with Skid Plate	NA	NA	252.2 (9.9) 	251.6 (9.9) 	
Fuel-Tank Capacity 	98-litre (26-gal.)  (standard)
121-litre (32-gal.) (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-liter (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	

Crew Cab 5ft. 7in. Box Pickup - Air Suspension 4x2 and 4x4	
Tire Size 	265/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)  	3,569.4 (140.5) 	3,569.4 (140.5) 	3,569.4 (140.5) 	3,569.4 (140.5) 	
Track, Front 	1,728.2 (68.0) 	1,728.2 (68.0) 	1,728.2 (68.0) 	1,728.2 (68.0) 	
Track, Rear 	1,714.7 (67.5) 	1,714.7 (67.5) 	1,714.7 (67.5) 	1,714.7 (67.5) 	
Overall Length 	5,816.5 (229.0) 	5,816.5 (229.0) 	5,816.5 (229.0) 	5,816.5 (229.0) 	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	
Overall Height 	1,902.1 (74.9) 	1,955.1 (77.0) 	1,979.2 (77.9) 	2,006.1 (79.0) 	
Ground Clearance	
Front Axle 	232.3 (9.1) 	232.3 (9.1) 	232.3 (9.1) 	232.3 (9.1) 	
Rear Axle 	220.0 (8.7) 	220.0 (8.7) 	220.0 (8.7) 	220.0 (8.7) 	
Open Tailgate to Ground 	832.8 (32.8) 	871.2 (34.3) 	889.6 (35.0) 	922.2 (36.3) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	
Approach Angle (degrees) 	13.8	18.3	20.9	22.5	
Departure Angle (degrees)	23.0	24.8	25.6	27.1	
Ramp Breakover Angle (degrees) 	15.9	19.4	21.4	23.0	
Ground Clearance without Skid Plate	171.0 (6.7) 	223.5 (8.8) 	254 (10.0) 	274.3 (10.8) 	
Ground Clearance with Skid Plate	153.1 (6.0) 	205.7 (8.1) 	236.2 (9.3) 	256.5 (10.1) 	
Fuel-Tank Capacity 	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-liter (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	

Crew Cab 5ft. 7in. Box Pickup - Air Suspension 4x2 and 4x4	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal) 	3,569.4 (140.5) 	3,569.4 (140.5) 	3,569.4 (140.5) 	3,569.4 (140.5) 	
Track, Front 	1,742.2 (68.6) 	1,742.2 (68.6) 	1,742.2 (68.6) 	1,742.2 (68.6) 	
Track, Rear 	1,727.4 (68.0) 	1,727.4 (68.0) 	1,727.4 (68.0) 	1,727.4 (68.0) 	
Overall Length 	5,816.5 (229.0) 	5,816.5 (229.0) 	5,816.5 (229.0) 	5,816.5 (229.0) 	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4)	2,017.4 (79.4) 	
Overall Height 	1,917.4 (75.5) 	1,970.4 (77.6) 	1,994.5 (78.5) 	2,021.4 (79.6)	
Ground Clearance	
Front Axle 	248.5 (9.8) 	248.5 (9.8) 	248.5 (9.8) 	248.5 (9.8) 	
Rear Axle 	235.0 (9.3) 	235.0 (9.3) 	235.0 (9.3) 	235.0 (9.3) 	
Open Tailgate to Ground 	847.2 (33.4) 	885.7 (34.9) 	904.1 (35.6) 	936.7 (36.9) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	
Approach Angle (degrees) 	15.2	19.8	22.4	23.9	
Departure Angle (degrees)	23.7	25.5	26.4	27.8	
Ramp Breakover Angle (degrees) 	17.1	20.6	22.5	24.2	
Ground Clearance without Skid Plate	187.2 (7.4)	239.8 (9.4) 	269.5 (10.6) 	290.8 (11.4) 	
Ground Clearance with Skid Plate	169.3 (6.7)	222.8 (8.8) 	252.8 (9.9) 	273.7 (10.8) 	
Fuel-Tank Capacity 	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.) (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-liter (32-gal.)  (optional)	

	

Crew Cab 5ft. 7in. Box Pickup - Air Suspension 4x2 and 4x4 Outdoorsman	
Tire Size 	265/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)  	3,569.4 (140.5) 	3,569.4 (140.5) 	3,569.4 (140.5) 	3,569.4 (140.5) 	
Track, Front 	1,728.2 (68.0) 	1,728.2 (68.0) 	1,728.2 (68.0) 	1,728.2 (68.0) 	
Track, Rear 	1,714.7 (67.5) 	1,714.7 (67.5) 	1,714.7 (67.5) 	1,714.7 (67.5) 	
Overall Length 	5,816.5 (229.0) 	5,816.5 (229.0) 	5,816.5 (229.0) 	5,816.5 (229.0) 	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	
Overall Height 	1,902.1 (74.9) 	1,955.1 (77.0) 	1,979.2 (77.9) 	2,006.1 (79.0) 	

Ground Clearance	
Front Axle 	232.3 (9.1) 	232.3 (9.1) 	232.3 (9.1) 	232.3 (9.1) 	
Rear Axle 	220.0 (8.7) 	220.0 (8.7) 	220.0 (8.7) 	220.0 (8.7) 	
Open Tailgate to Ground 	832.8 (32.8) 	871.2 (34.3) 	889.6 (35.0) 	922.2 (36.3) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	
Approach Angle (degrees) 	15.2	19.7	21.8	22.9	
Departure Angle (degrees)	18.7	20.6	21.4	22.9	
Ramp Breakover Angle without Skid Plate	15.9	19.4	21.4	23.0	
Ramp Breakover Angle with Skid Plate	12.7	15.9	17.6	19.2	
Ground Clearance without Skid Plate	171.0 (6.7) 	223.5 (8.8) 	254 (10.0) 	274.3 (10.8) 	
Ground Clearance with Skid Plate	153.1 (6.0) 	205.7 (8.1) 	236.2 (9.3) 	256.5 (10.1) 	
Fuel-Tank Capacity 	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-liter (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	

Crew Cab 5ft. 7in. Box Pickup - Air Suspension 4x2 and 4x4 Outdoorsman	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)  	3,569.4 (140.5) 	3,569.4 (140.5) 	3,569.4 (140.5) 	3,569.4 (140.5) 	
Track, Front 	1,742.2 (68.6) 	1,742.2 (68.6) 	1,742.2 (68.6) 	1,742.2 (68.6) 	
Track, Rear 	1,727.4 (68.0) 	1,727.4 (68.0) 	1,727.4 (68.0) 	1,727.4 (68.0) 	
Overall Length 	5,816.5 (229.0) 	5,816.5 (229.0) 	5,816.5 (229.0) 	5,816.5 (229.0) 	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	
Overall Height 	1,917.4 (75.5) 	1,970.4 (77.6) 	1,994.5 (78.5) 	2,021.4 (79.6) 	
Ground Clearance	
Front Axle 	248.5 (9.8) 	248.5 (9.8) 	248.5 (9.8) 	248.5 (9.8) 	
Rear Axle 	235.0 (9.3) 	235.0 (9.3) 	235.0 (9.3) 	235.0 (9.3) 	
Open Tailgate to Ground 	847.2 (33.4) 	885.7 (34.9) 	904.1 (35.6) 	936.7 (36.9) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	
Approach Angle (degrees) 	16.6	20.9	22.9	24.0	
Departure Angle (degrees)	19.4	21.3	22.2	23.6	
Ramp Breakover Angle without Skid Plate	17.1	20.6	22.5	24.2	
Ramp Breakover Angle with Skid Plate	13.8	17.0	18.7	20.3	
Ground Clearance without Skid Plate	187.2 (7.4)	239.8 (9.4) 	269.5 (10.6) 	290.8 (11.4) 	
Ground Clearance with Skid Plate	169.3 (6.7) 	222.8 (8.8) 	252.8 (9.9) 	273.7 (10.8) 	
Fuel-Tank Capacity 	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-liter (32-gal.)  (optional)	98-litre (26-gal.) () (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	

Crew Cab 6ft. 4in. Box Pickup - Air Suspension 4x2 and 4x4	
Tire Size 	265/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)  	3,798.0 (149.5) 	3,798.0 (149.5) 	3,798.0 (149.5)	3,798.0 (149.5) 	
Track, Front 	1,728.2 (68.0)	1,728.2 (68.0) 	1,728.2 (68.0) 	1,728.2 (68.0) 	
Track, Rear 	1,714.7 (67.5) 	1,714.7 (67.5) 	1,714.7 (67.5) 	1,714.7 (67.5) 	
Overall Length 	6,042.6 (237.9) 	6,042.6 (237.9) 	6,042.6 (237.9) 	6,042.6 (237.9) 	
Overall Width 	2,017.4 (79.4)	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	
Overall Height 	1,897.7 (74.7) 	1,950.7 (76.8) 	1,975.2 (77.8) 	2,001.7 (78.8) 	
Ground Clearance	
Front Axle 	231.6 (9.1) 	231.6 (9.1) 	231.6 (9.1) 	231.6 (9.1) 	
Rear Axle 	217.7 (8.6) 	217.7 (8.6) 	217.7 (8.6) 	217.7 (8.6) 	
Open Tailgate to Ground 	827.9 (32.6) 	866.6 (34.1) 	885.2 (34.8) 	917.6 (36.1) 	
Pickup Body Height 	511.1 (20.1) 	511.1 (20.1) 	511.1 (20.1)	511.1 (20.1) 	
Approach Angle (degrees) 	13.8	18.3	20.9	22.5	
Departure Angle (degrees)	22.8	24.6	25.5	26.9	
Ramp Breakover Angle (degrees) 	15.3	18.7	20.5	22.2	
Ground Clearance without Skid Plate	170.0 (6.7) 	222.7 (8.8) 	252.4 (9.9) 	273.7 (10.8) 	
Ground Clearance with Skid Plate	152.3 (6.0) 	205.4 (8.1) 	235.4 (9.3) 	256.4 (10.1) 	
Fuel-Tank Capacity 	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-liter (26-gal.)  (standard)
121-liter (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	

Crew Cab 6ft. 4in. Box Pickup - Air Suspension 4x2 and 4x4 	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)  	3,798.0 (149.5) 	3,798.0 (149.5) 	3,798.0 (149.5) 	3,798.0 (149.5) 	
Track, Front 	1,742.2 (68.6) 	1,742.2 (68.6) 	1,742.2 (68.6) 	1,742.2 (68.6) 	
Track, Rear 	1,727.4 (68.0) 	1,727.4 (68.0) 	1,727.4 (68.0) 	1,727.4 (68.0) 	
Overall Length 	6,042.6 (237.9) 	6,042.6 (237.9) 	6,042.6 (237.9) 	6,042.6 (237.9) 	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	
Overall Height 	1,914.5 (75.4) 	1,967.5 (77.5) 	1,991.9 (78.4) 	2,018.5 (79.5) 	
Ground Clearance	
Front Axle 	247.9 (9.8) 	247.9 (9.8) 	247.9 (9.8) 	247.9 (9.8) 	
Rear Axle 	234.7 (9.2) 	234.7 (9.2) 	234.7 (9.2) 	234.7 (9.2)	
Open Tailgate to Ground 	819.5 (32.3) 	883.9 (34.8) 	902.5 (35.5) 	934.9 (36.8) 	
Pickup Body Height 	511.1 (20.1) 	511.1 (20.1) 	511.1 (20.1) 	511.1 (20.1) 	
Approach Angle (degrees) 	15.5	19.7	22.3	23.9	
Departure Angle (degrees)	22.5	25.5	26.4	27.8	
Ramp Breakover Angle (degrees) 	16.4	19.8	21.7	23.3	
Ground Clearance without Skid Plate	185.8 (7.3) 	239.0 (9.4) 	268.7 (10.6) 	290.0 (11.4) 	
Ground Clearance with Skid Plate	168.8 (6.6) 	221.7 (8.7) 	251.7 (9.9) 	272.7 (10.7) 	
Fuel-Tank Capacity 	98-litre (26-gal.)  (standard)
121-litre (32-gal.) (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-liter (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	

	
Crew Cab 6ft. 4in. Box Pickup - Air Suspension 4x2 and 4x4 Outdoorsman	
Tire Size 	265/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)  	3,798.0 (149.5) 	3,798.0 (149.5) 	3,798.0 (149.5) 	3,798.0 (149.5) 	
Track, Front 	1,728.2 (68.0) 	1,728.2 (68.0) 	1,728.2 (68.0) 	1,728.2 (68.0) 	
Track, Rear 	1,714.7 (67.5) 	1,714.7 (67.5) 	1,714.7 (67.5) 	1,714.7 (67.5) 	
Overall Length 	6,042.6 (237.9) 	6,042.6 (237.9) 	6,042.6 (237.9) 	6,042.6 (237.9) 	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	
Overall Height 	1,897.7 (74.7) 	1,950.7 (76.8) 	1,975.2 (77.8) 	2,001.7 (78.8) 	
					
Ground Clearance	
Front Axle 	231.6 (9.1) 	231.6 (9.1) 	231.6 (9.1) 	231.6 (9.1) 	
Rear Axle 	217.7 (8.6) 	217.7 (8.6) 	217.7 (8.6) 	217.7 (8.6) 	
Open Tailgate to Ground 	827.9 (32.6) 	866.6 (34.1) 	885.2 (34.8) 	917.6 (36.1) 	
Pickup Body Height 	511.1 (20.1) 	511.1 (20.1) 	511.1 (20.1) 	511.1 (20.1) 	
Approach Angle (degrees) 	15.3	19.7	21.8	22.9	
Departure Angle (degrees)	18.6	20.4	21.3	22.7	
Ramp Breakover Angle without Skid Plate	15.3	18.7	20.5	22.2	
Ramp Breakover Angle with Skid Plate	12.0	15.0	16.6	18.2	
Ground Clearance without Skid Plate	170.0 (6.7) 	222.7 (8.8) 	252.4 (9.9) 	273.7 (10.8)	
Ground Clearance with Skid Plate	152.3 (6.0) 	205.4 (8.1) 	235.4 (9.3) 	256.4 (10.1) 	
Fuel-Tank Capacity 	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.) (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-liter (32-gal.)  (optional)	

Crew Cab 6ft. 4in. Box Pickup - Air Suspension 4x2 and 4x4 Outdoorsman 	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)  	3,798.0 (149.5) 	3,798.0 (149.5) 	3,798.0 (149.5)	3,798.0 (149.5) 	
Track, Front 	1,742.2 (68.6) 	1,742.2 (68.6) 	1,742.2 (68.6) 	1,742.2 (68.6) 	
Track, Rear 	1,727.4 (68.0) 	1,727.4 (68.0) 	1,727.4 (68.0) 	1,727.4 (68.0) 	
Overall Length 	6,042.6 (237.9) 	6,042.6 (237.9) 	6,042.6 (237.9) 	6,042.6 (237.9) 	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	
Overall Height 	1,914.5 (75.4) 	1,967.5 (77.5) 	1,991.9 (78.4) 	2,018.5 (79.5) 	
Ground Clearance	
Front Axle 	247.9 (9.8) 	247.9 (9.8) 	247.9 (9.8) 	247.9 (9.8) 	
Rear Axle 	234.7 (9.2) 	234.7 (9.2) 	234.7 (9.2) 	234.7 (9.2) 	
Open Tailgate to Ground 	819.5 (32.3) 	883.9 (34.8) 	902.5 (35.5) 	934.9 (36.8) 	
Pickup Body Height 	511.1 (20.1) 	511.1 (20.1) 	511.1 (20.1) 	511.1 (20.1) 	
Approach Angle (degrees) 	16.6	20.9	22.9	24.0	
Departure Angle (degrees)	19.4	21.3	22.1	23.6	
Ramp Breakover Angle without Skid Plate	16.4	19.8	21.7	23.3	
Ramp Breakover Angle with Skid Plate	13.0	16.0	17.7	19.2	
Ground Clearance without Skid Plate	185.8 (7.3) 	239.0 (9.4) 	268.7 (10.6) 	290.0 (11.4) 	
Ground Clearance with Skid Plate	168.8 (6.6) 	221.7 (8.7) 	251.7 (9.9) 	272.7 (10.7) 	
Fuel-Tank Capacity 	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre 26-gal. () (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal).  (standard)
121-litre (32-gal.)  (optional)	

ACCOMMODATIONS
mm (inches) unless otherwise noted	
Model 	Regular Cab	Quad Cab	Crew Cab	
Seating Capacity, F/R 	3/0 or 2/0	3/3 or 2/3	3/3 or 2/3	

Front	
Head Room  	1,013.5 (39.9) 	1,041.4 (41.0) 	1,041.4 9 41.0) 	
Legroom  	1,041.4 (41.0) 	1,041.4 (41.0) 	1,041.4 (41.0) 	
Shoulder Room  	1,676.4 (66.0) 	1,676.4 (66.0) 	1,676.4 (66.0) 	
Hip Room  	1,598.7 (62.9) 	1,605.3 (63.2) 	1,605.3 (63.2) 	
Seat Travel  	230.0 (9.0) 	230.0 (9.0) 	230.0 (9.0) 	
Recliner Range (degrees) 	85 (38 RWD, 47 FWD)	56 (38 RWD 18 FWD)	56 (38 RWD, 18 FWD)	
Rear	
Head Room  	N/A	1,008.4 (39.7) 	1,013.5 (39.9) 	
Legroom  	N/A	880.9 (34.7) 	1,023.3 (40.3) 	
Shoulder Room  	N/A	1,668.8 (65.7) 	1,668.8 (65.7) 	
Hip Room  	N/A	1,598.3 (62.9) 	1,605.3 (63.2) 	
Interior Volume	
Front 	1,679.8 litres 
(62.5 cu. ft.) 	1,817.9 litres (64.2 cu. ft.) 	1,817.9 litres (64.2 cu.ft.) 	
Rear 	N/A	1,483.8 litres (52.4 cu. ft.) 	1,730.2 litres (61.1 cu.ft.) 	

Quad Cab 6ft. 4in. Box Pickup – Outdoorsman	
Model – Tire Size 	2WD –275/60R20	4WD –275/60R20	
Wheelbase (nominal)	3,569.4 (140.5) 	3,573.5 (140.7) 	
Track, Front	1,742.2 (68.6) 	1,743.2 (68.6) 	
Track, Rear 	1,727.4 (68.0) 	1,727.4 (68.0) 	
Overall Length	5,816.5 (229.0) 	5,816.5 (229.0) 	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4) 	
Overall Height	1,979.4 (77.9) 	2,001.6 (78.8) 	
Ground Clearance	
Front Axle 	244.8 (9.6) 	248.6 (9.8) 	
Rear Axle 	237.0 (9.3) 	233.2 (9.2) 	
Open tailgate to ground 	887.7	903.5	
Pickup Body Height 	511.1 (20.1) 	511.1 (20.1) 	
Approach Angle (degrees)	21.3	23.9	
Departure Angle, (degrees)	21.4	22.1	
Ramp Breakover Angle (degrees)	20.9	18.8	
Ground Clearance without Skid Plate	261.5 (10.3) 	NA	
Ground Clearance with Skid Plate	NA	252.2 (9.9) 	
Fuel-Tank Capacity	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	

Quad Cab 6ft. 4in. Box Pickup - Air Suspension 4x2 and 4x4	
Tire Size 	265/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)  	3,569.4 (140.5) 	3,569.4 (140.5) 	3,569.4 (140.5) 	3,569.4 (140.5) 	
Track, Front 	1,728.2 (68.0) 	1,728.2 (68.0) 	1,728.2 (68.0) 	1,728.2 (68.0) 	
Track, Rear 	1,714.7 (67.5) 	1,714.7 (67.5) 	1,714.7 (67.5) 	1,714.7 (67.5) 	
Overall Length 	5,816.5 (229.0) 	5,816.5 (229.0) 	5,816.5 (229.0) 	5,816.5 (229.0) 	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	
Overall Height 	1,909.0 (75.2) 	1,962.0 (77.2) 	1,986.6 (78.2) 	2,013.0 (79.2) 	
Ground Clearance	
Front Axle 	232.3 (9.1) 	232.3 (9.1) 	232.3 (9.1) 	232.3 (9.1) 	
Rear Axle 	220.0 (8.7) 	220.0 (8.7) 	220.0 (8.7) 	220.0 (8.7) 	
Open Tailgate to Ground 	832.8 (32.8) 	871.2 (34.3) 	889.6 (35.0) 	922.2 (36.3) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	
Approach Angle (degrees) 	13.8	18.3	20.9	22.5	
Departure Angle (degrees)	23.0	24.8	25.6	27.1	
Ramp Breakover Angle (degrees) 	15.9	19.4	21.4	23.0	
Ground Clearance without Skid Plate	171.0 (6.7) 	223.5 (8.8) 	254 (10.0) 	274.3 (10.8) 	
Ground Clearance with Skid Plate	153.1 (6.0) 	205.7 (8.1) 	236.2 (9.3) 	256.5 (10.1) 	
Fuel-Tank Capacity 	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	

Quad Cab 6ft. 4in. Box Pickup - Air Suspension 4x2 and 4x4	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal)  	3,569.4 (140.5) 	3,569.4 (140.5) 	3,569.4 (140.5) 	3,569.4 (140.5) 	
Track, Front 	1,742.2 (68.6) 	1,742.2 (68.6) 	1,742.2 (68.6) ()	1,742.2 (68.6) 	
Track, Rear 	1,727.4 (68.0) 	1,727.4 (68.0) 	1,727.4 (68.0) 	1,727.4 (68.0) 	
Overall Length 	5,816.5 (229.0) 	5,816.5 (229.0)	5,816.5 (229.0) 	5,816.5 (229.0) 	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	
Overall Height 	1,924.4 (75.8) 	1,977.4 (77.8) 	2,002.0 (78.8) 	2,028.4 (79.9) 	
Ground Clearance	
Front Axle 	248.5 (9.8) 	248.5 (9.8) 	248.5 (9.8) 	248.5 (9.8) 	
Rear Axle 	235.0 (9.3) 	235.0 (9.3) 	235.0 (9.3) 	235.0 (9.3) 	
Open Tailgate to Ground 	847.2 (33.4) 	885.7 (34.9) 	904.1 (35.6) 	936.7 (36.9) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	
Approach Angle (degrees) 	15.2	19.8	22.4	23.9	
Departure Angle (degrees)	23.7	25.5	26.4	27.8	
Ramp Breakover Angle (degrees) 	17.1	20.6	22.5	24.2	
Ground Clearance without Skid Plate	187.2 (7.4) 	239.8 (9.4) 	269.5 (10.6) 	290.8 (11.4) 	
Ground Clearance with Skid Plate	169.3 (6.7) 	222.8 (8.8) 	252.8 (9.9) 	273.7 (10.8) 	
Fuel-Tank Capacity 	98-litre (26-gal.)  (standard)
121-litre  (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard
121-litre (32-gal.)  (optional)	

Quad Cab 6ft. 4in. Box Pickup - Air Suspension 4x2 and 4x4 Outdoorsman	
Tire Size 	265/70R17	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal) 	3,569.4 (140.5) 	3,569.4 (140.5) 	3,569.4 (140.5) 	3,569.4 (140.5) 	
Track, Front 	1,728.2 (68.0) 	1,728.2 (68.0) 	1,728.2 (68.0) 	1,728.2 (68.0) 	
Track, Rear 	1,714.7 (67.5) 	1,714.7 (67.5) 	1,714.7 (67.5) 	1,714.7 (67.5) 	
Overall Length 	5,816.5 (229.0) 	5,816.5 (229.0) 	5,816.5 (229.0) 	5,816.5 (229.0) 	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	
Overall Height 	1,909.0 (75.2) 	1,962.0 (77.2) 	1,986.6 (78.2) 	2,013.0 (79.2) 	
Ground Clearance	
Front Axle 	232.3 (9.1) 	232.3 (9.1) 	232.3 (9.1) 	232.3 (9.1) 	
Rear Axle 	220.0 (8.7) 	220.0 (8.7) 	220.0 (8.7) 	220.0 (8.7) 	
Open Tailgate to Ground 	832.8 (32.8) 	871.2 (34.3) 	889.6 (35.0) 	922.2 (36.3) 	
Pickup Body Height 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	508.6 (20.0) 	
Approach Angle (degrees) 	15.2	19.7	21.8	22.9	
Departure Angle (degrees)	18.7	20.6	21.4	22.9	
Ramp Breakover Angle without Skid Plate 	15.9	19.4	21.4	23.0	
Ramp Breakover Angle, with Skid Plate 	12.7	15.9	17.6	19.2	
Ground Clearance without Skid Plate	171.0 (6.7) 	223.5 (8.8) 	254 (10.0) 	274.3 (10.8) 	
Ground Clearance with Skid Plate	153.1 (6.0) 	205.7 (8.1) 	236.2 (9.3) 	256.5 (10.1) 	
Fuel-Tank Capacity 	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.) (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	98-litre (26-gal.)  (standard)
121-litre (32-gal.)  (optional)	

Quad Cab 6ft. 4in. Box Pickup - Air Suspension 4x2 and 4x4 Outdoorsman	
Tire Size 	275/60R20	
Suspension Mode 	Entry / Exit	Normal Ride Height	Off Road 1	Off Road 2	
Wheelbase (nominal) 	3,569.4 (140.5) 	3,569.4 (140.5) 	3,569.4 (140.5) 	3,569.4 (140.5) 	
Track, Front 	1,742.2 (68.6) 	1,742.2 (68.6) 	1,742.2 (68.6) 	1,742.2 (68.6) 	
Track, Rear 	1,727.4 (68.0) 	1,727.4 (68.0) 	1,727.4 (68.0) 	1,727.4 (68.0) 	
Overall Length 	5816.5 (229.0) 	5,816.5 (229.0) 	5,816.5 (229.0) 	5,816.5 (229.0) 	
Overall Width 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	2,017.4 (79.4) 	
Overall Height 	1,924.4 (75.8) 	1,977.4 (77.8) 	2,002.0 (78.8) 	2,028.4 (79.9) 	

• • •