2014 Chrysler 300 SRT
SPECIFICATIONS

Specifications are based on the latest product information available at the time of publication. 
All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Vehicle Type	Full-size	
Assembly Plant	Brampton Assembly Plant, Ontario	
EnerGuide Vehicle Class	Large car	
Introduction Date	Summer 2013 as 2014 model	
		
BODY/CHASSIS		
Layout	Longitudinal front engine, rear-wheel-drive (RWD)	
Construction	Unitized steel body and aluminum hood	
		
ENGINE: 6.4-LITRE HEMI® V8 WITH FUEL SAVER TECHNOLOGY	
Availability	Standard 	
Type and Description	90-degree V-type, liquid-cooled	
Displacement	6,417 cu. cm (392 cu. in.)	
Bore x Stroke	103.9 x 94.5 (4.09 x 3.72) 	
Valve System	Pushrod-operated overhead valves, 16 valves with sodium-filled exhaust valves and hollow stem intake valves, 16 conventional hydraulic lifters, all with roller tips	
Fuel Injection	Sequential, multi-port, electronic, returnless; automatic features Fuel Saver mode	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.9:1	
Power 	470 hp at 6,000 rpm	
Torque 	470 lb.-ft. at 4,300 rpm	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Premium 91 octane (R+M)/2 — recommended	
Oil Capacity	6.6 litres (7 qt.) 	
Factory Oil Fill 	0W-40 Pennzoil Ultra synthetic	
Coolant Capacity	13.25 litres (14 qt.) 	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad-heated oxygen sensors and internal engine features	
Exhaust Type 	Dual 2.75-in. active exhaust with dual 4-in. round tips 	
EnerGuide Fuel Economy L/100 km (mpg) City/Hwy	15.0 (19) / 8.7 (32)	
Assembly Plant	Saltillo (Mexico)	
	
TRANSMISSION: W5A580 FIVE-SPEED AUTOMATIC		
Availability	Standard 	
Description	Adaptive electronic control or driver-interactive manual control with Auto/Stick or paddle controls; “Track” mode (features performance shifting and gear holding feature combined with “Sport” mode suspension damping rates)	
Gear Ratios		
1st	3.59	
2nd	2.19	
3rd	1.41	
4th	1.00	
5th	0.83	
Reverse	3.16	
Final Drive Ratio	3.06 – Getrag limited-slip differential	
Overall Top Gear	2.54	
		
ELECTRICAL SYSTEM		
Alternator	220-amp	
Battery	H7 case, 730 CCA, maintenance free	
		
SUSPENSION 		
Type	SRT tuned three-mode adaptive damping system: “Auto” mode = sporty but compliant ride; “Sport” mode = firm, maximum handling; “Track” mode = firm, maximum handling plus performance shifting and gear holding feature 	
Front 	Independent SLA with high upper “A” arm, coil spring over ADS Bilstein shock absorber, 30 mm stabilizer bar, lateral and diagonal lower links 	
Rear	Five-link independent with coil spring, ADS Bilstein shock absorber and isolated suspension cradle, link type 18 mm. stabilizer bar	
		
STEERING		
Type	SRT tuned rack and pinion with hydraulic power assist	
Overall Ratio	14.4:1	
Steering Turns (lock-to-lock)	2.75	
		
DIMENSIONS AND CAPACITIES(a) mm (in.) unless otherwise noted	
Wheelbase	3,053 (120.2) 	
Track, Front	1,610 (63.4) 	
Track, Rear	1,603 (63.1) 	
Overall Length	5,088 (200.33) 	
Overall Width	1,886 (74.24) 	
Overall Height	1,480 (58.26) 	
Frontal Area	2.5 m2 (6.2 ft.²)	
Ground Clearance (Minimum) 	111 (4.37) — front 	
Drag Coefficient (Cd)	0.334 	
Curb Weight	1,979 kg (4,365 lb.) 	
Weight Distribution, per cent Front/Rear	54/46	
Fuel Tank Capacity	73.4 litres (16.1 gal.) 	
(a) All dimensions measured at curb weight with standard tires.	
		
ACCOMMODATIONS mm (in.) unless otherwise noted	
Seating Capacity, F/R	2/3	
Front		
Head room	980 (38.6) 
937 (36.9)  with dual-pane sunroof	
Legroom	1,062 (41.8) 	
Shoulder room	1,511 (59.5) 	
Hip room	1,428 (56.2) 	
Seat travel	Driver — 269 (10.6) 
Passenger — 220 (8.66) 	
Recliner angle range, deg.	Power — 70.7
Manual — 70	
Front row interior volume	1,574.3 litres (55.6 cu. ft.) 	

		
Rear Seat		
Head room	963 (37.9) 
937 (36.9)  with dual-pane sunroof	
Legroom	1,018 (40.1) 	
Knee clearance	99 (3.9) 	
Shoulder room	1,465 (57.7) 	
Hip room	1,425 (56.1) 	
Second row interior volume	1,435.7 litres (50.7 cu. ft.) 	
Total Interior Volume	3,010.1 litres (106.3 cu.ft.) 	
Luggage Compartment Volume	461.6 litres (16.3 cu. ft.) 	
Interior Volume Index	3,471.6 litres (122.6 cu. ft.) 	
Trunk Liftover Height	768.9 (30.1) 	
		
TIRES		
Front and Rear	Standard on 300 SRT	
Size and type	245/45ZR20 All-season 	
Mfr. and model	Goodyear Eagle RS-A 2	
Revs per km (mile)	456 (731) 	
		
Front and Rear	Optional on 300 SRT 	
Size and type	245/45ZR20 Three-season	
Mfr. and model	Goodyear F1 Supercar	
Revs per km (mile)	450 (726) 	
		
WHEELS (in.)		
Availability 	Standard on 300 SRT 	
Type and material	Fully forged aluminum	
Size	20 x 9.0	
		
Availability 	Optional on 300 SRT 	
Type and material	Fully forged aluminum with Black Vapour chrome finish	
Size	20 x 9.0	
		
BRAKES		
Front		
Rotor size and type	360 x 32 (14.2 x 1.26)  vented and slotted	
Caliper size and type	44 (1.73)  Brembo four-piston fixed with aluminum housing	
Swept area	2,261 sq. cm (351 sq. in.) 	
Rear		
Rotor size and type	350 x 28 (13.8 x 1.10)  vented and slotted	
Caliper size and type	32 (1.26)  Brembo four-piston fixed with aluminum housing	
Swept area	2,036 sq. cm (316 sq. in.)