2015 Chrysler 200
CANADIAN SPECIFICATIONS

Specifications are based on the latest product information available at the time of publication. 
All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Body Style	Four-door sedan 	
Assembly Plant 	Sterling Heights, Michigan (U.S.A.)	
EnerGuide Vehicle Class 	Mid-size sedan 	
Introduction Date	Spring 2014	
		
BODY/CHASSIS		
Layout 	Transverse front engine with front-wheel drive (FWD) or all-wheel drive (AWD)	
Construction 	Steel uni-frame	
		
ENGINE: 2.4-LITRE, I-4, MULTIAIR TIGERSHARK, 16-VALVE, GASOLINE, SOHC 	
Availability	Standard on all models	
Type and Description	Four-cylinder inline, 16-valve MultiAir with multiport fuel injection	
Displacement	2,360 cu. cm (144 cu. in.) 	
Bore x Stroke	88 x 97 (3.46 x 3.82) 	
Valve System	SOHC, 16 valves (4 valves per cylinder) 	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	High-pressure die-cast aluminum block with dry iron liners, cast-aluminum cylinder heads, cast-aluminum ladder frame, forged-steel crankshaft	
Compression 	10.0:1	
Power 	184 hp @ 6,250 rpm (preliminary)	
Torque 	173 lb.-ft. @ 4,600 rpm (preliminary)	
Max. Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane	
Oil Capacity	5.2 litres (5.5 qt.) 	
Coolant Capacity	6.7 litres (7.1 qt.) 	
Emission Controls	GPEC3 engine-management system with close-coupled catalyst; and wide range O2 sensor	
Engine Assembly Plant	Dundee, Michigan (U.S.A.)	
Estimated EnerGuide Fuel Economy L/100km (mpg) City/Hwy*	10.2 (28) / 6.4 (44) 	
* Based on 2014 EnerGuide fuel consumption ratings. New 5-cycle test method shown.	
ENGINE: 3.6-LITRE PENTASTAR™ V6, DOHC GASOLINE, 24-VALVE, VVT	
Availability	Available on 200 Limited, 200S, and 200C models; Standard on AWD models	
Type and Description	60-degree bank angle, liquid-cooled, three-plenum intake manifold with electronically controlled manifold tuning valve and short-runner valves	
Displacement	3605 cu. cm (220 cu. in.)	
Bore x Stroke	96 x 83 mm (3.78 x 3.27) 	
Valve System	Chain-drive DOHC, 24 valves (4 valves per cylinder), hydraulic end-pilot roller rockers, variable cam phasing on intake an exhaust cams	
Fuel Injection	Sequential, multiport, electronic	
Construction	High-pressure die-cast A380 aluminum block with iron liners and semi-permanent mould A319 aluminum heads	
Compression Ratio	10.2:1	
Power 	295 bhp @ 6,350 rpm  	
Torque 	262 lb.-ft. @ 4,250 rpm 	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity	5.7 litres (6 qt.) with dry filter SAE 5W30	
Coolant Capacity	8.12 litres (8.58 qt.) 	
Emission Controls	Integrated cast-aluminum header manifolds; positive crankcase ventilation; inlet and exhaust cam phasers with internal exhaust gas recirculation (no EGR/AIR required); evaporative emissions system	
Estimated EnerGuide 5-cycle Fuel Economy L/100km (mpg) City/Hwy*	12.4 (23) / 7.5 (38) (FWD)
12.8 (22) / 8.1 (35) (AWD)	
Engine Assembly Plant	Trenton, Michigan (U.S.A.)	
* Based on 2014 EnerGuide fuel consumption ratings. New 5-cycle test method shown.	
	
TRANSMISSION: 948TE/9HP48, AUTOMATIC NINE-SPEED 	
Availability	Standard on all models	
Description	Nine-speed FWD/AWD, electronically controlled automatic overdrive transmission with torque converter clutch. Clutch-to-clutch architecture, with integral electro/hydraulic controls module	
Gear Ratios		
1st 	4.70 	
2nd	2.84 	
3rd	1.91	
4th 	1.38  	
5th	1.00	
6th	0.81	
7th	0.70	
8th	0.58	
9th	0.48	
Reverse 	3.81    	
Spread	9.81	
Final Drive Ratio – 948TE	3.73 with 2.4-litre engine	
Final Drive Ratio – 9HP48	4.08 with 3.6-litre engine	
		
SUSPENSION		
Front	MacPherson strut, dual reacting twin tube shock absorbers	
Rear 	Multi-link independent dual reacting twin tube shock absorbers 	
		
STEERING		
Type	Electric power rack and pinion 	
Overall Ratio	15:2 (FWD and AWD)	
Turning Diameter (curb-to-curb)	FWD: 11.94 m (39.2 ft.) , AWD: 12.03 m (39.5 ft.) 	
Steering Turns (lock-to-lock)	2.67	
		
BRAKES 
mm (in.) unless otherwise noted		
Power-assist Type	Vacuum assist	
Availability	Standard on all models 	
Front		
Size and Type	2.4-litre: (305 x 28) rotors with (60.0) single-piston iron caliper
3.6-litre: (330 x 28) rotors with (60.0) single-piston iron caliper	
Swept Area (Total Front)	2.4-litre: 394.1 sq. cm (61.1 sq. in.) 
3.6-litre: 436.8 sq. cm (67.7 sq. in.)	
Rear		
Size and Type	(278 x 12) rotors with (38.0) single-piston aluminum caliper	
Swept Area (Total Rear)	638.6 sq. cm (98.98 sq. in.) 	
Parking Brake Type	Electronic Park Brake 	
Anti-lock Brake System (ABS)	Standard    	
Electronic Stability Control (ESC) 	Standard	
Traction Control	Standard	
Brake Assist	Standard	
		
DIMENSIONS AND CAPACITIES
mm (in.) unless otherwise noted		
Wheelbase	2,742 (108.0) 	
Track, Front	1,577 (62.1) 	
Track, Rear	1,576 (62.0) 	
Overall Length	4,885 (192.3) 	
Overall Width	1,871 (73.6) 	
Overall Height	1,491 (58.7) 	
Front Overhang	1,039 (40.9) 	
Rear Overhang	1,103 (43.4) 	
Approach Angle (Deg.)	13.5	
Departure Angle (Deg.)	17.8	
Ground Clearance	3.6-litre FWD with 17-in. Tire (lowest available): 147mm	
Aero	 	
Cd	0.270	
Fuel Tank Capacity 	59.8 litres (15.8 gal.)	
Towing Capabilities, NAFTA Markets kg (lbs.)	No Trailer Tow Recommended	
Curb Weight, Base Vehicle	1,575 kg (3,473 lb.) 	
GVWR (Base vehicle)	2,092 kg (4,612 lb.) 	
		
ACCOMMODATIONS
mm (in.) unless otherwise noted		
Seating Capacity - F/R	2/3	
Total Interior Passenger Volume	2,871 litres (101.4 cu.ft.) 	
Front		
Head Room	983 (38.7) 	
Legroom	1,071 (42.2) 	
Shoulder Room	1,485 (58.5) 	
Hip Room	1,384 (54.5) 	
Seat Travel 	210	
Front Compartment Volume 	1,666 litres (55.3 cu.ft.)	
Rear		
Head Room 	950 (37.4) 	
Legroom	956 (37.6) 	
Shoulder Room 	1,441 (56.7) 	
Hip Room	1,338 (52.7) 	
Knee Clearance	71.3	
Rear Compartment Volume Index	1,305 litres (46.1 cu. ft.)	
Cargo		
Trunk Lift-over Height	726	
Trunk Volume 	410 litres (14.5 cu. ft.) 	
Interior Volume	3,282 litres (115.9 cu. ft.)	
Passenger Volume	2,871 litres (101.4 cu. ft.)	
		
WHEELS (in.)		
Availability	200 LX 	
Type and Material	Steel with cover 	
Size 	17 x 7.0 	
		
Availability	200 Limited 	
Type and Material	Cast Aluminum, Painted-Tech Silver – Standard
Cast Aluminum, Painted – Available	
Size	17 x 7.5 – Standard
18 x 8.0 – Available	
		
Availability	200S	
Type and Material	Cast Aluminum, Painted-Satin Carbon – Standard
Cast Aluminum, Painted-Hyper Black – Available	
Size	18 x 8.0 – Standard
19 x 8.0 – Available	
		
Availability	200C 	
Type and Material	Cast Aluminum, Painted-Satin Silver – Standard FWD
Cast Aluminum, Polished-Satin Clear – Standard AWD
Cast Aluminum, Polished Face-Painted Pockets – Available FWD & AWD	
Size	17 x 7.5  – Standard FWD
18 x 8.0 – Standard AWD
19 x 8.0 – Available FWD & AWD	
		
TIRES		
Availability	200 LX	
Size and Type (Revs per kilometre)	Bridgestone 215/55R17 (492)
Nexen 215/55R17 (492)
Goodyear 215/55R17 (492)	
		
Availability	200 Limited	
Size and Type (Revs per kilometre)	Bridgestone 215/55R17 (492)
Nexen 215/55R17 (492)
Goodyear 215/55R17 (492)
Bridgestone 235/45R18 (492)
Nexen 235/45R18 (492)
Kuhmo 235/45R18 (490)	
		
Availability	200S	
Size and Type (Revs per kilometre)	Bridgestone 235/45R18 (492)
Kuhmo 235/45R18 (490)
Nexen 235/45R18 (492)
Nexen 235/40R19 (490)	
		
Availability	200C	
Size and Type (Revs per kilometre)	Bridgestone 215/55R17 (492)
Nexen 215/55R17 (492)
Goodyear 215/55R17 (492)
Bridgestone 235/45R18 (492)
Nexen 235/45R18 (492)
Kuhmo 235/45R18 (490)
Nexen 235/40R19 (490)