2015 Fiat 500L
CANADIAN SPECIFICATIONS

Specifications are based on the latest product information available at the time of publication. 
All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Vehicle Type	B-segment multipurpose vehicle (MPV)	
EnerGuide Vehicle Class	Station Wagon - Small	
Assembly Plant	Kragujevac (Serbia)	
Introduction Date	Mid-2013 as a 2014 model	
	
BODY/CHASSIS	
Layout	Transverse-mounted front engine, front-wheel drive	
Construction	Unitized steel body 	
	
ENGINE: 1.4-LITRE SOHC 16-VALVE TURBOCHARGED MULTIAIR® INLINE FOUR-CYLINDER	
Availability	Standard on all 500L models	
Type and Description	Inline four-cylinder, liquid-cooled, turbocharged	
Displacement	1,368 cu. cm (83.48 cu. in.)	
Bore x Stroke	72.0 x 84.0  (2.83 x 3.31)	
Valve System	Belt-driven, MultiAir, SOHC, 16 valves, hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Cast-iron block with aluminum-alloy head and aluminum-alloy bedplate	
Compression Ratio	9.8:1	
Maximum Turbo Boost	21 psi / 1.45 bar	
Power 	160 hp @ 5,500 rpm (114 hp/litre)	
Torque 	184 lb.-ft. @ 2,500-4,000 rpm	
Max. Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	87 octane (R+M)/2 acceptable 
91 octane recommended	
Oil Capacity	3.8 litres (4.0 qt.) with dry filter	
Coolant Capacity	4.4 litres (4.6 qt.)	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors and internal engine features	
Max. Gross Trailer Weight	Not rated for trailer tow	
EnerGuide 5-cycle Fuel Economy L/100km (mpg) City/Hwy*	9.3 (30) / 7.2 (39) (six-speed manual transmission)
10.0 (28) / 7.2 (39) (Euro Twin Clutch six-speed automatic transmission)
N/A (6-speed heavy-duty automatic transmission)	
Engine Assembly Plant	Termoli (Italy)	
*Based on 2014 EnerGuide fuel consumption ratings. New 5-cycle test method shown.	
		
C635 SIX-SPEED MANUAL TRANSMISSION		
Availability	Standard on all 500L models	
Description	1st, 2nd gear: Double Cone 
3rd, 4th, 5th, 6th gear: Single Cone	
Gear Ratios		
1st	4.154	
2nd	2.118	
3rd	1.361	
4th	0.978	
5th	0.756	
6th	0.622	
Reverse	4.00	
Final-drive Ratio	3.833	
Overall Top Gear	2.38	
		
C635 EURO TWIN CLUTCH SIX-SPEED TRANSMISSION	
Availability	Optional on 500L Pop	
Description	1st, 2nd gear: Double Cone 
3rd, 4th, 5th, 6th gear: Single Cone	
Gear Ratios		
1st	4.154	
2nd	2.269	
3rd	1.435	
4th	0.978	
5th	0.755	
6th	0.622	
Reverse	4.00	
Final-drive Ratio	4.118	
Overall Top Gear	2.56	
		
AISIN SIX-SPEED AUTOMATIC TRANSMISSION	
Availability	Optional on 500L Sport, Trekking and Lounge	
Gear Ratios		
1st	4.04	
2nd	2.37	
3rd	1.56	
4th	1.16	
5th	0.85	
6th	0.67	
Reverse	3.19	
Final-drive Ratio	3.683	
Overall Top Gear	2.47	
		
BRAKES		
Availability	Standard on all 500L models	
Front		
Rotor size and type	305 x 28 (12.0 x 1.10) vented	
Caliper size and type	57 (2.24) single-piston with cast iron	
Swept area	876.1 sq. cm (345 sq. in.)	
Rear		
Rotor size and type	264 x 10 (10.4 x 0.4) solid	
Caliper size and type	38 (1.49) single-piston with aluminum housing	
Swept area	591.8 sq. cm (233 sq. in.)	
		
DIMENSIONS AND CAPACITIES(a)
mm (in.) unless otherwise noted		
Wheelbase	2,611 (102.8)	
Track, Front	1,501 (59.1)	
Track, Rear	1,510 (59.4)	
Overall Length	4,249 (167.3)	
Overall Width	1,773 (69.8)   — without mirrors
2,037 (80.2)  — with mirrors	
Overall Height	1,669 (65.7)	
Ground Clearance	119 (4.7)	
Drag Coefficient (Cd) (estimated)	0.310 — 500L Pop/Sport/Lounge 
0.320 — 500L Trekking	
Curb Weight (estimated)	1,453 kg (3,203 lb.)  — (six-speed manual)
1,476 kg (3,254 lb.)  — (six-speed Euro Twin Clutch automatic)
1,475 kg (3,251 lb.)  — (six-speed automatic)	
Weight Distribution, per cent F/R	61/39 — (six-speed manual)
61/39 — (six-speed Euro Twin Clutch automatic)
58/42 — (six-speed automatic)	
Fuel Tank Capacity	50 litres (11 gal.)	
(a) All dimensions measured at curb weight with standard tires.	
		
ACCOMMODATIONS
mm (in.) unless otherwise noted		
Seating Capacity, F/R	2/3	
Front Seat		
Head room	1,034 (40.7)
1,026 (40.4) with dual-pane sunroof	
Legroom	1,016 (40.0)	
Shoulder room	1,455 (57.3)	
Hip room	1,394 (54.9)	
Total seat travel	211 (8.3)  — driver
229 (9.0)  — passenger 	
Front row interior volume	1,529 litres (54.0 cu. ft.)	
Rear Seat		
Head room	983 (38.7) 
965 (38.0) with dual-pane sunroof	
Legroom	932 (36.7) 	
Shoulder room	1,387 (54.6) 	
Hip room	1,255 (49.4)	
Total seat travel	119 (4.7)	
Second row interior volume	1,269 litres (44.8 cu. ft.)	
Total Interior Volume	2,798 litres (98.8 cu. ft.)	
Luggage Compartment Volume	603 litres (21.3 cu. ft.)	
Interior Volume Index	3,401 litres (120.1 cu. ft.)	
Trunk Liftover Height	658 (25.9)	
		
TIRES		
Availability 	Standard on 500L Pop, Sport and Lounge	
Size and Type	205/55R16 BSW All-season 	
Mfr. and Model	Continental Conti ProContact or Goodyear Eagle LS2	
Revs per km (mile)	519 (836) 	
		
Availability	Standard on 500L Trekking
Included with 17-in. wheels on 500L Lounge 	
Size and Type	225/45R17 BSW All-Season	
Mfr. and Model	Continental Conti ProContact or Goodyear Eagle LS2	
Revs per km (mile)	517 (832) 	
		
WHEELS (in.)		
Availability 	Standard on 500L Pop	
Type and Material	Steel wheels with grey painted wheel covers	
Size	16 x 6.0	
		
Availability	Standard on 500L Sport and Lounge	
Type and Material	Cast-aluminum, 13-spoke radial design, fully painted grey 	
Size	16 x 6.5	
		
Availability	Optional on 500L Sport	
Type and Material	Cast-aluminum, seven-spoke, oval-twist design, painted grey with black pockets	
Size	16 x 6.5	
		
Availability	Standard on 500L Trekking	
Type and Material	Cast-aluminum, seven-hole design, machined face with painted grey pockets	
Size	17 x 7.0	
		
Availability	Optional on 500L Trekking and Lounge	
Type and Material	Cast-aluminum, five-oval design, painted grey with grey pockets	
Size	17 x 7.0	

Availability	Optional on 500L Lounge	
Type and Material	Cast-aluminum, seven-spoke, dual-twist design, painted grey with black pockets	
Size	17 x 7.0	
		
Availability	Optional on 500L Lounge	
Type and Material	Cast-aluminum, seven-spoke, dual-twist design, painted grey with white pockets	
Size	17 x 7.0