2015 Jeep® Renegade
CANADIAN SPECIFICATIONS

Specifications are based on the latest product information available at the time of publication. 
All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Body Style 	Sport-utility vehicle (SUV)	
Assembly Plant	Melfi (Italy)	
EnerGuide Vehicle Class 	Multipurpose vehicle	
	
BODY AND CHASSIS	
Layout	Transverse front engine, 4x2 and 4x4	
Construction 	Steel uniframe	

ENGINE: 1.4-LITRE MULTIAIR® TURBO	
Availability	Standard: Renegade Sport (4x2 and 4x4) and North (4x2 and 4x4)	
Type and Description	In-line four-cylinder, liquid-cooled, turbocharged	
Displacement	1,368 cu. cm  (83.48 cu. in.)  	
Bore x Stroke	72.0 x 84.0 (2.83 x 3.31) 	
Valve System	Belt-driven, MultiAir, SOHC, 16 valves,
hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Cast-iron block with aluminum-alloy head and aluminum-alloy bedplate	
Compression Ratio	9.8:1	
Maximum Turbo Boost (psi / bar)	22 psi / 2.49 bar	
Power 	160 horsepower @ 5,500 rpm	
Torque 	184 lb.-ft. @ 2,500-4,000 rpm	
Max. Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	87 octane (R+M)/2 acceptable 
91 octane recommended	
Oil Capacity	3.8 litres (4.0 qt.) with dry filter	
Coolant Capacity	5.2 litres (5.5 qt.) 	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors and internal engine features	
Fuel Economy 	TBD	
Towing	Not recommended 	
Engine Assembly Plant	Dundee, Michigan (U.S.A.)	
ENGINE: 2.4-LITRE MULTIAIR TIGERSHARK 		
Availability	Standard: Renegade Limited (4x2 and 4x4) and Trailhawk (4x4)
Available: Renegade Sport and North (4x2 and 4x4)	
Type and Description	In-line four-cylinder, 16-valve MultiAir with multiport fuel injection	
Displacement	2,360 cu. cm (144 cu. in.)  	
Bore x Stroke	88 X 97 (3.46 X 3.82) 	
Valve System	SOHC, four valves per cylinder 	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum block, aluminum cylinder head	
Compression Ratio	10:1	
Power 	180 horsepower @ 6,400 rpm	
Torque 	175 lb.-ft. @ 4,400 rpm	
Max. Engine Speed	6,500 rpm	
Fuel Requirement	Unleaded regular, 87 octane	
Oil Capacity	5.2 litres (5.5 qt.) (total)	
Coolant Capacity	6.45 litres (6.8 qt.) 	
Emission Controls	Single catalytic converter, heated wide band lambda sensor upstream and mid-catalyst heated oxygen sensor	
Fuel Economy 	TBD 	
Towing	907 kg  (2,000 lb.) 	
Engine Assembly Plant 	Dundee Engine Plant, Dundee, Mich. (U.S.A.)	
		
TRANSMISSION: 948TE NINE-SPEED AUTOMATIC	
Availability	2.4-litre MultiAir Tigershark engine (4x2 or 4x4)	
Description 	Planetary gear train, transverse layout	
Ratio Spread	9.81	
Gear Ratios		
1st	4.71	
2nd	2.84	
3rd	1.91	
4th	1.38	
5th	1.00	
6th	0.81	
7th	0.70	
8th	0.58	
9th	0.48	
Reverse	3.83	
Axle Ratios	2.4-litre 4x2  — 3.734
2.4-litre 4x4  — 3.734 
2.4-litre 4x4 (Trailhawk) — 4.334	
		
C635 SIX-SPEED MANUAL TRANSMISSION		
Availability	1.4-litre MultiAir Turbo engine (4x2 or 4x4)	
Description	1st, 2nd, 3rd gear: Triple cone 
4th: Double cone	
Gear Ratios		
1st 	4.154	
2nd	2.118	
3rd	1.361	
4th	0.978	
5th	0.756	
6th	0.622	
Reverse	4.00	
Final-drive Ratio	4.438 / 4.438 / 3.579 / 3.833	
Overall Top Gear	2.38	
		
4X4 SYSTEMS: JEEP ACTIVE DRIVE, JEEP ACTIVE DRIVE LOW	
Availability 	Jeep Active Drive is standard on Sport 4x4, North 4x4 and Limited 4x4
Jeep Active Drive Low is standard on Trailhawk	
Type	Fully disconnecting 4x2 mode with automatic 4x4 engagement
Full-time 4x4 mode with active on demand clutch	
Operating Modes	Auto 4x2/4x4, Neutral	
Centre Differential Type	None	
Terrain Response	Unique tuning in all terrain modes	
Crawl Ratio	20:1 (with Jeep Active Drive Low)	
		
ELECTRICAL SYSTEM		
Alternator 	150-amp (1.4-litre MultiAir Turbo) 
160-amp (2.4-litre Tigershark w/ MultiAir)  	
Battery	500-amp  (1.4-litre MultiAir Turbo)
600-amp (2.4-litre Tigershark w/ MultiAir) 	
		
SUSPENSION		
Front 	McPherson strut, coil springs, flat front steel crossmember, high-strength steel double shell lower control arms for 4x4 and high-strength steel mono shell lower control arms for 4x2, stabilizer bar	
Rear	Chapman strut, high-strength steel links, isolated steel rear cradle for 4x4 and not-isolated for 4x2, coil springs, stabilizer bar	
		
STEERING		
Type 	Electric power rack and pinion	
Overall Ratio 	15.7 	
Turning Diameter (curb-to-curb) 	11.07 m (36.3 ft.)  4x2 and 4x4
10.76 m (35.3 ft.) Trailhawk 4x4	
Steering Turns (lock-to-lock)	2.68 (4x2 and 4x4)
2.76 (Trailhawk 4x4)	
		
BRAKES
mm (in.) unless otherwise noted		
Front		
Size and Type	305 x 28 (12 x 1.1) vented rotor with 
60 (2.36) single-piston floating caliper	
	281 x 26 (11.06 x 1) vented rotor with
57 (2.24) single-piston floating caliper	
Swept Area (per caliper)	895.3 sq. cm (138.77 sq. in.), 1 x 60
747.6 sq. cm  (115.88 sq. in.), 1 x 57 	
Rear		
Size and Type 	278 x 12 (10.95 x 0.47) solid rotor with 
38 (1.5) single-piston floating caliper	
Swept Area (per caliper)	656.4 sq. cm (101.7 sq. in.), 1 x 38	
Power-assist Type 	254 (10) vacuum assist 	
Four-wheel anti-lock brake system (ABS)	Standard	
Electronic Stability Control (ESC)	Standard	
Parking Brake Type	Electric motor on caliper	
		
DIMENSIONS AND CAPACITIES
mm (in.) unless otherwise noted		
Wheelbase	2,570 (101.2) 	
Track, Front	1,539 (60.6) 	
Track, Rear	1,539 (60.6) 	
Overall Length	4,232 (166.6) 	
Overall Width	1,803 (71.0) 	
Overall Width (with folded side mirrors)	1,887 (74.2)	
Overall Width (with open side mirrors)	2,023 (79.6)	
Overall Height 	1,689 (66.5) 	
Load-floor height	757 (29.8) 	
Sill-step height	493 (19.4) front, 498 (19.6) rear	
Ground Clearances 
	170 (6.7) 4x2
201 (7.9) 4x4 
221 (8.7) Trailhawk 4x4 	
Approach Angle, (with air dam) (degrees)	17.9 4x2
21.0 4x4
30.5 Trailhawk 4x4	
Breakover Angle (degrees)	21.2 4x2
24.0 4x4
25.7 Trailhawk 4x4	
Departure Angle (degrees)	29.7 4x2
32.1 4x4 
34.3 Trailhawk 4x4	
Curb Weight kg (lb.)	1,372 (3,025) 4x2 and 1.4-litre MultiAir Turbo 
1,447 (3,190) 4x4 and 1.4-litre MultiAir Turbo
1,418 (3,126) 4x2 and 2.4-litre MultiAir Tigershark
1,502 (3,311) 4x4 and 2.4-litre MultiAir Tigershark
1,583 (3,490) Trailhawk 4x4 with 2.4-litre MultiAir Tigershark	
Aero Cd	0.350 4x2
0.360 4x4
0.370 Trailhawk 4x4	
Fuel-tank Capacity	48 litres (10.6 imperial gallons.) 	
		
ACCOMMODATIONS
mm (in.) unless otherwise noted		
Seating Capacity — Front/Rear 	2/3	
Front Row		
Head Room without Sunroof	1,044 (41.1) 	
Head Room with Sunroof	1,008 (39.7) 	
Legroom 	1,046 (41.2) 	
Shoulder Room 	1,420 (55.9) 	
Hip Room	1,349 (53.1) 	
Seat Travel 	229 (9.0) driver / 259 (10.2) front passenger	
Recliner Range (degrees)	From 25 nominal, 38 forward and 30 rearward (from vertical 13 forward, 55 rearward)	
Volume (standard roof) 	1,552 litres (54.8 cu. ft.)	
Second Row		
Head Room 	1,029 (40.5) 	
Legroom 	892 (35.1) 	
Shoulder Room 	1,400 (55.1) 	
Hip Room	1,318 (51.9) 	
Volume	1,283 litres (45.3 cu. ft.)	
Cargo Access		
Liftover Height	767 (30.2) 	
Maximum Cargo Width at 
Liftgate Opening	1,019 (40.1) 	
Minimum Cargo Width at 
Liftgate Opening 	991 (39.0) at bottom of opening	
Maximum Cargo Height at 
Liftgate Opening	749 (29.5) 	
Minimum Cargo Height at 
Liftgate Opening	737 (29.0) 	
Distance Between Wheelhouse 
Interior Trim	955 (37.6) 	
Cargo Volume		
Rear Seats Up	524 litres (18.5 cu. ft.)	
Rear Seats Folded	1,438 litres (50.8 cu. ft.)	
Interior Volume Index	3,358 litres (118.6 cu. ft.) 	
Behind Rear Seat	524 litres (18.5 cu. ft.) (rear seat at design position)	
Behind Front-row Seats 
with Rear Seats Folded	1,438 litres (50.8 cu. ft.)	
		
TIRES		
Availability	Standard on Sport / North 	
Size and Type 	215/65R16 BSW, All-season 	
Mfr. and Model 	Continental, CrossContact LX Sport	
Revs per km (mile) 	464 (749)	
		
Availability	Standard on North (with 2.4-litre Tigershark w/ MultiAir) 	
Size and Type 	215/60R17 BSW, All-season 	
Mfr. and Model 	Continental, CrossContact LX Sport	
Revs per km (mile)	478 (768) 	
		
Availability	Standard on Limited 
Optional on North 	
Size and Type 	225/55R18 BSW, All-season 	
Mfr. and Model	Goodyear Eagle Sport or Kumho KL33 	
Revs per km (mile)	452 (729) 	
		
Availability	Standard on Trailhawk  	
Size and Type	215/65R17 OWL, All-season	
Mfr. and Model	Goodyear Wrangler SRA or Falken Wildpeak 	
Revs per km (mile)	448 (722)