2015 Jeep® Wrangler Unlimited
CANADIAN SPECIFICATIONS

Specifications are based on the latest product information available at the time of publication. 
All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions measured at curb weight with standard tires and wheels.

General Information		
Vehicle Type	Four-door sport-utility vehicle	
Assembly Plant	Toledo, Ohio (U.S.A)	
Vehicle Class	Multi-purpose vehicle	
Introduction Date	1987 	
		
BODY/CHASSIS		
Layout	Longitudinal front engine, four-wheel drive	
Construction	Ladder-type frame, open steel body	
		
Engine:  3.6-LITRE PENTASTAR™ V6		
Availability	Standard on all models	
Type and Description	60-degree, V-type, liquid-cooled	
Displacement 	3,604 cu. cm (220 cu. in.)	
Bore x Stroke 	96 x 83 (3.78 x 3.27)	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless 	
Construction	Aluminum deep-skirt block, aluminum alloy heads 	
Compression Ratio	10.2:1	
Power 	285 hp at 6,400 rpm	
Torque 	260 lb.-ft. at 4,800 rpm	
Max. Engine Speed 	6,600 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R + M)/2	
Oil Capacity 	5.7 litres (6.0 qt.)	
Coolant Capacity 	13.25 litres (14 qt.)	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors
and internal engine features	
EnerGuide Fuel Economy 
L/100 km (mpg), City/Hwy*	Automatic - 14.8 (19) / 11.7 (24) Manual - 15 (19) / 11.4 (25) 	
Engine Assembly Plant	Trenton, Mich. (U.S.A.)	
*Based on 2015 EngerGuide fuel consumption ratings. 5-cycle test method used.	
Transmission: W5A580 automatic, five speed overdrive	
Availability	Optional on all models	
Description	Adaptive electronic control or Electronic Range Select (ERS) 
driver-interactive manual control and electronically modulated 
torque converter clutch	
Gear Ratios Automatic		
1st	3.59	
2nd	2.19	
3rd	1.41	
4th	1	
5th	0.83	
Reverse	3.16	
Final Drive Ratio	3.06:1	
Overall Top Gear	2.54	
		
Transmission: NSG 370 Manual, Six speed with overdrive	
Availability	Standard on all models	
Description	Synchronized in all forward gears and Reverse, 
multi-rail shift system with top-mounted shift lever	
Clutch	Hydraulic actuation	
Gear Ratios		
1st	4.46	
2nd	2.61	
3rd	1.72	
4th	1.25	
5th	1	
6th	0.797	
Reverse	4.06	
Final Drive ratio	3.21 standard, 3.73 optional (4.10 Rubicon)	
Overall Top Gear	2.53 standard, 2.95 optional (3.24 Rubicon)	
		
TRANSFER CASE: NV241 command-trac	
Available	Standard on Sport and Sahara	
Type	Part-time	
Operating Modes	2WD High; 4WD High; Neutral; 4WD Low	
Centre Differential Type	None	
Low Range Ratio	2.72:1	
TRANSFER CASE: NV241OR Rock-trac	
Available	Standard Rubicon	
Type	Part-time	
Operating Modes	2WD High; 4WD High; Neutral; 4WD Low	
Centre Differential Type	None	
Low Range Ratio	4.0:1	
Axle Ratio 	3.21 standard, 3.73 optional (3.73 standard Rubicon with automatic) 
4.10 standard Rubicon with manual (optional for automatic)	
Overall Top-gear		2.53 standard, 2.95 optional  (2.95 standard Rubicon with automatic, 
3.24 standard Rubicon with manual (optional for automatic)	
		
Axles		
Front   	Dana 30, Dana 44 on Rubicon models	
Differential Type	Open (Dana 30) or Tru-Lok electronic locking (Dana 44)	
Axle Ratios 	3.21, 3.73, 4.10	
Rear  	Dana 44	
Differential Type	Open (Sport and Sahara) with available Trac-Lok anti-spin, Tru-Lok electronic locking (Rubicon)	
Axle Ratios 	3.21, 3.73, 4.10	
		
Electrical System		
Alternator	160 amp	
Battery	600 CCA, maintenance free	
		
Suspension		
Front	Live axle, Link coil, leading arms, track bar, coil springs, stabilizer bar	
Stabilizer bar	Electronic Sway-Bar Disconnect System — Standard, Rubicon	
Shock type	Low-pressure (on 16-in. wheel packages) gas-charged shock absorbers — Standard	
	Monotube high-pressure (on 17- and 18-in. wheel packages) 
gas-charged shock absorbers — Standard	
Rear	Live axle, Link coil, trailing arms, track bar, coil springs, stabilizer bar	
Shock type	Low-pressure (on 16-in. wheel packages) gas-charged shock absorbers — Standard	
	Monotube high-pressure (on 17- and 18-in. wheel packages) 
gas-charged shock absorbers — Standard	
		
STEERING		
Type	Power, recirculating ball with damper	
Overall Ratio	16.7:1 overall	
Turning Diameter (curb-to-curb) 	10.62 m (34.9 ft.)	
Steering Turns (lock-to-lock)	3.5	
P/S pump	Hydraulic	
		
BRAKES		
Type	Power-assisted, anti-lock braking system 	
Availability	Standard	
Front		
Rotor size and type	302 x 28 (11.9 x 1.1) vented rotor	
Caliper size and type	254 (10) single-diaphragm vacuum	
Rear		
Rotor size and type	302 x 28 (11.9 x 1.1) vented rotor	
Caliper size and type	66 (2.6) single-piston floating caliper	
		
Dimensions and Capacities 
mm (in.) unless otherwise noted		
Wheelbase	2,947 (116)	
Overhang — Front 	679 (26.7) 	
Overhang — Rear	778 (30.6) 	
Track — Front	1,572 (61.9) 	
Track — Rear	1,572 (61.9) 	
Overall Length	3,881 (152.8) 	
Overall Width	1,872 (73.7) 	
Overall Height	1,800 (70.9) 	
Liftover Height 	706 (27.8) 	
Cargo Width at Swing-Gate Opening	1,491 (58.7) 	
Cargo Height at Swing-Gate Opening	942 (37.1) 	
Load Floor Height	706 (27.8) 	
		
CLEARANCES		
	P225/75R16	P255/75R17	P255/70R18	LT255/75R17	
Approach Angle, Deg. 	40.6	43.6	44.4	44.4	
Breakover Angle, Deg. 	17.8	20.3	20.9	20.8	
Drture Angle, Deg. 	37.4	40.3	40.7	40.5	
Front Axle to Ground 	229 (9.0)	259 (10.2)	267 (10.5)	267 (10.5)	
Rear Axle to Ground 	221 (8.7)	254 (10.0)	259 (10.2)	257 (10.1)	
Fuel Tank Capacity	85 litres (18.7 gal.)	
		
CURB WEIGHT		
Wrangler Sport, Manual Transmission	1,848 kg  (4,075 lb.) 	
Wrangler Sport, Automatic Transmission	1,860 kg (4,100 lb.)	
Wrangler Sahara, Manual Transmission	1,936 kg (4,269 lb.) 	
Wrangler Sahara, Automatic Transmission	1,948 kg (4,294 lb.) 	
Wrangler Rubicon, Manual Transmission	1,957 kg (4,315 lb.) 	
Wrangler Rubicon, Automatic Transmission	1,969 kg (4,340 lb.) 	
		
Accommodations 
mm (in.) unless otherwise noted		
Seating Capacity (front/rear) 	2/3	
Total Interior Passenger Volume	2,945 litres (104 cu. ft.)	
Front		
Head Room	1,048.4 (41.3) 	
Legroom	1,041.4 (41.0) 	
Shoulder Room	1,416.7 (55.8) 	
Hip Room	1,412.8 (55.6) 	
Seat Travel	239.5 (9.4) 	
 Front Volume Index	1,546 litres (54.6 cu. ft.)  	
Rear		
Head Room	1,025 (40.4) 	
Legroom	944.8 (37.2) 	
Knee Clearance	1,566 (61.6) 	
Shoulder Room	1,443 (56.8) 	
Hip Room	1,440 (56.7) 	
 Rear Seat Volume Index 	1,399 litres (49.4 cu.ft.)	
Liftover Height	798 (31.4) 	
Maximum Cargo Width 
at Liftgate Opening	1,491 (58.7) 	
Minimum Cargo Width 
at Liftgate Opening	1,047 (41.2) 	
Maximum Cargo Height 
at Liftgate Opening	942 (37.1) 	
Minimum Cargo Height 
at Liftgate Opening	940 (37.0) 	
Distance between Wheelhouse 
Interior Trim	1,135 (44.7) 	
Cargo Volume		
Rear Seat Folded	1,999 litres (70.6 cu. ft.) 	
Rear Seat Upright	892 litres (31.5 cu. ft.) 	
Total Passenger plus Cargo Volume, 	4,259 litres (150.4 cu. ft.)	
		
WHEELS (in.)		
Availability	Standard on Wrangler Unlimited Sport	
Type and Material	Painted steel, available Low Gloss Black painted 	
Size	16 x 7.0 	
		
Availability	Standard on Wrangler Unlimited Sahara 	
Type and Material	Painted and polished cast-aluminum	
Size	18 x 7.5 	
		
Availability	Standard on Wrangler Unlimited Rubicon 	
Type and Material	Painted and polished cast-aluminum	
Size	17 x 7.5	
		
TIRES		
Availability	Standard on Wrangler Unlimited Sport	
Size and Type 	P225/75R16, on/off-road, black sidewall	
Mfr. and Model	Goodyear Wrangler ST	
Revs per km (miles)	441 (712)	
		
Availability	Available on Wrangler Unlimited Sport	
Size and Type	P245/75R16, on/off-road, OWL	
Mfr. and Model	Bridgestone Dueler A/T Revo2	
Revs per km (miles)	424 (684)	
		
Availability	Standard on Wrangler Unlimited Sahara	
Size and Type	P255/70R18, on/off-road, OWL	
Mfr. and Model	Bridgestone Dueler 693	
Revs per km (miles)	404 (653)	
		
Availability	Standard on Wrangler Unlimited Rubicon	
Size and Type	LT255/75R17, on/off-road, black sidewall	
Mfr. and Model	BF Goodrich Mud Terrain	
Revs per km (miles)	403 (650)	
Parking Brake Type	Drum-in-hat	
		
Power-assist Type		
Four–wheel Anti-lock Brakes	Standard	
Electronic stability control	Standard	
All-speed traction control	Standard	

Towing Capacities kg (lb.)	
WRANGLER UNLIMITED SPORT 4WD 	
Engine	Trans
Type	Transmission	Axle
Ratio	Payload	Base Wt.	Base Wt.
Front	Base Wt.
Rear	GAWR
Front	GAWR
Rear	GCWR	Max 
Trailer	
3.6L V6 gas (EGT) 	M6	NSG370 6-SPD MANUAL (DEH)	3.21	454 (1000)	1940 (4277)	1015 (2238)	925 (2039)	1259 (2775)	1451 (3200)	2915
(6427)	907 (2000)	
3.6L V6 gas (EGT)	M6	NSG370 6-SPD MANUAL (DEH)	3.73	454 (1000)	1940 (4277)	1015 (2238)	1016 (2039)	1259 (2775)	1451 (3200)	3596 (7927)	1588 (3500)	
3.6L V6 gas (EGT)	A5	WA580 5-SPD AUTO (DGL)	3.21	454 (1000)	2232
(4921)	1015 (2237)	932 (2054)	1259 (2775)	1451 (3200)	2922 (6441)	907 (2000)	
3.6L V6 gas (EGT)	A5	WA580 5-SPD AUTO (DGL)	3.73	454 (1000)	  1946
(4291)	1007
(2237)	932 (2054)	1259 (2775)	1451 (3200)	3602 (7941)	1588 (3500)	
1. GCWR = Base Weight + Maximum Trailer Weight + 68 kg (150 lb.) for driver.	

WRANGLER UNLIMITED SAHARA 4WD kg (lb.)	
Engine	Trans
Type	Transmission	Axle
Ratio	Payload	Base Wt.	Base Wt.
Front	Base Wt.
Rear	GAWR
Front	GAWR
Rear	GCWR	Max 
Trailer	
3.6L V6 gas (EGT) 	M6	NSG370 6-SPD MANUAL (DEH)	3.21	399 (880)	1994
(4397)	1031 (2273)	972
(2142)	1259 (2775)	1451 (3200)	2970 (6547)	907 (2000)	
3.6L V6 gas (EGT)	M6	NSG370 6-SPD MANUAL (DEH)	3.73	399 (880)	1994
(4397)	1031 (2273)	972
(2142)	1259 (2775)	1451 (3200)	3650 (8047)	1588 (3500)	
3.6L V6 gas (EGT)	A5	WA580 5-SPD AUTO (DGL)	3.21	399 (880)	2001
(4411)	1031 (2283)	970 (2139)	1259 (2775)	1451 (3200)	2976 (6561)	907 (2000)	
3.6L V6 gas (EGT)	A5	WA580 5-SPD AUTO (DGL)	3.73	399 (880)	2001
(4411)	1031 (2272)	970 (2139)	1259 (2775)	1451 (3200)	3656 (8061)	1588 (3500)	
1. GCWR = Base Weight + Maximum Trailer Weight + 68 kg (150 lb.) for driver.	
	
WRANGLER UNLIMITED RUBICON 4WD kg (lb.)	
Engine	Trans
Type	Transmission	Axle
Ratio	Payload	Base Wt.	Base Wt.
Front	Base Wt.
Rear	GAWR
Front	GAWR
Rear	GCWR	Max 
Trailer	
3.6L V6 gas (EGT)	M6	NSG370 6-SPD MANUAL (DEH)	4.10	405 (892)	2051 (4521)	1067 (2352)	984 (2170)	1259 (2775)	1451 (3200)	3706 (8171)	1588 (3500)	
3.6L V6 gas (EGT)	A5	WA580 5-SPD AUTO (DGV)	3.73	405 (892)	2057 (4535)	1066 (2350)	991 (2185)	1259 (2775)	1451 (3200)	3712 (8185)	1588 (3500)	
3.6L V6 gas (EGT)	A5	WA580 5-SPD AUTO (DGV)	4.10	405 (892)	2057 (4535)	1066 (2350)	991 (2185)	1259 (2775)	1451 (3200)	3712 (8185)	1588 (3500)	
1. GCWR = Base Weight + Maximum Trailer Weight + 68 kg (150 lb.) for driver.