2015 Ram C/V (Cargo Van)
CANADIAN SPECIFICATIONS

Specifications are based on the latest product information available at the time of publication. 
All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Vehicle Type	Multipurpose vehicle, front-wheel drive	
Assembly Plant	Windsor, Ontario 	
EnerGuide Vehicle Class	Multipurpose vehicle	
Introduction date	August 2011 as a 2012 model year 	
		
BODY/CHASSIS		
Layout	Transverse front engine, front-wheel drive	
Construction	Unitized steel with hinged front doors; sliding left and right side doors — rear liftgate with gas props	
	
ENGINE: 3.6-Litre, GASOLINE, DOHC, 24-VALVE, V6	
Availability	Standard	
Type and Description	60-degree bank angle, liquid-cooled, with three-plenum intake manifold, electronically-controlled manifold tuning valve and short-runner valves	
Displacement 	3,605 cu. cm (220 cu. in.)	
Bore x Stroke	96 x 83 (3.78 x 3.27)	
Valve System	DOHC, 24 valves, hydraulic, roller finger followers	
Fuel Injection	Sequential, multi-port, electronic	
Construction	High-pressure die-cast A380 aluminum block with iron liners and semi-permanent mould A319 aluminum heads	
Compression Ratio	10.2:1 	
Power 	283 bhp  @ 6,400 rpm	
Torque 	260 lb.-ft.  @ 4,400 rpm	
Max. Engine Speed	6,800 rpm (electronically limited)	
Fuel Requirement	Unleaded mid-grade, 89 octane (R+M)/2 — preferred
Unleaded regular, 87 octane (R+M)/2 — acceptable	
Oil Capacity	5.88 litres (6 qt.) with dry filter	
Coolant Capacity	9.75 litres (10.3 qt.)	
Emission Controls 	Dual catalytic converter, four heated oxygen sensors, electronic EGR and internal engine features	
EnerGuide 5-Cycle Fuel Economy L/100 km (mpg) City/Hwy*	 13.3 (21) / 9.1 (31)*	
*Based on 2014 EnerGuide fuel consumption ratings for Ram C/V. 5-cycle test method used.	
Assembly Plant	Trenton, Michigan (U.S.A.)	
*Based on 2014 Energuide fuel consumption ratings. 5-cycle test method used.	
	
TRANSAXLE: 62TE, Automatic Six-Speed Overdrive	
Availability	Standard	
Description	Six-speed, adaptive electronic control, electronically-modulated torque converter clutch, Electronic Range Select (ERS)	
Gear Ratios		
1st	4.127	
2nd	2.842	
3rd	2.283	
4th	Upshift – 1.452 WOT kickdown – 1.570 	
5th 	1.0	
6th 	0.690	
Reverse	3.214	
Transfer Ratio	0.95	
Final Drive Ratio	3.16	
Overall Top Gear	2.24		
	
ELECTRICAL SYSTEM		
Alternator	160 amp	
Battery	730 CCA, maintenance-free	
	
SUSPENSION		
Front	Independent MacPherson strut, coil over gas-charged shock absorbers, stabilizer bar with isolated suspension cradle	
Rear	Twist-beam axle with coil springs, track bar 	
		
STEERING		
Type	Power rack and pinion	
Overall Ratio	14.3:1	
Turning Diameter (curb-to-curb)	11.92 m (39.1 ft.)	
Steering Turns (lock-to-lock)	2.90	

BRAKES 
mm (in.) unless otherwise noted		
Power Assist Type	All —230 x 230 (9 x 9) tandem-diaphragm vacuum — standard	
Power Assist Type	All — 204 x 230 (8 x 9) tandem-diaphragm vacuum — optional	
Availability	Standard on all models	
Front		
Size and Type	330 x 28 (13.0 x 1.1) vented rotors with 51 mm single-piston caliper — standard	
Swept Area (total front)	475 sq. cm (73.6 sq. in.) — standard	
Size and Type	302 x 28 (11.9 x 1.1) vented rotors with 66 mm single-piston caliper  —optional	
Swept Area (total front)	350 sq. cm (54.3 sq. in.) — optional	
Rear		
Size and Type	328 x 12 (12.9 x 0.47) solid rotors with 45 mm single-piston IPB caliper — standard	
Swept Area (total rear)	429 sq. cm (66.5 sq. in.) — standard	
Size and Type	305 x 12 (12.0 x 0.47) solid rotors with 42 mm single-piston IPB caliper - Optional	
Swept Area (total rear)	350 sq. cm (54.3 sq. in.) — optional	
Parking Brake Type	Integral parking brake	
Four-wheel Anti-lock brakes	Standard	
Electronic Stability Control 	Standard	
All-speed traction control	Standard	
		
DIMENSIONS AND CAPACITIES 
mm (in.) unless otherwise noted		
Wheelbase	3,078 (121.2)	
Overhang — Front	960 (37.8)	
Overhang — Rear	1,113 (43.8) 	
Track — Front	1,664 (65.5) 	
Track — Rear	1,646 (64.8) 	
Overall Length	5,151 (202.8) 	
Overall Width	1,999 (78.7) 	
Overall Width with Mirrors	2,273 (89.5) 	
Overall Height 	1,753 (69.0) 	
Liftover Height 	665 (26.2) 	
Cargo Width at Wheelhouse 	1,237 (48.7) 	
Maximum Cargo Height 	1,224 (48.2) 	
Angle of Approach (curb load) (degrees)	13.9	
Angle of Departure (curb load) (degrees)	20.6	
Breakover Angle (curb load) (degrees)	14.2	
Minimum Running Ground Clearance 
(curb load)	163 (6.4)	
Fuel Tank Capacity	76 litres (17 gal.)	
Gross Vehicle Weight Rating (GVWR)	2,744 kg (6,050 lb.) 	
Towing Capacity	1,633 kg (3,600 lb.)	
Curb Weight	1,882 kg (4,150 lb.) 	
Payload	816 kg (1,800 lb.) 	
Weight Distribution % F/R	59/41	
		
ACCOMMODATIONS 
mm (in.) unless otherwise noted		
Seating Capacity — F/I/R	2	
Front		
Head Room	1,011 (39.8) 	
Head Room with Sunroof 	945 (37.2) 	
Legroom	1,034 (40.7) 	
Shoulder Room	1,618 (63.7) 	
Hip Room	1,483 (58.4) 	
Seat Travel	221 (8.7) 	
Cargo Volume 		
Maximum Cargo Volume 	4,403 litres (155.5 cu. ft.) 	
Total Passenger plus Cargo Volume	5,544 litres (195.8 cu. ft.)	
	
WHEELS (in.)	
Availability	Standard	
Type and Material	Painted steel with bolt-on wheel cover	
Size	17 x 6.5	
		
TIRES 		
Availability	Standard	
Size and Type	225/65R17 BSW, All-season	
Model	Yokohama Avid S33	
Revs per km (mile)	456 (728)