2015 Ram ProMaster City
CANADIAN SPECIFICATIONS

Specifications are based on the latest product information available at the time of publication. 
All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Body Styles	ProMaster City Cargo Van 
ProMaster City Wagon	
Wheelbase	2,855 (122.4)	
Assembly Plant	Bursa (Turkey)	
		
ENGINE: 2.4-LITRE 24-VALVE DOHC I-4		
Description	Inline four-cylinder, 16-valve MultiAir2 with multiport fuel injection	
Displacement	2,360 cu. cm (144 cu. in.) 	
Bore x Stroke	88mm x 97mm	
Valve System	SOHC, four valves per cylinder (16 total)	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads	
Compression Ratio	10:1	
Power 	178 hp @ 6,400 rpm	
Torque 	174 lb.-ft. @ 3,900 rpm	
Max. Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane	
Oil Capacity	5.2 litres (5.5 qt.)	
Coolant Capacity	6.7 litres (7.1 qt.) 	
Emission Controls	Single catalytic converter, heated wide band lambda sensor upstream and mid-catalyst heated oxygen sensor	
		
TRANSMISSION: 948TE NINE-SPEED AUTOMATIC	
Description 	Planetary gear train, transverse layout	
Availability	Standard on all models	
Ratio Spread	9.79	
Gear Ratios		
1st	4.70	
2nd 	2.84	
3rd 	1.90	
4th	1.38	
5th	1.00	
6th	0.80	
7th	0.69	
8th	0.58	
9th	0.47	
Axle	3.73	
		
ELECTRICAL SYSTEM		
Alternator	160-amp	
Battery	95 amp with 700 CCA	
		
BODY AND CHASSIS		
Layout	Transverse front engine	
Construction	Unibody