2016 Chrysler 200
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Body Style	Four-door sedan 	
Assembly Plant 	Sterling Heights, Michigan (U.S.A.)	
EnerGuide Vehicle Class	Mid-size sedan 	
		
BODY AND CHASSIS		
Layout 	Transverse front engine with front-wheel drive (FWD) or all-wheel drive (AWD)	
Construction 	Steel uni-frame	
		
ENGINE: 2.4-LITRE MULTIAIR2 TIGERSHARK, I-4 WITH ENGINE 	
Availability	Standard — all models	
Type and Description	Four-cylinder inline, 16-valve MultiAir2 with multiport fuel injection	
Displacement	2,360 cu. cm (144 cu. in.)	
Bore x Stroke	88 x 97 (3.46 x 3.82)	
Valve System	SOHC, 16 valves (4 valves per cylinder)  	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	High-pressure die-cast aluminum block with dry iron liners, cast-aluminum cylinder heads, cast-aluminum ladder frame, forged-steel crankshaft	
Compression 	10.0:1	
Power 	184 hp @ 6,250 rpm (preliminary)	
Torque	173 lb.-ft. @ 4,600 rpm (preliminary)	
Max. Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane	
Oil Capacity	5.2 litres (5.5 qt.) 	
Coolant Capacity	7.1 litres (7.5 qt.) 	
Emission Controls	GPEC3 engine-management system with close-coupled catalyst; and wide range O2 sensor (a)	
Engine Assembly Plant	Dundee, Michigan (U.S.A.)	
2915 EnerGuide Fuel Economy L/100km (mpg) city/hwy 	10.2 (28) / 6.4 (44) 	
	
ENGINE: 3.6-LITRE PENTASTAR™ V6	
Availability	Optional — Limited, 200S and 200C models 	
Type and Description	60-degree bank angle, liquid-cooled, three-plenum intake manifold with electronically-controlled manifold tuning valve and short-runner valves 	
Displacement	3,605 cu. cm (220 cu. in.)	
Bore x Stroke	96 x 83 mm (3.78 x 3.27)	
Valve System	Chain-drive DOHC, 24 valves (4 valves per cylinder), hydraulic end-pilot roller rockers, variable cam phasing on intake and exhaust cams 	
Fuel Injection	Sequential, multiport, electronic	
Construction	High-pressure die-cast A380 aluminum block with iron liners and 
semi-permanent mould A319 aluminum heads	
Compression Ratio	10.2:1	
Power 	295 bhp @ 6,350 rpm  	
Torque 	262 lb.-ft. @ 4,250 rpm 	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity	5.7 litres (6 qt.) with dry filter SAE 5W30	
Coolant Capacity	8.12 litres (8.58 qt.) 	
Emission Controls	Integrated cast-aluminum header manifolds; positive crankcase ventilation; 
inlet and exhaust cam phasers with internal exhaust gas recirculation 
(no EGR/AIR required); evaporative emissions system	
2015 EnerGuide Fuel Economy L/100km (mpg) city/hwy	FWD 12.4 (23) / 7.5 (38
AWD 12.8 (22) / 8.1 (35) 	
Engine Assembly Plant	Trenton, Michigan (U.S.A.)	
	
TRANSMISSION: 948TE/9HP48, AUTOMATIC NINE-SPEED 	
Availability	Standard — all models	
Description	Nine-speed FWD/AWD, electronically-controlled automatic overdrive transmission with torque converter clutch. Clutch-to-clutch architecture, 
with integral electro/hydraulic controls module	
Gear Ratios		
1st 	4.71 	
2nd	2.84    	
3rd	1.91	
4th 	1.38  	
5th	1.00	
6th	0.81	
7th	0.70	
8th	0.58	
9th	0.48	
Reverse 	3.81    	
Spread	9.81	
Final Drive Ratio – 948TE	3.73 with 2.4-litre engine	
Final Drive Ratio – 9HP48	4.08 with 3.6-litre engine	
		
ELECTRICAL SYSTEM		
Alternator 	160-amp	
Battery	600-amp maintenance-free (LX, Limited) 
730-amp (200S, 200C)	
		
SUSPENSION		
Front	MacPherson strut, dual reacting twin tube shock absorbers	
Rear 	Multi-link independent dual reacting twin tube shock absorbers 	
		
STEERING		
Type	Electric power rack and pinion 	
Overall Ratio	15:2 (FWD and AWD)	
Turning Diameter (curb-to-curb)	FWD/AWD 12.13 m (39.8 ft.) 	
Steering Turns (lock-to-lock)	2.67	
		
BRAKES 
mm (in.) unless otherwise noted		
Power-assist Type	Vacuum assist	
Availability	Standard on Touring and Limited models 	
Front		
Size and Type	2.4-litre: (305 x 28) rotors with (60.0) single-piston floating caliper
3.6-litre: (330 x 28) rotors with (60.0) single-piston floating caliper	
Swept Area (Total Front)	2.4-litre: 820.08 sq. cm (127.11 sq. in.) 
3.6-litre: 901.76 sq. cm (139.77 sq. in.) 	
Rear		
Size and Type	(278 x 12) rotors with (38.0) single-piston aluminum caliper	
Swept Area (Total Rear)	638.6 sq. cm (98.98 sq. in.)	
Parking Brake Type	Electronic park brake 	
Anti-lock Brake System (ABS)	Standard    	
		
Electronic Stability Control (ESC) 	Standard	
Traction Control	Standard	
Brake Assist	Standard	
		
DIMENSIONS AND CAPACITIES 
mm (in.) unless otherwise noted		
Wheelbase	2,742 (108.0) 	
Track, Front	1,578 (62.1) 	
Track, Rear	1,576 (62.0) 	
Overall Length	4,885 (192.3) 	
Overall Width	1,871 (73.6) 	
Overall Height	1,491 (58.7) 	
Front Overhang	1,039 (40.9) 	
Rear Overhang	1,103 (43.4) 	
Approach Angle (Deg.)	13.5	
Departure Angle (Deg.)	17.8	
Ground Clearance	3.6-litre FWD with 17-in. tire (lowest available): 147mm	
Aero	 	
  Cd	0.27	
Fuel Tank Capacity	FWD and AWD: 59.8 litres (13.1 gal.)	
Towing Capabilities, NAFTA kg (lb.)	No trailer tow recommended	
Curb Weight, Base Vehicle	1,575 kg (3,473 lb.) 	
GVWR (Base vehicle)	2,092 kg (4,612 lb.) 	
		
ACCOMMODATIONS 
mm (in.) unless otherwise noted		
Seating Capacity - F/R	2/3	
Total Interior Passenger Volume	2,871 litres (101.4 cu.ft.)	
Front		
Headroom	983 (38.7) 	
Legroom	1,071 (42.2) 	
Shoulder Room	1,485 (58.5) 	
Hip Room	1,384 (54.5) 	
Seat Travel 	210 (8.3) 	
Front Compartment Volume	1,566 litres (55.3 cu.ft.)	
		
Rear		
Headroom 	950 (37.4) 	
Legroom	956 (37.6) 	
Shoulder Room 	1,441 (56.7) 	
Hip Room	1,338 (52.7) 	
Knee Clearance	71.3 (2.8) 	
Rear Compartment Volume Index,	1,305 litres (46.1 cu. ft.)	
Cargo		
Trunk Lift-over Height	726 (28.6 cu. ft)	
Trunk Volume 	453 litres (16 cu. ft.) 	
Interior Volume	3,324 litres (117.4 cu. ft.)	
Passenger Volume	2,871 litres (101.4 cu. ft.)	
		
WHEELS (in.)		
Availability	200 LX 	
Type and Material	Steel with cover 	
Size 	17 in. x 7.0 	
		
Availability	200 Limited 	
Type and Material	Cast Aluminum, Painted Tech Silver
Cast Aluminum, Painted Satin Silver	
Size	17 in. x 7.5 
18 in. x 8.0 	
		
Availability	200S	
Type and Material	Cast Aluminum, Painted Satin Carbon
Cast Aluminum, Painted Hyper Black	
Size	18 in. x 8.0 
19 in. x 8.0 	
		
Availability	200C 	
Type and Material	Cast Aluminum, Painted Satin Silver
Cast Aluminum, Polished Satin Clear
Cast Aluminum, Polished face, painted pockets	
Size	17 in. x 7.5 
18 in. x 8.0 
19 in. x 8.0 	
TIRES		
Availability	200 LX	
Size and Type (Revs per km)	Bridgestone 215/55R17 (489)
Nexen 215/55R17 (493)
Goodyear 215/55R17 (491)	
		
Availability	200 Limited	
Size and Type (Revs per km)	Bridgestone 215/55R17 (489)
Nexen 215/55R17 (493)
Goodyear 215/55R17 (491)
Nexen 235/45R18 (492)	
		
Availability	200S	
Size and Type (Revs per km)	Bridgestone 235/45R18 (495)
Nexen 235/40R19 (490)	
		
Availability	200C	
Size and Type (Revs per km)	Bridgestone 215/55R17 (489)
Goodyear 215/55R17 (491)
Bridgestone 235/45R18 (495)
Nexen 235/40R19 (490)