2016 Chrysler Town & Country
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

General Information		
Vehicle Type	Multipurpose vehicle 	
Assembly Plant	Windsor, Ontario	
EnerGuide Vehicle Class	Multipurpose vehicle	
		
BODY/CHASSIS		
Layout	Transverse front engine, front-wheel drive	
Construction	Unitized steel with hinged front doors; sliding left and right side doors — power standard; rear liftgate with gas props — power standard	
		
Engine:  3.6-litre PENTASTAR™, gasoline, DOHC, 24-VALVE, VARIABLE VALVE TIMING (VVT) V6	
Availability	Standard	
Type and Description	60-degree bank angle, liquid-cooled, with three-plenum intake manifold, electronically-controlled manifold tuning valve and short-runner valves	
Displacement	3,605 cu. cm (220 cu. in.)	
Bore x Stroke	96 x 83 (3.78 x 3.27)	
Valve System	DOHC, 24 valves, hydraulic, roller finger followers	
Fuel Injection	Sequential, multiport, electronic	
Construction	High-pressure die-cast A380 aluminum block with iron liners and semi-permanent mould A319 aluminum heads	
Compression Ratio	10.2:1	
Power 	283 hp @ 6,400 rpm	
Torque 	260 lb.-ft. @ 4,400 rpm	
Max. Engine Speed	6,800 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2 — acceptable	
Oil Capacity	5.7 litres (6 qt.) with dry filter	
Coolant Capacity	9.75 litres (10.3 qt.)	
Emission Controls 	Dual catalytic converter, four heated oxygen sensors, electronic EGR, and internal engine features	
2015 EnerGuide Fuel Economy L/100km (mpg) (city/hwy)	14.1 (20) / 9.5 (30)	
Engine Assembly Plant	Trenton, Michigan (U.S.A.)	
Transmission: 62TE, Automatic, six-speed overdrive	
Availability	Standard	
Description	Six-speed, adaptive electronic control, electronically-modulated torque converter clutch	
Gear Ratios		
1st	3.90	
2nd	2.69	
3rd	2.16	
4th	Upshift – 1.37 WOT kickdown – 1.49	
5th 	0.95	
6th 	0.65	
Reverse	3.04	
Transfer Ratio	0.95	
Final Drive Ratio	3.16	
Overall Top Gear	2.068	
		
Electrical System		
Alternator	160A	
Battery	730 CCA, maintenance-free	
		
Suspension		
Front	Independent MacPherson strut, coil over gas-charged shock absorbers, stabilizer bar with isolated suspension cradle	
Rear	Twist-beam axle with coil springs, track bar, gas-charged shock absorbers; self-levelling shock absorbers optional	
		
STEERING		
Type	Power rack and pinion	
Overall Ratio	14.3:1	
Turning Diameter (curb-to-curb)	11.92 m (39.1 ft.)	
Steering Turns (lock-to-lock)	2.90	
P/S pump	Hydraulic	
		
BRAKES mm (in.) unless otherwise noted		
Type	All — Power assist, 230 x 230 (9 x 9) tandem-diaphragm vacuum, anti-lock braking system (ABS)	
Availability	Standard on all models	
Front		
Rotor size and type	330 x 28 (13.0 x 1.1) vented rotor	
Caliper size and type	51 mm twin-piston caliper	
Swept area	475 sq. cm (73.6 sq. in.)	
Rear		
Rotor size and type	328 x 12 (12.9 x 0.47) solid rotor	
Caliper size and type	45 mm single-piston IPB caliper	
Swept area	429 sq. cm (66.5 sq. in.)	
		
Dimensions and Capacities mm (in.) unless otherwise noted		
Wheelbase	3,078 (121.2)	
Overhang—Front	961 (37.8)	
Overhang—Rear	1,112 (43.8)	
Track—Front	1,666 (65.6)	
Track—Rear	1,647 (64.8)	
Overall Length	5,151 (202.8)	
Overall Width	1,998 (78.7)	
Overall Width with Mirrors	2,247 (88.5)	
Overall Height 	1,751 (68.9)	
Liftover Height 	609 (24.0)	
Cargo Width at Wheelhouse 	1,239 (48.8)	
Maximum Cargo Height 	1,172 (46.2)	
Approach Angle (degrees)	14.7	
Ramp Breakover Angle (degrees)	14.6	
Departure Angle (degrees)	19.2	
Minimum Running Ground Clearance 
(curb load)	148 (5.8)	
Frontal Area	32.3	
Drag Coefficient (Cd)	.316	
Aero CdA	10.2	
Fuel Tank Capacity, litres (imp. gal.)	76 (16.7)	
Gross Vehicle Weight Rating (GVWR), 
kg (lb.)	2,744 (6,050)	
		
Maximum Towing Capacity	1,588 kg (3,500 lb.) — with Trailer-tow Prep Package	
Curb Weight 	2,115 kg (4,652 lb.) — Automatic transaxle	
Weight Distribution (per cent front/rear) 	56/44	
		
Accommodations 
mm (in.) unless otherwise noted		
Seating Capacity (front/second/third rows)	2/2/3 	
Total Interior Passenger Volume	4,630 litres (163.5 cu. ft.) / 4,420 litres (156.1 cu. ft.)	
Front		
Head Room	1,012 (39.8)	
Head Room with Sunroof 	946 (37.2)	
Leg Room	1,034 (40.7)	
Shoulder Room	1,619 (63.7)	
Hip Room	1,485 (58.4) 	
Seat Travel	220 (8.7)	
Recliner Angle Range (degrees)	Manual recline: 88
Power recline: 59	
Front Passenger Volume	1,654 litres (58.4 cu.ft.)	
Intermediate 		
Head Room	999 (39.3)	
Legroom	926 (36.5)	
Knee Clearance	81 (3.2)	
Shoulder Room	1,628 (64.1)	
Hip Room	1,651 (65.0)	
Intermediate Passenger Volume	1,529 litres (54.0 cu.ft.)	
Rear 		
Head Room	963 (37.9)	
Legroom	830 (32.7)	
Knee Clearance	153 (6.0)	
Shoulder Room	1,575 (62.0)	
Hip Room	1,238 (48.7) 	
Rear Passenger Volume 	1,447 litres (51.1 cu.ft.)	
Cargo Volume 		
Maximum Cargo Volume	4,072 litres (143.8 cu.ft.)	
Behind Second-row Seats	2,359 litres (83.3 cu.ft.)	
Aft of Third-row Seat	934.5 litres (33.0 cu.ft.)	
Total Passenger plus Cargo Volume	5,544.4 litres (195.8 cu.ft.)	
		
Wheels (in.)		
Availability	Standard on Town & Country Touring	
Type and Material	Cast aluminum 	
Size	17 x 6.5	
		
Availability	Standard on Town & Country S	
Type and Material	Hyper Black aluminum	
Size	17 x 6.5	
		
Availability	Standard on Town & Country Touring-L	
Type and Material	Tech Silver aluminum	
Size	17 x 6.5	
		
Availability	Standard on Town & Country Premium	
Type and Material	Fully polished aluminum	
Size	17 x 6.5	
		
Availability	Standard on Town & Country Limited 	
Type and Material	Satin Silver aluminum 	
Size	17 x 6.5	
		
Tires		
Availability	Standard on Town & Country Touring, S, Touring-L, Premium and Platinum	
Size and Type	P225/65R17 BSW, All-season Touring	
Model	Kumho and Yokohama 	
		
Parking Brake Type	Integral parking brake	
Four-wheel Anti-lock Brake System (ABS)	Standard	
Electronic Stability Control (ESC)	Standard	
All-speed Traction Control	Standard	
Brake Assist	Standard