2016 Dodge Dart
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

General Information		
Body Style	Four-door sedan	
Assembly Plant	Belvidere, Illinois (U.S.A.)	
Vehicle Class	Mid-size	
		
Body AND Chassis		
Layout	Transverse front engine, front-wheel drive (FWD)	
Construction	High-strength steel unibody	
		
ENGINE: 2.0-LITRE TIGERSHARK™ I-4 	
Availability	Standard — SE	
Type and Description 	Inline four-cylinder, dual overhead cam variable-valve timing (VVT), 
16 valves with multiport fuel injection	
Displacement	1,995 cu. cm (122 cu. in.)	
Bore x Stroke	88 X 82 (3.46 x 3.23)	
Valve System	DOHC, VVT, four valves per cylinder (16 total)	
Fuel Injection	Sequential, multiport, electronic, returnless 	
Construction	Aluminum block and cylinder head	
Compression Ratio	10.2:1	
Power 	160 hp @ 6,400 rpm	
Torque 	148 lb.-ft. @ 4,600 rpm	
Max. Engine Speed	6,750 rpm	
Fuel Requirement	Unleaded regular, 87 Octane, E85 flex fuel 	
Oil Capacity	4.7-litres (5.0 qt.)	
Coolant Capacity	6.7-litres (7.1 qt.)  	
Emission Controls 	Single catalyst, dual-heated oxygen sensors (1 upstream, one mid catalyst) (	
2015 EnerGuide Fuel Economy L/100 km (mpg) city/hwy	9.4 (30) / 6.5 (43) — manual 
9.9 (29) / 7.0 (40) — automatic 	
Engine Assembly Plant 	Dundee, Michigan (U.S.A.)	
	
ENGINE: 1.4-LITRE TURBOCHARGED MULTIAIR I-4	
Availability	Standard – Aero 	
Type and Description 	Inline turbocharged four-cylinder, liquid-cooled	
Displacement	1,368 cu. cm (84 cu. in.)	
Bore x Stroke	72 X 84 (2.83 x 3.31)	
Valve System	SOHC with MultiAir, four valves per cylinder (16 total)	
Fuel Injection	Sequential, multiport, electronic, returnless 	
Construction	Iron block, aluminum cylinder head	
Compression Ratio	9.8:1	
Power 	160 hp @ 5,500 rpm	
Torque 	184 lb.-ft. @ 2,500-4,000 rpm	
Max. Engine Speed	6,500 rpm	
Fuel Requirement	Unleaded regular, 87 octane accepted;
Unleaded premium, 93 octane preferred	
Oil Capacity	3.8 litres (4.0 qt.)	
Coolant Capacity	5.7 litres (6.0 qt.)  	
Emission Controls	Single catalytic converter, heated wide-band lambda sensor upstream and heated oxygen sensor downstream	
2015 EnerGuide Fuel Economy L/100 km (mpg) city/hwy	8.5 (33) / 5.8 (49) — manual 
8.4 (34) / 5.9 (48) — automatic, dual dry clutch transmission (DDCT)	
Engine Assembly Plant 	Dundee, Michigan (U.S.A.)	
	
ENGINE: 2.4-LITRE MULTIAIR 2 TIGERSHARK I-4	
Availability	Standard — SXT, GTand Limited	
Type and Description	Inline four-cylinder, 16-valve MultiAir with multiport fuel injection	
Displacement	2,360 cu. cm (144 cu. in.)	
Bore x Stroke	88 X 97 (3.46 x 3.82)	
Valve System	SOHC, four valves per cylinder (16 total)	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum block, aluminum cylinder head	
Compression Ratio	10:1	
Power  	184 hp  @ 6,250 rpm	
Torque  	174lb.-ft. @ 4,800 rpm	
Max. Engine Speed	6,500 rpm	
Fuel Requirement	Unleaded regular, 87 octane	
Oil Capacity	4.7 litres (5.0 qt.)  	
Coolant Capacity	6.7 litres (7.1 qt.)	
Emission Controls	Single catalytic converter, heated wide band lambda sensor upstream 
and mid-catalyst heated oxygen sensor	
Estimated EnerGuide Fuel Economy L/100km (mpg) city/hwy	10.5 (27) / 6.7 (42) SXT/Limited models — manual	
	10.2 (28) / 7.0 (40) GT model — manual 	
	10.1 (28) / 6.8 (42) SXT/Limited models — automatic	
	10.6 (27) / 7.5 (38) GT model — automatic	
Engine Assembly Plant 	Dundee, Michigan (U.S.A.)	
	
TRANSAXLE: c635 SIx-speed manual	
Availability	Standard with Dart SE, SXT, Aero, and GT	
Description	Six-speed, fully synchronized, FWD, manual transmission	
Gear Ratios		
1st	3.90	
2nd	2.11	
3rd	1.36	
4th	0.97	
5th	0.75	
6th	0.62	
Reverse	4.0	
Final-drive Ratio	4.11 with 1.4-litre engine	
Overall Top-gear	2.54 with 1.4-litre engine	
	
TRANSAXLE: 6F24 six-Speed Automatic Overdrive	
Availability	Standard with Dart Limited, Available with Dart SE, SXT, and GT	
Description	Six-speed, FWD, electronically controlled, automatic overdrive	
Gear Ratios		
1st	4.64	
2nd	2.83	
3rd	1.81	
4th	1.39	
5th	1.00	
6th	0.77	
Reverse	3.29	
Final-drive Ratio	3.20 with 2.0-litre engine and 2.4-litre engine (3.51 GT Model 2.4-litre engine)	
Overall Top-gear	2.46 with 2.0-litre engine and 2.4-litre engine (2.70 GT Model 2.4-litre engine)	
TRANSAXLE: C635 six-Speed Dual Dry Clutch Transmission (DDCT)	
Availability	Optional with Dart Aero	
Description	Six-speed, FWD, electronically controlled, automatic overdrive with dual dry clutch technology	
Gear Ratios		
1st	4.15	
2nd	2.26	
3rd	1.44	
4th	0.97	
5th	0.75	
6th	0.62	
Reverse	4.0	
Final-drive Ratio	3.83 with 1.4-litre engine – Aero	
Overall Top-gear	2.37 with 1.4-litre engine – Aero	
		
Suspension		
Front	Independent MacPherson strut, coil spring over gas-charged shock absorbers, stabilizer bar 	
Rear	Multi-link independent with coil springs, gas-charged shock absorbers 
and Rallye, Limited and GT models add link-type stabilizer bar 	
	
Steering		
Type	Electric, dual pinion	
Overall Ratio	15:1 (12.76:1 GT Model)	
Turning Diameter (curb-to-curb)	11.1 m (36.5 ft.) (17-in. wheels)
11.5 m (37.7 ft.) (18-in. wheels)	
Steering Turns (lock-to-lock)	3.3 (17-in. wheels)
3.0 (18-in. wheels)	
		
Brakes	
Availability	Standard	
Power-assist Type	Single 11-in. diaphragm vacuum	
Front		
Size and Type (mm)	305 x 28 mm vented rotors with 60 mm single piston floating caliper	
Swept Area (Total Front)	820.08 sq. cm (127.11 sq. in.) 	

Rear		
Size and Type (mm)	264 x 10 mm solid rotors with 38 mm single piston floating caliper	
Swept Area (Total Rear)	523.07 sq. cm (81.08 sq. in.) 	
Parking Brake Type	Rear caliper integrated park brake system	
Anti-lock Brake System (ABS)	Standard	
Electronic Stability Control (ESC)	Standard	
Traction Control	Standard	
Brake Assist	Standard	
		
Dimensions and Capacities 
mm (in.) unless otherwise noted		
Wheelbase	2,703 (106.40)  	
Track, Front	1,568 (61.7) 	
Track, Rear	1,565 (61.6) 	
Overall Length	4,672 (183.9) 	
Overall Width	1,830 (72.0) 	
Overall Height	1,465 (57.7) 	
Aero Cd	0.285	
Fuel Tank Capacity		
Aero	50 litres (11 imp. gal.)	
SE, SXT, Limited, Rallye	54 litres (11.9 imp. gal.)	
GT	60 litres (13.2 imp. gal.)	
Towing Capabilities		
2.0-litre automatic transmission	454 kg (1,000 lb.) 	
2.4-litre automatic transmission	454 kg (1,000 lb.) 	
Curb Weight, (with fuel) kg (lb.) 		
2.0-litre gasoline engine	1,416 kg (3,122 lb.) (manual)
1,439 kg (3,172 lb.) (automatic)	
1.4-litre gasoline engine	1,398 kg (3,081 lb.) (manual)
1,423 kg (3,137 lb.) (automatic, DDCT)	
2.4-litre gasoline engine	1,436 kg (3,165 lb.) (manual)
1,458 kg (3,215 lb.) (automatic)	

accommodations 
mm (in.) unless otherwise noted		
Seating Capacity — front/rear	2/3 	
Total Interior Passenger Volume	2,752 litres (97.2 cu.ft.)	
Head Room without Sunroof	980 (38.6)	
Head Room with Sunroof	950 (37.4)	
Leg Room	1,071 (42.2)	
Shoulder Room	1,477 (58.2)	
Hip Room	1,392 (54.8)	
Seat Travel	260 (10.32)	
Front Compartment Volume	1,552 litres (54.8 cu.ft.)	
Headroom without Sunroof 	940 (37.0)	
Legroom	894 (35.2)	
Shoulder Room	1,425 (56.1)	
Hip Room	1,336 (52.6)	
Knee Clearance	30.5 (1.2)	
Rear Compartment Volume	1,201 litres (42.4 cu.ft.)	
Cargo		
Trunk Lift-over Height	754 (29.7)	
Luggage Compartment Volume	371 litres (13.1 cu.ft.)	
		
Wheels (in.)		
Availability	Standard — SE	
Type and Material	Steel wheel with Tech Silver painted wheel cover	
Size 	16 x 7 	
		
Availability	Standard — Aero	
Type and Material	Cast-aluminum, Tech Silver painted	
Size 	16 x 7	
		
Availability	Standard — SXT	
Type and Material	Cast-aluminum, Tech Silver painted	
Size 	16 x 7	
		
Availability	Standard — Limited	
Type and Material	Cast-aluminum, Satin Silver painted	
Size 	17 x 7.5	
Availability	Available on SXT with Rallye Appearance Group	
Type and Material	Cast-aluminum, Granite Crystal	
Size 	17 x 7.5	
	
Availability 	Available on Limited	
Type and Material	Cast-aluminum, polished	
Size 	17 x 7.5	
	
Availability	Standard — GT	
Type and Material	Cast-aluminum, Hyper Black, painted	
Size 	18 x 7.5	
		
Availability	Optional — on GT with Blacktop Package	
Type and Material	Cast-Aluminum, 10-spoke Gloss Black painted	
Size 	18 x 7.5	
		
Tires		
Availability	Standard — SE, Aero, SXT	
Size and Type	205/55R16, all season	
Model	Kumho Solus KH25	
Revs per km (mile)	519 (836)	
		
Availability 	Optional — SE	
Size and Type	205/55R16, all season	
Model	Continental Conti ProContact 	
Revs per km (mile)	502 (808)	
		
Availability	Standard — Limited; Optional on Rallye	
Size and Type	225/45R17, all season	
Model	 Yokohama Avid S34	
Revs per km (mile)	516 (831)	

Availability	Optional — Rallye, Limited	
Size and Type	225/45R17, all season	
Model	Kumho Solus KH25	
Revs per km (mile)	515 (830)	
		
Availability	Standard — GT; Available on SXT with Blacktop Package	
Size and Type	225/40R18, all season	
Model	Yokohama 	
Revs per km (mile)	500 (804)