2016 Dodge Durango
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

General Information		
Vehicle Type	Four-door sport-utility vehicle	
Assembly Plant	Detroit, Michigan (U.S.A.)	
EnerGuide Vehicle Class	Multipurpose vehicle 	
		
BODY/CHASSIS		
Layout	Longitudinal front engine, rear drive (transfer case with full-time 
all-wheel drive available)	
Construction	Steel unibody	
	
Engine: 3.6-Litre pentastar™ v6	
Availability	Standard on SXT, Limited and Citadel (RWD and AWD, not available on R/T)	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	3,604 cu. cm (220 cu. in.)	
Bore x Stroke	96.0 x 83.0 (3.78 x 3.27)	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads	
Compression Ratio	10.2:1	
Power (est.) 	TBD 	
Torque (est.) 	TBD	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R + M)/2 	
Oil Capacity	5.7 litres (6.0 qt.)	
Coolant Capacity	9.9 litres (10.4 qt.) without trailer tow 
10.4 litres (11 qt.) with trailer tow	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors 
and internal engine features	
2015 EnerGuide Fuel Economy L/100 km (mpg) city/hwy	13.9 (20) / 9.8 (29) 	
Engine Assembly Plant	Trenton, Michigan (U.S.A.)	
ENGINE: 5.7-LITRE HEMI® V8		
Availability	Standard on R/T and optional on Citadel 	
Type and Description	90-degree V-type, liquid-cooled	
Displacement	5,654 cu. cm (345 cu. in.)	
Bore x Stroke	99.5 x 90.9 (3.92 x 3.58)	
Valve System	Variable-valve timing (VVT), pushrod-operated overhead valves, 16 valves, eight deactivating and eight conventional hydraulic lifters, all with roller followers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, 
aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.5:1	
Power (est.) 	360 hp at 5,150 rpm	
Torque (est.) 	390 lb.-ft. at 4,250 rpm	
Max. Engine Speed	5,800 rpm (electronically limited)	
Fuel Requirement	Unleaded mid-grade, 89 octane (R+M)/2—recommended;
unleaded regular, 87 octane (R+M)/2—acceptable	
Oil Capacity	6.6 litres (7 qt.)	
Coolant Capacity	14.6 litres (15.4 qt.) without trailer tow 
15.2 litres (16 qt.) with trailer tow	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad heated oxygen 
sensors and internal engine features	
2015 EnerGuide Fuel Economy 
L/100km (mpg) city/hwy	17.3 (16) / 11.5 (25) 	
Engine Assembly Plant	Saltillo (Mexico)	
	
TRANSMISSION: torqueflite EIGHT-SPEED automatic	
Availability	Standard on all models	
Description	Driver-interactive manual control via steering wheel paddle shifters and electronically modulated torque converter clutch	
Gear Ratios		
1st 	4.714	
2nd 	3.143	
3rd  	2.106	
4th 	1.667	
5th 	1.285	
6th	1.000	
7th	0.839	
8th	0.667	
Reverse 	3.295	
TRANSFER CASE: MP 3010 		
Availability	Standard with V6 engine 	
Type	Single-speed	
Operating Mode	Full-time AWD	
Low Range Ratio	None	
Torque Split, Front/Rear	50/50	
		
TRANSFER CASE: MP 3023		
Availability	Standard with V8 engine and AWD	
Type	Two-speed, electronically shifted	
Operating Modes	AWD Low (Lock), Neutral; full-time active AWD	
Low Range Ratio	2.72	
Torque Split, Front/Rear	Variable	
		
Axles		
Front		
Differential Type	Conventional	
Availability	Standard on AWD models 	
Ring Gear Diameter	195 (7.7)	
Axle Ratios	3.45:1 (V6)  
3.09:1 (V8)	
Rear		
Differential Type	Conventional	
Availability	Standard on all engines	
Ring Gear Diameter	195 (7.7) (V6) 
230 (9.1) (V8)	
Axle Ratios	3.45:1 (V6)
3.09:1 (V8)	
		
Electrical System		
Alternator	160-amp; 180-amp or 220-amp depending on option content	
Battery	Maintenance-free 
H6 650 CCA + Auxiliary 200 CCA on Electronic Stop/Start (ESS) (V6)
H7 700 CCA (V8)	
		
Suspension		
Front	Short- and long-arm independent (SLA), coil springs, gas-charged, twin-tube coil-over shock absorbers, steel upper- and aluminum lower-control arms (“A” arms), aluminum knuckle, stabilizer bar	
Rear	Multi-link rear suspension, coil spring, twin tube shocks (including load leveling for towing), aluminum lower control arm, independent upper links (tension and camber) plus a separate toe link	
		
STEERING		
Type	Rack and pinion with electric power assist	
Steering Ratio	16.7 (V6 and V8)	
Lock-to-Lock Steering Wheel Rotations	3.2 (V6 and V8)	
		
BRAKES		
Type	Power-assisted, anti-lock braking system (ABS)	
Availability		
Front		
Rotor size and type	330 x 32 (13.0 x 1.26) vented disc (V6)
350 x 32 (13.8 x 1.26) vented disc (V8)	
Caliper size and type	1.89 (48) two-piston pin-slider caliper	
Swept area	1,969 sq. cm (305 sq. in.) (V6) 
2,088 sq. cm (324 sq. in.) (V8)	
Rear		
Rotor size and type	330 x 14 (13.0 x 0.55) solid disc (V6) 
330 x 22 (13.0 x 0.87) vented disc (V8)	
Caliper size and type	48 (1.89) single-piston floating caliper	
Swept area	1,658 sq. cm (257 sq. in.)	
		
Dimensions and Capacities 
mm (in.) unless otherwise noted		
Wheelbase	3,042 (119.8)	
Track, Front	1,623 (63.9)	
Track, Rear	1,627 (64.1)	
Overall Length	5,110 (201.2)	
Overall Width (Width at Mirrors)	2,172 (85.5)	
Body Width	1,924 (75.8)	
Overall Height (at Roof Rail / at Antenna)	1,801 (70.9) / 1,847 (72.7), R/T - 1,827 (71.9)  	
Load Floor Height	817 (32.2) R/T – 798 (31.4)	
Sill Step Height	521.5 (20.5) / 522.6 (20.6)	
Ground Clearance (with P265/60R18 Tire and 3.6 litre engine)	207 (8.1)	
Chassis (Fuel Tank) 	254 (10.0)	
Front Axle	243 (9.6)	
Rear Axle	256 (10.1)	
Approach Angle (degrees)	16.3 	
Ramp Breakover Angle (degrees)	18.1	
Departure Angle (degrees)	21.5 	
Frontal Area 	2.88 sq.m (31.0 sq. ft.)	
Drag Coefficient 	0.35	
Fuel Tank Capacity	93.1 litres (24.6 gal.)	
		
Accommodations 
mm (in.) unless otherwise noted		
Seating Capacity (front/second/third rows)	2/3/2, 2/2/2 with optional second-row captain’s chairs	
Front		
Head Room	1,013 (39.9)	
Legroom	1,025 (40.3)	
Shoulder Room 	1,486 (58.5)	
Hip Room	1,449 (57.0)	
Seat Travel	280 (11.0) driver, 230 (9.0) passenger 	
Front Volume Index	1,540 litres (54.4 cu. ft.)	
Second Row		
Head Room	1,011 (39.8) 	
Legroom	981 (38.6) 	
Shoulder Room	1,281 (50.4) 	
Hip Room 	1,088 (42.8) 	
Volume	1,269 litres (44.8 cu. ft.) 	
Third Row 		
Head Room	960 (37.8) 	
Legroom	800 (31.5) 	
Shoulder Room	1,281 (50.4) 	
Hip Room 	1,088 (42.8) 	
Volume	983 litres (34.7 cu. ft.) 	
		
Cargo Volume		
Behind Third Row	487 litres (17.2 cu. ft.) 	
Behind Second Row	1,351 litres (47.7 cu. ft.) 	
Behind Front-row Seats with 
Rear Seats Folded	2,393 litres (84.5 cu. ft.)	
		
WEIGHTS (Estimates)		
	MODEL	ENGINE	GVWR kg (lb.)	CURB WEIGHT kg (lb.)	PAYLOAD kg (lb.)	
AWD	SXT 	3.6-litre	2,948 (6,500) 	2,229 (4,913) 	640 (1,410)  	
	Limited	3.6-litre
5.7-litre	2,948 (6,500) 
3,221 (7,100)	2,262 (4,987) 
2,418 (5,330)	645 (1,420) 
650 (1,430)	
	Citadel	3.6-litre
5.7-litre	3,221 (7,100) 
3,221 (7,100) 	2,312 (5,097) 
2,448 (5,397) 	615 (1,360) 
620 (1,370) 	
	R/T	5.7-litre	3,221 (7,100) 	2,418 (5,331) 	605 (1,340) 	
		
Wheels (in.)		
Availability	Standard on SXT and Limited 	
Type and Material	Painted machine cast-aluminum, 10-spoke 	
Size 	18 x 8	
		
Availability	Optional on Limited and Blacktop Package	
Type and Material	Polished machined cast-aluminum, 15-spoke
(Gloss Black on Blacktop Package)	
Size 	20 x 8	
		
Availability	Standard on R/T and Brass Monkey Appearance Package	
Type and Material	Painted machined cast-aluminum, twin five-spoke 
(Bronze on Brass Monkey Appearance Package)	
Size 	20 x 8	
		
Availability	Standard on Citadel	
Type and Material	Polished machined cast-aluminum, 10-spoke 	
Size 	20 x 8	
		
Tires		
Availability 	Standard on SXT and Limited	
Size and Type	P265/60R18	
Mfr. and Model	Kuhmo Crugen Black Sidewall All-season	
		
Availability 	Standard on R/T and Citadel, optional on SXT and Limited	
Size and Type	P265/50R20	
Mfr. and Model	Pirelli Scorpion Verde Black Sidewall All-season	
		
Availability 	Available on R/T and Citadel, optional on SXT and Limited	
Size and Type	P265/50R20	
Mfr. and Model	Bridgestone Ecopia H/L 422 Plus Black Sidewall All-season	
		
Availability 	Optional on R/T	
Size and Type	P265/50R20	
Mfr. and Model	Pirelli Scorpion Verde Black Sidewall All-season Performance	
		
Parking Brake Type	Rear, mechanical, drum-in-hat	
Power Assist	Single-rate, tandem diaphragm vacuum	
Four–wheel Anti-lock Brakes	Standard	
Electronic stability control	Standard	
All-speed traction control	Standard	
Brake Assist	Standard	
		
TRAILER TOWING(a)		
	Engine	Axle Ratio	Maximum Trailer Weight(b)  kg (lb.)	
AWD 	3.6-litre V6
5.7-litre V8	3.45 
3.09	2,812 (6,200)
3,265 (7,200)