2016 Dodge Journey
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

General Information		
Body Style	Four-door; five- or seven-passenger	
Assembly Plant	Toluca (Mexico)	
EnerGuide Vehicle Class	Sport-utility vehicle	
	
BODY/CHASSIS	
Layout	Transverse front engine, front-wheel drive or all-wheel drive	
Construction	Steel unibody	
		
Engine:  2.4-litre dohc 16-valve, vvt, smpi i-4	
Availability	CVP, SE Plus, SXT	
Type and Description	Four cylinders in-line, tuned intake manifold with dual counter-rotating balance shafts and dual variable-valve timing	
Displacement	2,360 cu. cm (144 cu. in.)	
Bore x Stroke	88 x 97 (3.46 x 3.82)	
Compression Ratio	10.5:1	
Power 	173 hp @ 6,000 rpm (71 hp/litre)	
Torque 	166 lb.-ft. @ 4,000 rpm	
Maximum Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity	4.26 litres (4.5 qt.) SAE 5W-20	
Coolant Capacity	7.5 litres (7.9 qt.) — single-zone climate control 	
Emission Controls	Single catalytic converter, dual heated oxygen sensors 
and internal engine features	
2015 EnerGuide Fuel Economy L/100km (mpg) city/hwy	12.7 (22) / 9.1 (31)	
Engine Assembly Plant	Dundee, Michigan (U.S.A.)	
	
Engine:  3.6-litre dohc 24-valve, vARIABLE vALVE tIMING (VVT) DOHC V6	
Availability	SXT, Crossroad, Limited, R/T and R/T Rallye	
Type and Description	60-degree bank angle, liquid-cooled, three-plenum intake manifold with electronically controlled manifold tuning valve and short-runner valves 	
Displacement	3,605 cu. cm (220 cu. in.)  	
Bore x Stroke	96 x 81 (3.78 x 3.19)	
Compression Ratio	10.2:1	
Valve System	DOHC, 24 valves, hydraulic, center-pivot roller rocker arms 	
Fuel Injection	  Sequential, multiport, electronic 	
Power 	283 hp @ 6,350 rpm (67.1 hp/litre)	
Torque 	260 lb.-ft. @ 4,400 rpm 	
Maximum Engine Speed	6,800 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2 
Ethanol E85	
Oil Capacity	5.2-litres (5.5 qt.) SAE 10W-30 MAF 	
Coolant Capacity	10-litres (10.6 qt.) — single- or dual-zone climate control 
11-litres  (11.6 qt.) — tri-zone climate control 	
Emission Controls	Three-way catalytic converter, electronic EGR, 
and internal engine features	
2015 EnerGuide Fuel Economy L/100km (mpg) city/hwy	FWD: 14.2 (20) / 9.4 (30)
AWD: 14.5 (19) / 9.9 (29)	
Engine Assembly Plant	Trenton, Michigan (U.S.A.)	
	
Transmission: 40TES Automatic four-speed overdrive	
Availability	CVP, SE Plus and SXT with 2.4-litre engine	
Description	Four-speed overdrive, adaptive electronic control, 
electronically modulated converter clutch	
Gear Ratios		
1st	2.842	
2nd	1.57	
3rd	1.0	
4th	0.69	
Reverse	2.21	
Final-drive Ratio	4.28	
Overall Top-gear	2.95	
	
Transmission: 62te/62tea Automatic six-speed overdrive	
Availability	SXT, Crossroad, Limited, R/T and R/T Rallye with 3.6-litre V6	
Description	Six-speed, adaptive electronic control and electronically 
modulated torque converter clutch	
Gear Ratios		
1st	4.127	
2nd	2.842	
3rd	2.283	
4th	1.452 — Upshift 
1.570 — WOT kickdown	
5th	1.00	
6th	0.690	
Reverse	3.214	
Transfer Ratio	0.95	
Final-drive Ratio	3.16	
Overall Top-gear	2.06	
	
Drivetrain 	
Front-wheel Drive		
Availability	CVP, SE Plus, SXT, Crossroad and Limited	
All-wheel Drive		
Availability	Crossroad, R/T and R/T Rallye	
Type	Electronically controlled coupling (ECC) with variable torque output	
Rear Differential	Open	
	
Electrical System	
Alternator	160-amp — Standard on all Journey models	
Battery	525-amp maintenance-free	
	
Suspension	
Front	Independent MacPherson strut, coil spring over gas-charged shock absorbers, stabilizer bar with isolated suspension cradle	
Rear	Multi-link independent with coil springs, link-type stabilizer bar, 
gas-charged shock absorbers and isolated rear suspension cradle	
	
STEERING	
Type	Power rack and pinion	
Overall Ratio	16.45	
Turning Diameter (curb-to-curb) 	11.7 m (38.5 ft.) — 17-in. wheels
11.9 m (39.0 ft.) — 19-in. wheels 	
Steering Turns (lock-to-lock)	2.92	
P/S pump	Hydraulic	
	
BRAKES	
Front		
Rotor size and type	330 x 28 (13.0 x 1.1) vented rotor	
Caliper size and type	51.0 (2.0) two-piston floating caliper	
Swept area 	475 sq. cm (73.6 sq. in.)	
Rear		
Rotor size and type	328 x 12 (12.9 x 0.47) solid rotor	
Caliper size and type	45.0 (1.8) single-piston floating caliper	
Swept area 	429 sq. cm (66.5 sq. in.)	
	
Dimensions and Capacities mm (in.) unless otherwise noted	
Wheelbase	2,890 (113.8)	
Overhang — Front	989 (38.9)	
Overhang — Rear	1,009 (39.7)	
Track — Front	1,571 (61.8)	
Track — Rear	1,582 (62.3)	
Overall Length	4,888 (192.4)	
Overall Width	1,835 (72.2)	
Overall Width with Mirrors 	2,127 (83.7)	
Overall Height	1,693 (66.6)	
Vehicle Height including Roof Rack Assembly	1,765 (69.5)	
Drag Coefficient (Cd)	0.368	
Fuel Tank Capacity, litres (imp. gal)	2.4-litre and 3.6-litre FWD — 77.6 (17.1)
3.6-litre AWD —79.9 (17.6)	
Gross Vehicle Weight Rating (GVWR)		
Five-passenger Vehicle, FWD 2.4-litre	2,270 kg (5,005 lb.)	
Seven-passenger Vehicle, FWD 2.4-litre	2,404 kg (5,300 lb.)	
Five-passenger Vehicle, FWD 3.6-litre	2,313 kg (5,100 lb.)	
Seven-passenger Vehicle, FWD 3.6-litre	2,472 kg (5,450 lb.)	
Five-passenger Vehicle, AWD 3.6-litre	2,540 kg (5,600 lb.)	
Seven-passenger Vehicle, AWD 3.6-litre	2,540 kg (5,600 lb.)	
Towing Capabilities		
2.4-litre I-4 with Automatic Transaxle	454 kg (1,000 lb.)	
3.6-litre V6 with Automatic Transaxle, 
FWD or AWD	1,134 kg (2,500 lb.)	
Curb Weight, Five-passenger Vehicle, Automatic Transaxle		
2.4-litre I-4 	FWD — 1,732 kg (3,818 lb.)	
3.6-litre V6 	FWD — 1,839 kg (4,054 lb.)
AWD — 1,922 kg (4,238 lb.)	
	
Accommodations 
mm (in.) unless otherwise noted	
Seating Capacity (front/second/third rows)	2/3 standard, 2/3/2 optional	
Volume Index	3,792 litres (133.9 cu.ft.) – seven-passenger 
3,811 litres (134.6 cu.ft.) – five-passenger	
Total Interior Passenger Volume	3,503 litres (123.7 cu.ft.) – seven-passenger 
2,820 litres (99.6 cu.ft.) – five-passenger	
Front row		
Headroom without Sunroof	1,036 (40.8)	
Headroom with Sunroof	995 (39.2)	
Legroom	1,036 (40.8)	
Shoulder Room	1,460 (57.5)	
Hip Room	1,367 (53.8)	
Seat Travel	260 (10.23)	
Front Compartment Volume	1,569 litres (55.39 cu.ft.)	
Second row	
Headroom without Sunroof	1,013 (39.9)	
Headroom with Sunroof	995 (39.2)	
Legroom	917 (36.1)	
Couple, First to Second Row	774 (30.5)	
Shoulder Room	1,444 (56.9)	
Hip Room	1,382 (54.4)	
Rear Seat Volume Index or Third row Volume	1,249 litres (44.1 cu.ft.)	

Third row 	
Headroom	957 (37.7)	
Legroom	596 (23.4)	
Couple, Second to Third Row	765 (30.1)	
Shoulder Room	1,105 (43.5)	
Hip Room	1,016 (40.0)	
Rear Passenger Volume	629 litres (22.2 cu.ft.)	
Cargo Width @ Wheelhouse	1,051 (41.4)	
Trunk Liftover Height	782 (30.8)	
Cargo Volume		
Behind First-Row Seat	1,914 litres (67.6 cu.ft.)	
Behind Second-Row Seat
(5-passenger vehicles)	1,122 litres (39.61 cu.ft.) 	
Behind Second-Row Seat
(7-passenger vehicles)	1,048 litres (37.0 cu.ft.)	
Behind Third-Row Seat	303 litres (10.7 cu.ft.)	
	
Wheels (in.)	
Availability	Available on CVP 	
Type and Material	Steel with wheel covers 	
Size	17 x 6.5	
		
Availability	Standard on CVP and SE Plus	
Type and Material	Machined cast-aluminum, five-spoke	
Size	17 x 6.5	
		
Availability	Standard on SXT	
Type and Material	Machined cast-aluminum, twin five-spoke Tech Silver	
Size	17 x 6.5	
		
Availability	Standard on Limited, R/T and R/T Rallye; optional on SXT	
Type and Material	Machined cast-aluminum, 10-spoke (Standard–Limited and R/T; Optional – SXT), Satin Carbon finish (R/T Rallye) or Gloss Black finish (SXT Blacktop package)	
Size	19 x 7.0	

Availability	Standard Crossroad FWD and AWD	
Type and Material	Machined cast-aluminum, five-spoke Hyper Black finish 	
Size	19 x 7.0	
		
Availability	Available on Limited and R/T	
Type and Material	Chrome-clad cast-aluminum, six-spoke	
Size	19 x 7.0	
		
Availability	Standard on all models 	
Type and Material	Temporary spare steel wheel	
		
Tires	
Availability	Standard on CVP, SE Plus and SXT 	
Size and Type	P225/65R17, All-season Touring	
Model	Kumho Solus KH16	
Revs per km (mile)	471 (725) 	
		
Availability	Standard on Crossroad, Limited, R/T and R/T Rallye	
Size and Type	225/55R19, All-season Touring	
Model	Kumho Solus KH16	
Revs per km (mile)	444 (711) 	
		
Availability	Standard on all Journey models 	
Size and Type	T145/70 R17 temporary spare tire	
Parking Brake Type	Standard on all Journey models	
Power-assist Type	230 x 230 (9 x 9) tandem-diaphragm vacuum	
Four–wheel Anti-lock Brakes	Standard	
Electronic stability control	Standard	
All-speed traction control	Standard	
Brake Assist	Standard