2016 Fiat 500L
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Vehicle Type	B-segment multipurpose vehicle (MPV)	
EnerGuide Vehicle Class	Small Station Wagon	
Assembly Plant	Kragujevac (Serbia)	
	
BODY AND CHASSIS	
Layout	Transverse-mounted front engine, front-wheel drive	
Construction	Unitized steel body 	
	
ENGINE: 1.4-LITRE SOHC 16-VALVE TURBOCHARGED MULTIAIR® INLINE FOUR-CYLINDER	
Availability	Standard — 500L Pop, Sport, Trekking and Lounge models	
Type and Description	Inline four-cylinder, liquid-cooled, turbocharged 	
Displacement	1,368 cu. cm (83.48 cu. in.)	
Bore x Stroke	72.0 x 84.0  (2.83 x 3.31)	
Valve System	Belt-driven, MultiAir, SOHC, 16 valves, hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Cast-iron block with aluminum-alloy head and aluminum-alloy bedplate	
Compression Ratio	9.8:1 	
Maximum Turbo Boost (psi / bar)	21 psi / 1.45 bar	
Power 	160 bhp @ 5,500 rpm (117 bhp/litre)	
Torque 	184 lb.-ft. @ 2,500-4,000 rpm	
Max. Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	87 octane (R+M)/2 acceptable 
91 octane recommended	
Oil Capacity	3.8 litres (4.0 qt.) with dry filter	
Coolant Capacity	14.4 litres (4.6 qt.)	
Emission Controls 	Three-way catalytic converters, heated oxygen sensors and internal engine features	
Max. Gross Trailer Weight	Not rated for trailer tow	

Estimated EnerGuide Fuel Economy L/100km (mpg) city/hwy	9.3 (30) / 7.1 (40) with 6-speed manual transmission
9.9 (29) / 7.2 (39) with Euro Twin Clutch 6-speed transmission
10.6 (27) / 7.8 (36) with 6-speed automatic transmission	
Engine Assembly Plant	Termoli (Italy)	
	
C635 6-SPEED MANUAL TRANSMISSION		
Availability	Standard — 500L Pop, Sport,Trekking and Lounge models	
Description	1st, 2nd, 3rd gear: Triple Cone 
4th and Reverse: Double Cone
5th, 6th gear: Single Cone	
Gear Ratios		
1st	4.154	
2nd	2.118	
3rd	1.361	
4th	0.978	
5th	0.756	
6th	0.622	
Reverse	4.00	
Final-drive Ratio	3.833	
Overall Top Gear	2.38	
		
C635 EURO TWIN CLUTCH 6-SPEED TRANSMISSION	
Availability	Optional — 500L Pop	
Description	1st, 2nd gear: Double Cone 
3rd, 4th, 5th, 6th gear: Single Cone	
Gear Ratios		
1st	4.154	
2nd	2.269	
3rd	1.435	
4th	0.978	
5th	0.755	
6th	0.622	
Reverse	4.00	
Final-drive Ratio	4.118	
Overall Top Gear	2.56	
		
AISIN 6-SPEED AUTOMATIC TRANSMISSION	
Availability	Optional — 500L Sport, Trekking and Lounge models	
Gear Ratios		
1st	4.04	
2nd	2.37	
3rd	1.56	
4th	1.16	
5th	0.85	
6th	0.67	
Reverse	3.19	
Final-drive Ratio	3.683	
Overall Top Gear	2.47	
Steering Turns (lock-to-lock)	3.0	
		
BRAKES		
Availability	Standard — all 500L models	
Front		
Rotor size and type	305 x 28 (12.0 x 1.10) vented	
Caliper size and type	57 (2.24) single-piston with cast iron 	
Swept area	876.1 sq. cm (345 sq. in.)	
Rear		
Rotor size and type	264 x 10 (10.4 x 0.4) solid	
Caliper size and type	38 (1.49) single-piston with aluminum housing 	
Swept area	591.8 sq. cm (233 sq. in.)	
		
DIMENSIONS AND CAPACITIES(a) 
mm (in.) unless otherwise noted		
Wheelbase	2,612 (102.8)	
Track, Front	1,502 (59.1)	
Track, Rear	1,510 (59.4)	
Overall Length	4,249 (167.3) 4,270 (168.1)  — 500L Trekking	
Overall Width	1,774 (69.8)  — without mirrors 
2,036 (80.2)  — with mirrors
1,800 (70.9)  — 500L Trekking	
Overall Height	1,670 (65.7) 	
Ground Clearance	120 (4.7) 	
		
Drag Coefficient (Cd) (estimated)	0.310 — 500L Pop/Sport/Lounge
0.320 — 500L Trekking	
Curb Weight (estimated)	1,457 kg (3,212 lb.) — 500L with 6-speed manual 
1,470 kg (3,262 lb.)  — 500L with 6-speed Euro Twin Clutch
1,476 kg (3,254 lb.)  — 500L with6-speed automatic 	
Weight Distribution, per cent F/R	60/40 — 500L with 6-speed manual
60/40 — 500L with 6-speed Euro Twin Clutch
60/40 — 500L with 6-speed automatic 	
Fuel Tank Capacity	50 litres (13.2 imp. gal.) 	
(a) All dimensions measured at curb weight with standard tires.	
		
ACCOMMODATIONS 
mm (in.) unless otherwise noted		
Seating Capacity, F/R	2/3	
Front Seat		
Headroom	1,034 (40.7)
1,028 (40.5) with dual-pane sunroof 	
Legroom	1,015 (40.0)	
Shoulder room	1,456 (57.3)	
Hip room	1,394 (54.9)	
Total seat travel	211 (8.3)  — driver 
229 (9.0)  — passenger 	
Front row interior volume	1,529 litres (54.0 cu. ft.)	
Rear Seat		
Headroom	983 (38.7) 
965 (38.0) with dual-pane sunroof 	
Legroom	931 (36.7)	
Shoulder room	1,388 (54.6)	
Hip room	1,256 (49.4)	
Total seat travel	120 (4.7)	
Second row interior volume	1,268 litres (44.8 cu. ft.)	
Total Interior Volume	2,798 litres (98.8 cu. ft.)	
Luggage Compartment Volume	634 litres (22.4 cu. ft.) 	
Volume behind front row (maximum cargo)	1,926 litres (68.0 cu. ft.) 	
Interior Volume Index	3,429 litres (121.1 cu. ft.) 	
Trunk Liftover Height	657 (25.9)	
TIRES		
Availability 	Standard — 500L Pop, Sport and Lounge	
Size and Type	205/55R16 BSW All-season 	
Mfr. and Model	Continental Conti ProContact or Goodyear Eagle LS2 or Nexen CP671 Classe Premiere	
Revs per km (mile)	519 (836) 	
		
Availability	Standard — 500L Trekking
Included with 17-in. wheels on 500L Lounge 	
Size and Type	225/45R17 BSW All-Season	
Mfr. and Model	Continental Conti ProContact or Goodyear Eagle LS2 or Nexen CP671 Classe Premiere	
Revs per km (mile)	517 (832) 	
		
WHEELS 		
Availability	Standard — 500L Sport and 500L Lounge	
Type and Material	Cast-aluminum, 13-spoke radial design, fully painted Argento 	
Size	16 x 6.5 in.	
		
Availability	Optional — 500L Lounge	
Type and Material	Cast-aluminum, seven-spoke, oval-twist design, painted Argento 
with Grigio (grey) pockets	
Size	16 x 6.5 in.	
		
Availability	Standard — 500L Trekking	
Type and Material	Cast-aluminum, seven-hole design, machined face with painted 
Grigio pockets	
Size	17 x 7.0 in.	
		
Availability	Optional — 500L Lounge and 500L Trekking	
Type and Material	Cast-aluminum, five-oval design, painted Argento with Grigio pockets	
Size	17 x 7.0 in.	
		
Availability	Optional — 500L Lounge	
Type and Material	Cast-aluminum, seven-spoke, dual-twist design, painted Argento with Nero (black) pockets (must have optional Nero painted roof)	
Size	17 x 7.0 in.	

Availability	Optional — 500L Lounge	
Type and Material	Cast-aluminum, seven-spoke, dual-twist design, painted Argento with Bianco (white) pockets (must have optional Bianco painted roof)	
Size	17 x 7.0 in.