2016 Jeep® Grand Cherokee / Grand Cherokee SRT
CANADIAN SPECIFICATIONS

Specifications are based on the latest product information available at the time of publication. 
All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Vehicle Type	Four-door sport-utility vehicle	
Assembly Plant	Detroit, Mich. (U.S.A.)	
EnerGuide Vehicle Class	Multipurpose vehicle	
		
BODY AND CHASSIS		
Layout	Front engine, rear- or four-wheel drive	
Construction	Steel uniframe	
		
ENGINE: 3.6-LITRE PENTASTAR™ V6		
Availability	Standard on all models other than SRT	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	3,604 cu. cm (220 cu. in.)	
Bore x Stroke	96 x 83 (3.77 x 3.26)	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless 	
Construction	Aluminum deep-skirt block, aluminum alloy heads	
Compression Ratio	10.2:1	
Power (est.) 	Up to 295 hp 	
Torque (est.) 	260 lb.-ft.	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R + M)/2	
Oil Capacity	5.7 litres (6.0 qt.)	
Coolant Capacity	13.25 litres (14.0 qt.)	

Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors  and internal engine features	
Max. Gross Trailer Weight	3,812 kg (6,200 lb.)	
EnerGuide Fuel Economy 
L/100km (mpg) (city/hwy)	12.8 (22) / 9.5 (30)	
Engine Assembly Plant	Trenton, Mich., (U.S.A.)	
		
ENGINE: 5.7-LITRE V8		
Availability	Optional — Limited, Overland and Summit	
Type and Description	90-degree V-type, liquid-cooled	
Displacement	5,654 cu. cm (345 cu. ft.)	
Bore x Stroke	99.5 x 90.9 (3.92 x 3.58)	
Valve System	Variable-valve timing (VVT), pushrod-operated overhead valves, 16 valves, eight deactivating and eight conventional hydraulic lifters, all with roller followers 	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.5:1	
Power (est.) 	360 hp  at 5,150 rpm	
Torque (est.) 	390 lb.-ft. at 4,250 rpm	
Max. Engine Speed	5,800 rpm (electronically-limited)	
Fuel Requirement	Unleaded mid-grade, 89 octane (R+M)/2 — recommended; unleaded regular, 87 octane (R+M)/2 — acceptable	
Oil Capacity	6.6 litres (7 qt.)	
Coolant Capacity	13.72 litres (14.5 qt.)	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad heated oxygen sensors and internal engine features	
Max. Gross Trailer Weight	3,265 kg (7,200 lb.) 	
EnerGuide Fuel Economy 
L/100km (mpg) (city/hwy)	16.7 (17) / 10.7 (26)	
Engine Assembly Plant	Saltillo (Mexico)	

		
ENGINE:  3.0-LITRE DOHC ECODIESEL V6	
Availability	Optional — Overland and Summit	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	2,988 cu. cm (182 cu. in.)	
Bore x Stroke	83 x 92 (3.27 x 3.60)	
Valve System	Chain-driven DOHC, 24 valves 	
Fuel Injection	Common-rail, 2000 bar, Solenoid Injectors	
Construction	Iron block, aluminum alloy heads	
Compression Ratio	16.5:1	
Power (est.) 	240 hp at 3,600 rpm 	
Torque (est.) 	420 lb.-ft. at 2,000 rpm	
Max. Engine Speed	4,800 rpm (electronically limited)	
Fuel Requirement	Ultra Low-sulfur diesel	
Oil Capacity	7.8 litres (8.2 qt.)	
Coolant Capacity	11.4 litres (12 qt.)	
Emission Controls 	Cooled EGR, Oxidation catalyst, Diesel particulate filter, SCR withurea injection	
Max. Gross Trailer Weight	2,240 kg (7,200 lb.) 	
EnerGuide Fuel Economy 
L/100km (mpg) (city/hwy)	11.2 (25) / 8.4 (34)	
Engine Assembly Plant	Ferrara (Italy)	
		
ENGINE: 6.4-LITRE V8	
Availability	Standard — SRT 	
Type and Description	90-degree V-type, liquid-cooled	
Displacement,	6,417 cu. cm (392 cu. in.) 	
Bore x Stroke	103.9 x 94.5 (4.09 x 3.72) 	
Valve System	Pushrod-operated overhead valves, 16 valves with sodium-filled exhaust valves and hollow stem intake valves, 16 conventional hydraulic lifters, all with roller tips	
Fuel Injection	Sequential, multi-port, electronic, returnless; automatic features Fuel Saver mode	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.9:1	
Power 	475 hp at 6,000 rpm 	
Torque 	470 lb.-ft.  at 4,300 rpm 	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Premium 91 octane (R+M)/2 — recommended	
Oil Capacity 	6.6 litres (7 qt.) 	
Coolant Capacity	13.25 litres (14 qt.) 	
Factory Oil Fill 	0W-40 Pennzoil Ultra synthetic	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad-heated oxygen sensors and internal engine features	
Exhaust Type 	Dual exhaust with dual 102-mm (4-in.) oval black chrome tips 	
EnerGuide Fuel Economy 
L/100km (mpg) (city/hwy)	18.5 (15) / 12.6 (22)	
Engine Assembly Plant	Saltillo (Mexico) 	

TRANSMISSION: ZF AUTOMATIC, EIGHT-SPEED OVERDRIVE	
Availability	Standard — all models	
Description	Driver-interactive manual control via steering wheel paddle shifters and electronically-modulated torque converter clutch with Eco mode	
Gear Ratios		
1st	4.71	
2nd 	3.14	
3rd	2.11	
4th 	1.67	
5th 	1.29	
6th	1.00	
7th	0.84	
8th 	0.67	
Reverse 	3.30	
		
TRANSFER CASE: MP 3010		
Availability	Optional with V6	
Type	Single-speed	
Operating Mode	Full-time AWD	
Low Range Ratio	None	
Torque Split, Front/Rear	50/50 	

TRANSFER CASE: MP 3010	
Availability	Standard with 6.4-litre V8 engine 	
Type	Single-speed, electronic proportioning	
Operating Mode	Full-time 4WD	
Torque Split, Front/Rear	Variable – 40/60 Auto, 50/50 Snow and Tow, 35/65 Sport and 30/70 Track	

TRANSFER CASE: MP 3022		
Availability	Optional with the V6, V8 and EcoDiesel engines	
Type	Two-speed, electronically shifted	
Operating Modes	4x4 Low (Lock), Neutral; full-time active 4x4	
Low Range Ratio	2.72	
Torque Split, Front/Rear	Variable	
		
AXLES		
Front		
Differential Type	Conventional	
Availability	Standard on 4x4 models 	
Ring Gear Diameter	195 (7.7) 	
Axle Ratios	3.45:1 — 3.6-litre V6 and EcoDiesel
3.09:1 — 5.7-litre V8
3:70:1 — 6.4-litre V8	
Rear		
Differential Type	Conventional (optional Electronic Limited Slip on 5.7-litre V8 and EcoDiesel, Standard on 6.4-litre V8)	
Availability	Standard on all engines	
		
Ring Gear Diameter	195 (7.7)  — V6 4x4	
		
ELECTRICAL SYSTEM		
Alternator	160-amp; 180-amp or 220-amp depending on model	
Battery	Maintenance-free 
H6 650 CCA + Auxiliary 200 CCA on Electronic Stop/Start (ESS)
H7 700 CCA on V8, H8 800 CCA on 3.0-litre EcoDiesel (not equipped with ESS)	
		
SUSPENSION		
Front	Short- and long-arm independent (SLA), coil springs, gas-charged, twin-tube coilover shock absorbers, steel upper- and aluminum lower-control arms (“A” arms), aluminum knuckle, hollow stabilizer bar	
Front – SRT 	Short- and long-arm independent (SLA) with aluminum lower control arm, aluminum knuckle, aluminum clevis, coil springs, Bilstein adaptive damping suspension (ADS), upper- and lower-control arms (“A” arms), hollow stabilizer bar	
Rear	Multi-link rear suspension, coil spring, twin tube shocks (including load leveling for towing), aluminum lower control arm, independent upper links (tension and camber) plus a separate toe link, hollow stabilizer bar	
Rear - SRT	Multi-link rear suspension, coil spring, Bilstein adaptive damping suspension (ADS), aluminum lower control arm, independent upper links (tension and camber) plus a separate toe link, hollow stabilizer bar	
		
STEERING		
Type	Electric rack and pinion, SRT-tuned on SRT model	
Overall Ratio	16.7:1 	
Turning Diameter (curb-to-curb) 	11.3 m (37.1 ft.) 	
Steering Turns (lock-to-lock)	3.2 	

BRAKES		
Type	Power, single-rate, tandem diaphragm vacuum, anti-lock braking system (ABS)	
Availability	Standard	
Front		
Rotor size and type	330 x 32 (13.0 x 1.3)  vented disc – V6
350 x 32 (13.8 x 1.3)  – EcoDiesel and 5.7-litre V8
380 x 34 (15.0 x 1.34)  vented disc with Brembo six-piston caliper and ABS – SRT 6.4-litre V8
380 x 34 (15.0 x 1.34)  2-piece aluminum hat performance rotor, directionally slotted with Brembo six-piston caliper and ABS – available on SRT model	
Caliper size and type	48 (1.89)  two-piston pin-slider caliper	
Swept area	1,820 sq. cm (282 sq. in.) 
672 sq. cm (104.2  sq. in.) - SRT	
Rear		
Rotor size and type	330 x 14 (13.0 x 0.55)  disc – V6
330 x 22 (13.0 x 0.87)  vented disc – EcoDiesel and V8
350 x 28 (13.78 x 1.10)  disc with Brembo four-piston caliper and single-channel ABS – SRT
350 x 28 (13.78 x 1.10)  Performance disc , directionally slotted with Brembo four-piston caliper and single-channel ABS available on SRT	
Caliper size and type	48 (1.89)  single-piston pin-slider caliper	
Swept area	1,658 sq. cm (257 sq. in.) 
508 sq. cm (79.0 sq. in.)  — SRT	
		
DIMENSIONS AND CAPACITIES 
mm (in.) unless otherwise noted		
Wheelbase	2,915 (114.8)	
Track, Front	1,623 (63.9)
1,636 (64.4)  — SRT 	
Track, Rear	1,627 (64.1) 
1,634 (64.7)  — SRT	
Overall Length	4,822 (189.8) 	
Overall Width (Width at Mirrors)	2,154 (84.8)	
Body Width	1,943 (76.5)	
Overall Height (at Roof Rail / at Antenna)	1,761 (69.3)  / 1,779 (70.0) 
1,717/1,773 (67.6/69.8)  - SRT	
Load Floor Height	822 (32.4)  — standard suspension and SRT
807 (31.8)  — air suspension	
Sill Step Height	520 (20.5)  — standard suspension
508 (20.0)  — air suspension
527 (20.7)  — SRT	
Ground Clearance  (with P245/70R17 Tire and 3.6-litre engine)	218 (8.6)  — standard suspension
264 (10.4)  — air suspension (Pos#2)
210.8 (8.3)  — SRT	
Chassis (Fuel Tank) 	243 (9.6)  — standard suspension
271 (10.7)  — air suspension (Pos#2)
230 (9)  — SRT	
Front Axle 	236 (9.3)  — standard suspension
246 (9.7)  — air suspension (Pos#2)
227.8 (8.97)  — SRT	
Rear Axle 	253 (10.0)  — standard suspension
282 (11.1)  — air suspension (Pos#2)
228.3 (8.99)  — SRT	
Approach Angle (degrees)	26.2 — standard suspension
36.1 — air suspension (Pos#2, air-dam off)
18.45 — SRT	
Ramp Breakover Angle (degrees)	19.0 — standard suspension
22.8 — air suspension (Pos#2)
17.84 — SRT	
Departure Angle (degrees)	24.0 — standard suspension
27.1 — air suspension (Pos#2)
21.9 — SRT	
Frontal Area 	2.88 m (31.0 ft.) 
2.93 m (31.5 ft.)  — SRT	
Drag Coefficient 	0.371
0.39 - SRT	
Aero CdA	11.5 (Cd x cross-sectional area)
12.2 (Cd x cross-sectional area) — SRT	
Fuel Tank Capacity	93.1 litres (20.5 gal.) 	

ACCOMMODATIONS
 mm (in.) unless otherwise noted		
Seating Capacity (front/rear) 	2/3	
Total Interior Passenger Volume	2,985 litres (105.4 cu. ft.)	
Front		
Headroom	1,013 (39.9)	
Legroom	1,025 (40.3)	
Shoulder Room	1,491 (58.7)	
Hip Room	1,449 (57.0)	
Seat Travel	280 (11.0)	
Front Volume Index 	1,546 litres (54.6 cu. ft.)	
Rear 		
Headroom	995 (39.2)	
Legroom	981 (38.6)	
Knee Clearance	110 (4.3)	
Shoulder Room	1,474 (58.0)	
Hip Room	1,428 (56.2)	
Rear Seat Volume Index 
	1,438 litres (50.8 cu. ft.)	
Maximum Cargo Volume 	1,934 litres (68.3 cu. ft.)	
Behind Second-row Seats 
	1,028 litres (36.3 cu. ft.)	
Total Passenger plus Cargo Volume 
	3,979 litres (140.5 cu. ft.)	

WEIGHTS (Estimates)						
	MODEL	ENGINE	GVWR(a) 
kg (lb.) 	CURB WEIGHT(b) 
kg (lb.) 	PAYLOAD(c) 
kg (lb.) 	
4WD	Laredo	3.6-litre	2,948 (6,500) 	2,121 (4,677) 	600 (1,320) 	
	Limited	3.6-litre
5.7-litre
3.0-litre EcoDiesel	2,948 (6,500) 3,084 (6,800) 
3,084 (6,800) 	2,211 (4,875) 
2,329 (5,135) 
2,393 (5,275) 	580 (1,270)
585 (1,290)
580 (1,270) 	
	Overland	3.6-litre
5.7-litre
3.0-litre EcoDiesel	2,948 (6,500) 
3,084 (6,800) 
3,084 (6,800) 	2,261 (4,984) 
2,381 (5,250) 
2,446 (5,393) 	520 (1,150) 
520 (1,150) 
530 (1,170) 	
	Summit	3.6-litre
5.7-litre
3.0-litre EcoDiesel	2,948 (6,500) 
3,084 (6,800)
3,084 (6,800) 	2,247 (4,955) 
2,367 (5,219) 
2,437 (5,374) 	475 (1,050) 
475 (1,050) 
475 (1,050)	
	SRT	6.4-litre 	2,948 (6,500) 	2,315 (5,104)	612 (1,350) 	
(a) Gross Vehicle Weight Rating. 
(b) Curb weight includes standard equipment and full quantities of fuel, lubricant and coolant.
(c) Payload is the maximum allowable weight of driver, passengers, cargo, and options, rounded to the nearest 5 kg (10 lb.).	
	
WEIGHT DISTRIBUTION, F/R	
	MODEL	ENGINE	DISTRIBUTION 	
4WD	Laredo	3.6-litre	53/47	
	Limited	3.6-litre
5.7-litre
3.0-litre EcoDiesel	52/48
54/46
54/46	
	Overland	3.6-litre
5.7-litre
3.0-litre EcoDiesel	52/48
53/47
53/47	
	Summit	3.6-litre
5.7-litre
3.0-litre EcoDiesel	51/49
53/47
53/47	
	SRT 	6.4-litre 	55/45	

Wheels (in.)	
Availability	Standard on Laredo 	
Type and Material	Painted machine cast-aluminum, 5-spoke 	
Size 	17 x 8	
		
Availability	Standard Limited, available on Overland 	
Type and Material	Painted machine cast-aluminum, 10-spoke 	
Size 	18 x 8	
		
Availability	Standard on Overland, available on Limited	
Type and Material	Polished machined cast-aluminum, 5-spoke	
Size 	20 x 8	
		
Availability	Standard on Summit	
Type and Material	Polished machined cast-aluminum, twin 5-spoke (Satin Carbon painted with Premium Plus Appearance Group)	
Size 	20 x 8	
		
Availability	Standard on SRT	
Type and Material	Forged aluminum, polished, five-spoke “Goliath”	
Size 	20 x 10	
		
Availability	Optional on SRT	
Type and Material	Forged aluminum, Mineral Grey, split five-spoke	
Size 	20 x 10	
		
Availability	Optional on SRT	
Type and Material	Forged aluminum, Black Vapor Chrome, split five-spoke “Spider Money”	
Size 	20 x 10	
		
TIRES		
Availability	Standard — Laredo	
Size and Type	P245/70R17	
Mfr. and Model	Goodyear Fortera HL Black Sidewall All-Season 	
Revs per km (mile)	685 (1,103)  	
		
Availability	Standard — Limited; Optional — Laredo	
Size and Type	265/60R18 	
Mfr. and Model	Michelin Premier LTX Black Sidewall All-Season 	
Revs per km (mile)	679 (1,093)  	
		
Availability	Standard — SRT	
Size and Type	P295/45ZR20	
Mfr. and Model	Pirelli Scorpion Verde – All-season Performance (run flat)	
Revs per km (mile)	699 (1,125) 	

Availability	Optional — SRT	
Size and Type 	P295/45ZR20	
Mfr. and Model	Pirelli P-Zero – Three-season (run flat)	
Revs per km (mile)	699 (1,125)  	
		
Availability 	Standard — Overland/Summit; Optional- Limited	
Size and Type	265/50R20	
Mfr. and Model	Bridgestone Ecopia H/L 422 Plus Black Sidewall All-Season 	
Revs per km (mile)	685 (1,102) 	
		
Availability	Optional — Overland/Summit/Limited	
Size and Type	265/50R20 	
Mfr. and Model	Pirelli Scorpion Verde Black Sidewall All-Season	
Revs per km (mile)	686 (1,104) 	
		
Packaged with Off-road Adventure II (AWY)	Packaged with Off-road Adventure II (AWY)	
Size and Type	265/60R18	
Mfr. and Model	Goodyear Wrangler All-Terrain Adventure with Kevlar Black Sidewall	
Revs per km (mile)	685 (1,102) 	
		
Parking Brake Type	Drum-in-hat	
Four–wheel Anti-lock Brakes	Standard	
Electronic stability control	Standard	
All-speed traction control	Standard	
Brake Assist	Standard	

TRAILER TOWING				
	Engine	Axle Ratio	Maximum Trailer  
Weight  kg (lb.) 	
4WD 	3.6-litre V6
5.7-litre V8
3.0-litre EcoDiesel V6	3.45 
3.09
3.45	2,818 (6,200) 
3,265 (7,200) 
3,265 (7,200)	
	6.4-litre V8	3.70	3265 (7,200)