2016 Jeep® Patriot
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Vehicle Type	Sport-utility vehicle	
Assembly Plant	Belvidere, Illinois (U.S.A.)	
EnerGuide Vehicle Class	Compact SUV	
		
BODY AND CHASSIS		
Layout	Transverse front-engine front-wheel drive or four-wheel drive	
Construction	Unitized steel body 	
		
ENGINE: 2.0-LITRE I-4 WORLD GAS ENGINE 	
Availability	Standard — 2WD Patriot Sport and 2WD Patriot Latitude	
Type and Description 	Four cylinders in-line, tuned intake manifold with electronic active charge motion control valves, dual counter-rotating balance shafts	
Displacement	1,998 cu. cm (121.9 cu. in.)	
Bore x Stroke	86 x 86 (3.39 x 3.39)	
Valve System	Chain-driven DOHC, 16 valves, electronically controlled dual variable-valve timing (VVT), direct-acting shimless mechanical bucket tappets 	
Fuel Injection 	Sequential, multiport, electronic, returnless	
Construction 	High-pressure die-cast aluminum block with dry iron liners, cast-aluminum cylinder head, cast-aluminum ladder frame, forged steel crankshaft	
Compression Ratio	10.5:1	
Power 	158 bhp @ 6,400 rpm (79 bhp/litre)	
Torque 	141 lblb-ft @ 5,000 rpm 	
Maximum Engine Speed	6,750 rpm (electronically limited)	
Fuel Requirement 	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity	4.7 litres (5.0 qt.) SAE 5W/20	
Coolant Capacity	6.8 litres (7.2 qt.)	
Emission Controls	Single catalytic converter, dual heated oxygen sensors and engine features	
Smog-forming Pollution	0.56 g/km (0.9 g/mile)	
2015 EnerGuide Fuel Economy 
L/100km (mpg) city/hwy	7.8 (36) / 10.2 / 9.2 – 4x2 with 5-speed manual
8.8 (32) / 10.7 / 9.9 – 4x2 with CVT	
ENGINE: 2.4-LITRE WGE I-4	
Availability	Standard — 4x4 models, optional 4x2 	
Type and Description	Four-cylinder in-line, tuned intake manifold with electronic active charge motion control valves, dual counter-rotating balance shafts	
Displacement	2,360 cu. cm (144 cu. in.)	
Bore x Stroke	88 x 97 (3.46 x 3.82)	
Valve System	Chain-driven DOHC, 16 valves, electronically controlled dual VVT, direct-acting shimless mechanical bucket tappets 	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	High-pressure die-cast aluminum block with dry iron liners, cast-aluminum cylinder head, cast-aluminum ladder frame, forged steel crankshaft	
Compression Ratio	10.5:1	
Power 	172 bhp @ 6,000 rpm (72 bhp/litre)	
Torque 	165 lb.-ft. @ 4,400 rpm 	
Maximum Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity	4.7 litres (5.0 qt.) SAE 5W/20	
Coolant Capacity	6.8 litres (7.2 qt.)	
Emission Controls 	Single catalytic converter — 2WD 
Dual catalytic converter — 4WD 
Dual heated oxygen sensors and engine features 	
Smog-forming Pollution	0.56 g/km (0.9 g/mile)	
Maximum Gross Trailer Weight	450 kg (1,000 lb.)  900 kg (2,000 lb.)  — with Freedom Drive II Package, Trailer-tow Prep Group	
2015 EnerGuide Fuel Economy L/100km (mpg) city/hwy	8.2 (34) / 10.2 (28)  – 4x2 with 5-speed manual
8.6 (33) / 11.2 (25) – 4x2 with 6-speed automatic
8.6 (33) / 10.6 (27) – 4x4 with 5-speed manual
8.7 (32) / 11.4 (25) – 4x4 with 6-speed automatic	
	
TRANSAXLE: MAGNA DRIVELINE T355 FIVE-SPEED MANUAL	
Availability	Standard — 2.0-litre engine
Standard — 2.4-litre engine	
Description	Five-speed, overdrive, synchronized in all forward ratios, cable-operated, 
3-plane shifter	
Gear Ratios		
1st	3.77	
2nd	2.16	
3rd	1.41	
		
4th	1.026	
5th	0.72	
Reverse	3.417	
Final-drive Ratio	4.12	
Overall Top-gear	2.97	
		
TRANSAXLE: SIX-SPEED AUTOMATIC 6F24 PowerTech WITH AUTO STICK	
Availability	Optional — 2.4-litre engine (FWD and AWD)	
Description	Six-speed automatic transmission, lockup torque converter, electronic controls	
Gear Ratios		
1st	4.212	
2nd	2.637	
3rd	1.800	
4th	1.386	
5th	1.000	
6th	0.772	
Reverse 	3.285	
Final-drive Ratio	3.367:1 (2.4-litre engine)	
Overall Top-gear Ratio	2.600 (2.4-litre engine)	
Auto Stick	Standard	
		
TRANSAXLE: AUTOMATIC JATCO MODEL CVT2	
Availability	Optional — 2.0-litre engine	
Description	Continuously variable ratio, lockup torque converter, electronic controls	
Gear Ratios		
Forward	2.349:1 to 0.394:1 continuously variable	
Reverse	1.75:1	
Final-drive Ratio	6.12:1	
Overall Top-gear Ratio	2.41:1	
Effective Maximum Low-gear Ratio	19.11:1	
	
TRANSAXLE: AUTOMATIC JATCO MODEL CVT2L	
Availability	Optional — Patriot 4WD with 2.4-litre engine and Freedom Drive II	
Description	Continuously variable ratio, lockup torque converter, electronic controls	
Gear Ratios		
Forward	2.349:1 to 0.394:1 continuously variable	
Reverse	1.75:1	
Final-drive Ratio	8.135:1	
Overall Top-gear Ratio	3.21:1	
Effective Maximum Low-gear Ratio	19.11:1	
		
DRIVETRAIN		
Front-wheel Drive		
Availability	Standard	
Front Differential 	Open	
Four-wheel Drive		
Availability	Optional	
Type	Electronically-controlled coupling (ECC) with four-wheel drive Lock	
Rear Differential 	Open	
		
ELECTRICAL SYSTEM		
Alternator	120-amp
140-amp with CVT2L	
Battery	525 CCA, maintenance-free	
		
DIMENSIONS AND CAPACITIES 
mm (in.) unless otherwise noted		
Wheelbase	2,634 (103.7)	
Track — Front	1,520 (59.8)	
Track — Rear	1,520 (59.8)	
Overall Length	4,414 (173.8)	
Overall Width	1,757 (69.2)	
Overall Height	1,663 (65.5) — 2WD, 1,696 (66.8) — 4x4 	
Overhang — Front	885 (34.7)	
Overhang — Rear	894 (35.1)	
Approach Angle with P215/60/R17 Tire (degrees)	26.4	
Breakover Angle with P215/60/R17 Tire (degrees)	20.9	
Departure Angle with P215/60/R17 Tire (degrees)	28.5	
Ground Clearance with P215/60/R17 Tire	205 (8.1) 	
Approach Angle with Freedom Drive II 
Off-road Package including P215/65/R17 Tire (degrees)	29.0	
Breakover Angle with Freedom Drive II 
Off-road Package including P215/65/R17 Tire (degrees)	23.7	
Departure Angle with Freedom Drive II 
Off-road Package including P215/65/R17 Tire (degrees)	33.9	
Ground Clearance with Freedom Drive II Off-road Package including P215/65/R17 Tire	231 (9.1)	
Aero (CdA)	10.4 — 2WD
11.0 — 4WD	
Curb Weight, Estimated	1,421 kg (3,133 lb.)  — Sport 2WD, 2.0-litre MTX
1,456 kg (3,211 lb.) — Sport 2WD, 2.0-litre CVT2 ATX
1,423 kg (3,137 lb.)  — Sport 2WD, 2.4-litre MTX
1,457 kg (3,213 lb.)  — Sport 2WD, 2.4-litre ATX
1,492 kg (3,290 lb.)  — Sport 4WD, 2.4-litre MTX
1,527 kg (3,367 lb.) — Sport 4WD, 2.4-litre ATX
1,530 kg (3,373 lb.) — Sport 4WD, 2.4-litre CVT2L ATX	
Weight Distribution, per cent F/R	58/42 — 2WD
57/43 — 4WD	
Fuel Tank Capacity litre (gal.)	51.5 (13.6) — 2WD
51.1 (13.5) — 4WD	
		
ACCOMMODATIONS mm (in.) unless otherwise noted		
Seating Capacity — F/R	2/3	
Front		
Headroom without Sunroof	1,040 (41.0)	
Legroom	1,032 (40.6)	
Shoulder Room	1,385 (54.5)	
Hip Room	1,328 (52.3)	
Seat Travel	Driver — 260 (10.2)  
Passenger — 260 (10.2)	

Recliner Angle Range (degrees)	Driver — Up to 88 
Passenger — up to 88 	
Front Volume Index	1,481 litres (52.3 cu ft)	
Rear		
Headroom	1,014 (39.9)	
Leg Room	1,001 (39.4)	
Knee Clearance	44.1 (1.7)	
Shoulder Room	1,372 (54.0)	
Hip Room	1,295 (51.0)	
Rear Seat Volume Index	1,390 litres (49.1 cu. ft.)	
Interior Volume	2,956 litres (104.4 cu. ft.)	
Cargo Volume Indexes		
Rear Seats Up	651 litres (23.0 cu. ft.)	
Rear Seats Folded	1,532 litres (54.1 cu. ft.)	
Interior Volume Index	3,523 litres (124.4 cu. ft.)	
Trunk Lift-over Height	779.8 (30.7)	
Cargo Volume with Front Passenger Fold-flat seat and Rear-seat folded	1,795 litres (63.4 cu.ft.)	
Minimum Cargo Width at 
Liftgate Opening	988 (38.9)	
Minimum Cargo Height at 
Liftgate Opening	656 (25.9)	
Maximum Cargo Width at 
Liftgate Opening	1,146 (45.1)	
Maximum Cargo Height at 
Liftgate Opening	966 (27.4)	
Distance Between Wheelhouse 
Interior Trim 	965 (38)	
		
SUSPENSION 		
Front	Independent MacPherson strut, coil spring over gas-charged shock absorbers and stabilizer bar — standard	
Rear	Multi-link independent with coil springs, link-type stabilizer bar, gas-charged shock absorbers — standard 	

STEERING		
Type	Rack and pinion with hydraulic power assist	
Overall Ratio	16.4:1	
Turning Diameter (curb-to-curb)	With 16- or 17-in. wheels — 10.8 m (35.6 ft.)	
Steering Turns (lock-to-lock)	With 16- or 17-in. wheels and tires — 2.88	
		
WHEELS (in.)		
Availability	Standard on Patriot Sport	
Type and Material	Styled steel	
Size	16 x 6.5 	
		
Availability	Standard on Patriot North	
Type and Material	Polished aluminum	
Size	17 x 6.5	
		
Availability	Standard on Patriot High Altitude	
Type and Material	Polished aluminum with Granite painted pockets	
Size	17 x 6.5	
		
TIRES		
Availability	Standard on Patriot Sport and North	
Size and Type	P205/70R16 BSW All-season Touring	
Manufacturer and Model	Goodyear Eagle LS2	
Revs per km (mile)	470 (758) 	
		
Availability	Standard on Patriot High Altitude	
Size and Type	P215/60R17 BSW All-season Touring	
Manufacturer and Model	Firestone Affinity	
Revs per km (mile)	479 (771) 	
		
Availability	Included with Freedom Drive II Off-road Package and Tire and Wheel Group	
Size and Type	P215/65R17 OWL All-terrain	
Manufacturer and Model	Goodyear Wrangler GTA 03	
Revs per km (mile)	462 (743) 	

Availability	Optional on North	
Size and Type	P225/60R17 BSW All-season Touring	
Manufacturer and Model	Kumho Solus KL21	
Revs per km (mile)	470 (756) 	
		
BRAKES 		
Availability	Standard on Patriot Sport 4x2, Patriot Latitude 4x2	
Front		
Size and Type	294 x 26 (11.5 x 1.0) vented disc with 57 (2.2) single-piston floating caliper	
Swept Area	1,442 sq. cm (223 sq. in.)	
Rear		
Size and Type	229 x 35 (9.0 x 1.38) drums 	
Swept Area	503.6 sq. cm (78.1 sq. in.)	
Power-assist Type	254 (10.0) single-diaphragm vacuum	
Anti-lock Brake System (ABS)	Standard	
Electronic Stability Control (ESC)	Standard	
		
Availability	Standard on Patriot Sport 4x4, Latitude 4x4 and Limited 4x2 and 4x4	
Front		
Size and Type	294 x 26 (11.5 x 1.0) vented disc with 57 (2.2) single-piston floating caliper	
Swept Area	1,442 sq. cm (223 sq. in.)	
Rear		
Size and Type	262 x 10 (10.3 x 0.39) solid disc with 35 (1.4) single-piston 
floating caliper	
Swept Area	894.6 sq. cm (138.64 sq. in.)	
Power-assist Type	254 (10) single-diaphragm vacuum 	
Anti-lock Brakes with On- and Off-road Calibrations	Standard	
Electronic Stability Control (ESC)	Standard	
Hill-start Assist (HSA)	Standard with manual transmission and Freedom Drive II Off-road Package	
Off-road brake Traction-control System (BTCS)	Included with Freedom Drive II Off-road Package 	
Hill-descent Control (HDC)	Included with Freedom Drive II Off-road Package