2017 Chrysler Pacifica
Canadian SPECIFICATIONS

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

General Information		
Vehicle Type	Multipurpose vehicle 	
Assembly Plant	Windsor, Ontario 	
EnerGuide Vehicle Class	Multipurpose vehicle	
Introduction Date	Spring 2016	
		
BODY/CHASSIS		
Layout	Transverse front engine, front-wheel drive	
Construction	Steel unibody with hinged front doors; aluminum-skinned sliding left and right side doors — power available; magnesium-structured/aluminum-skinned rear liftgate with gas props — power available	
		
Engine: 3.6-Litre Pentastar™ V6	
Availability	Standard on gas engine models	
Type and Description	60-degree dual overhead cam engine. 	
Displacement	3,605 cu. cm (220 cu. in.) 	
Bore x Stroke	96mm x 83mm	
Valve System	24-valve, end pivot roller finger followers with variable valve lift (intake only) and continuous variable-valve timing on both intake and exhaust cams; chain-driven	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	High-pressure die-cast A380 aluminum block with iron liners and semi-permanent mould A319 aluminum heads	
Compression Ratio	11.3:1	
Power 	287 hp @ 6,400 rpm	
Torque 	262 lb.-ft. @ 4,000 rpm	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane, or E0 to E15	
Oil Capacity	4.7 litre (5 qt.)  	
Coolant Capacity	6.8 litre (7.2 qt.) 	

Emission Controls 	Integrated cast-aluminum header manifolds; positive crankcase ventilation; inlet and exhaust cam phasers with internal cooled exhaust gas recirculation; evaporative emissions system	
EnerGuide Fuel Economy L/100km (mpg) (city/hwy)	12.9 (22) / 8.4 (34)	
Assembly Plant	Saltillo (Mexico)	
		
Engine: 3.6-Litre Pentastar V6 HYBRID	
Availability	Standard on hybrid models	
Type and Description	60-degree dual overhead cam engine	
Displacement	3,605 cu. cm (220 cu. in.) 	
Bore x Stroke	96mm x 83mm	
Valve System	24-valve, end pivot roller finger followers and continuous variable-valve timing on both intake and exhaust cams; chain-driven	
Fuel System	Port-fuel injection (PFI)	
Construction	High-pressure die-cast A380 aluminum block with iron liners and semi-permanent mould A319 aluminum heads	
Compression Ratio	12.5:1	
Power 	Estimated 248 hp @ 5,800 rpm	
Torque 	Estimated 230 lb.-ft. @ 4,400 rpm	
Max. Engine Speed	5,800 rpm (electronically limited) 	
Fuel Requirement	Unleaded regular, 87 octane, or E0 to E15	
Oil Capacity	4.7 litre  (5 qt.) 	
Coolant Capacity	6.8 litre (7.2 qt.) 	
Emission Controls 	Integrated cast-aluminum header manifolds; positive crankcase ventilation; intake and exhaust cam phasers; evaporative emissions system	
EnerGuide Fuel Economy Le/100km (mpge) (city/hwy)	TBD	
Assembly Plant	Trenton (Mich.) and 
Saltillo (Mexico)	
	
TRANSMISSION: 948TE TORQUEFLITE AUTOMATIC NINE-SPEED 	
Availability	Standard on gas engine models	
Description	Nine-speed FWD, electronically controlled automatic overdrive transmission with torque converter clutch. Clutch-to-clutch architecture, 
with integral electro/hydraulic control module	
Gear Ratios		
1st 	4.70	
2nd	2.84    	
3rd 	1.91	
4th	1.38  	
5th 	1.00	
6th 	0.81	
7th 	0.70	
8th 	0.58	
9th 	0.48	
Reverse 	3.81    	
Spread	9.81	
Final Drive Ratio	3.25	
	
TRANSMISSION: ELECTRICALLY VARIABLE 	
Availability	Standard on hybrid models	
Description	Electrically variable transmission with dual-motor EV drive capability 	
		
Suspension		
Front	Independent MacPherson strut, coil over gas-charged shock absorbers, stabilizer bar with hydroformed steel perimeter cradle 	
Rear	Independent twist-blade with coil springs, twin-tube shock absorbers with integrated rebound springs (gas engine models)
Independent twist-blade with coil springs, twin-tube shock absorbers with integrated rebound springs (hybrid models)	
		
STEERING		
Type	Electric rack and pinion	
Overall Ratio	16.2:1	
Turning Diameter (curb-to-curb)	12.1 m (39.7 ft.) 	
Steering Turns (lock-to-lock)	3.13	
		
BRAKES mm (in.) unless otherwise noted		
Power-assist Type	Vacuum assist	
Availability	Standard on all models	
Front		
Size and type	330 x 28 (13.0 x 1.1)  vented rotor with 51.0 single-piston floating caliper	
Swept area	475 sq. cm (73.6 sq. in.) 	
Rear		
Size and type	330 x 12 (13.0 x 0.47)  solid rotor with 44.0 single-piston floating caliper	
Swept area	429 sq. cm (66.5 sq. in.) 	
Parking Brake Type	Electric park brake 	
Anti-lock Brake System (ABS)	Standard    	
Electronic Stability Control (ESC) 	Standard	
Traction Control	Standard	
Brake Assist	Standard	
		
Dimensions and Capacities 
mm (in.) unless otherwise noted		
Wheelbase	3,089 (121.6) 	
Overhang—Front	956 (37.6) 	
Overhang—Rear	1,127 (44.3) 	
Track—Front	1,735 (68.3)  gas engine models
1,734 (68.2)  hybrid models	
Track—Rear	1,736 (68.3)  gas engine models
1,735 (68.3)  hybrid models	
Overall Length	5,172 (203.6) 	
Overall Width	2,022 (79.6) 	
Overall Width with Mirrors	2,297 (90.4) 	
Overall Height 	1,777 (69.9) 	
Liftover Height 	632 (24.9) 	
Cargo Width at Wheelhouse 	1,239 (48.8) 	
Maximum Cargo Height 	1,214 (47.8) 	
Approach Angle (degrees)	14.0 gas engine models
13.5 hybrid models	
Ramp Breakover Angle (degrees)	12.5	
Departure Angle (degrees)	18.8 gas engine models
18.6 hybrid models	
Ground Clearance 	131 (5.1)  gas engine models
130 (5.1)  hybrid models	
Drag Coefficient (Cd)	0.300	
Aero CdA	9.95	
Fuel Tank Capacity, litres (imp. gal.)	71.9 (15.8) gas engine models
64.3 (14.1) hybrid models	
Gross Vehicle Weight Rating, kg (lbs.)	2,724 (6,005)  gas engine models
2,858 (6,300)  hybrid models	
Maximum Towing Capacity, kg (lbs.)	1,633 (3,600)  gas engine models (when properly equipped)
Not recommended for hybrid models	

Curb Weight, kg (lbs.)	1,964 (4,330)  gas engine models
2,242 (4,943)  hybrid models	
Weight Distribution (per cent front/rear)	55/45 gas engine models
56.5/43.5 hybrid models	
		
Accommodations 
mm (in.) unless otherwise noted		
Seating Capacity (front/second/third rows)	2/2/3 or 2/3/3 gas engine models
2/2/3 hybrid models	
Total Interior Volume	5,587 litres (197.3 cu.ft.)	
Front		
Head Room	1,020 (40.1) 	
Head Room with Sunroof 	975 (38.4) 	
Leg Room	1,045 (41.1) 	
Shoulder Room	1,622 (63.8) 	
Hip Room	1,500 (59.0)  	
Seat Travel	220 (8.7) 	
Recliner Angle Range (degrees)	58	
First Row Volume 	1,730 litres (61.1 cu.ft.)	
Second Row 		
Head Room	1,006 (39.6) 	
Head Room with Sunroof 	975 (38.4) 	
Legroom	992 (39.0) 	
Minimum Knee Clearance	119 (4.7) 	
Shoulder Room	1,602 (63.0) 	
Hip Room	1,647 (64.8) 	
Second Row Volume	1,600 litres (56.5 cu.ft.)	
Third Row 		
Head Room	984 (38.7) 	
Head Room with Sunroof 	984 (38.7) 	
Legroom	929 (36.5) 	
Knee Clearance	88.7 (3.5) 	
Shoulder Room	1,555 (61.2) 	
Hip Room	1,262 (49.6) 	
Third Row Volume	1,345 litres (47.5 cu.ft.)	
		
Cargo Volume 		
Maximum Passenger Volume	4,672 litres (165.0 cu.ft.)	
Maximum Volume 
behind First Row	3,979 litres (140.5 cu.ft.)	
Maximum  Volume 
behind Second Row	2,478 litres (87.5 cu.ft.)	
Maximum Volume 
behind Third Row	915 litres (32.3 cu.ft.)	
Total Passenger plus Volume 
behind Third Row	5,587 litres (197.3 cu.ft.)	
		
Wheels (in.)		
Availability	Standard on Touring-L, Touring-L Plus, Touring Hybrid, Limited Hybrid	
Type and Material	Cast aluminum 	
Size	17 x 7	
Availability	Standard on Limited; Optional on Touring-L Plus	
Type and Material	Cast aluminum	
Size	18 x 7.5	
Availability	Optional on Limited	
Type and Material	Cast aluminum	
Size	20 x 7.5	
		
Tires		
Availability	Standard on Touring-L, Touring-L Plus, Touring Hybrid, Limited Hybrid	
Size and Type	235/65R17 BSW, All-season 	
Model	Kumho Solus TA31, Yokohoma Avid S34	
Availability	Standard on Limited; Optional on Touring-L Plus	
Size and Type	235/60R18 BSW, All-season	
Model	Michelin Premier A/S, Bridgestone Turanza EL440, 	
Availability	Optional on Limited	
Size and Type	245/50R20 BSW, All-season 	
Model	Kumho Solus TA31, Falken Ziex CT50	

• • •