2016 Ram ProMaster™
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Body Styles and Wheelbase	ProMaster 1500 Cargo Van 2,997 mm (118 in.) wheelbase low roof
ProMaster 1500 Cargo Van 3,454 mm (136 in.) wheelbase low roof
ProMaster 1500 Cargo Van 3,454 mm (136 in.) wheelbase high roof	
	ProMaster 2500 Cargo Van 3,454 mm (136 in.) wheelbase high roof
ProMaster 2500 Cargo Van 4,039 mm (159 in.) wheelbase high roof	
	ProMaster 3500 Cargo Van 4,039 mm (159 in.) wheelbase high roof
ProMaster 3500 Cargo Van 4,039 mm (159 in.) wheelbase high roof extended body	
	ProMaster 2500 Window Van 4,039 mm (159 in.) wheelbase high roof
ProMaster 3500 Window Van 4,039 mm (159 in.) wheelbase high roof extended body	
	ProMaster 2500 Chassis Cab 3,454 mm (136 in.) wheelbase
ProMaster 3500 Chassis Cab 4,039 mm (159 in.) wheelbase
ProMaster 3500 Chassis Cab 4,039 mm (159 in.) wheelbase extended body	
	ProMaster 2500 Chassis Cab Cutaway 3,454 mm (136 in.) 136-in. wheelbase
ProMaster 3500 Chassis Cab Cutaway 4,039 mm (159 in.) 159-in. wheelbase
ProMaster 3500 Chassis Cab Cutaway 4,039 mm (159 in.) 159-in. wheelbase extended frame	
Assembly Plant	Saltillo (Mexico)	
		
BODY AND CHASSIS		
Layout	Transverse front engine	
Construction	Unibody and ladder frame	
	
ENGINE: 3.6-LITRE PENTASTAR™ V6 	
Type and Description	60-degree gasoline V-type	
Displacement	3,604 cu cm (220 cu. in.)	
Bore x Stroke	96.0 x 83.0 (3.78 x 3.27) 	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads	
Compression Ratio	10.2:1	
Power 	280 hp at 6,400 rpm	
Torque 	260 lb.-ft. at 4,175 rpm	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity	5.7 litres (6.0 qt.)	
Coolant Capacity	13.25 litres (14.0 qt.)	
Emission Controls	Dual three-way catalytic converters, heated oxygen sensors	
		
ENGINE: 3.0-LITRE ECODIESEL I-4	
Type and Description	I-4 diesel variable geometry turbocharger 	
Displacement	2,998 cu. cm (183 cu. in.)	
Bore x Stroke	95.8 x 104 (3.78 x 4.09)	
Valve System	Gear driven DOHC	
Fuel Injection	Electronically controlled Common Rail MultiJet direct injection 	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps and aluminum alloy head 	
Compression Ratio	17.5:1	
Power 	174 hp @ 3,600 rpm	
Torque 	295 lb.-ft. @ 1,400 rpm	
Max. Engine Speed	4,200 rpm	
Fuel Requirement	Diesel	
Oil Capacity	9 litres (9.5 qt.)	
Coolant Capacity	13.33 litres (14.0 qt.)	
Emission Controls	Selective Catalytic Reduction (SCR)	
	
TRANSMISSION: 62TE AUTOMATIC SIX-SPEED, FRONT-WHEEL DRIVE	
Availability	Standard with 3.6-litre Pentastar V6	
Description	Three planetary gear sets, one overrunning clutch, full electronic control, electronically controlled converter clutch	
Gear Ratios		
1st	3.90	
2nd	2.69	
3rd	2.16	
4th	1.37 	
5th	0.95	
6th	0.65	
Reverse	3.04	
Final Drive and Overall Top Gear Ratios	3.86	
		
TRANSMISSION: MT40 MANUAL AUTOMATIC SIX-SPEED, FRONT-WHEEL DRIVE	
Availability	Standard with 3.0-litre I-4 turbo diesel	
Description	Single disc clutch with hydraulic release	
Gear Ratios		
1st	4.17 	
2nd 	2.35	
3rd 	1.46	
4th 	0.96	
5th 	0.70	
6th 	0.55	
Reverse 	4.08	
Final Drive and Overall Top Gear Ratios	4.56	
		
AXLES		
Front	IFS	
Rear	Solid axle	
	
ELECTRICAL SYSTEM	
Alternator	Cargo van with gas engine: 180-amp standard; 220-amp optional; Cargo van with diesel, all Chassis cab and all cut-away: 220-amp standard	
Battery	95 amp with 800 CCA; 100 amp with 950 CCA (diesel) 	
		
SUSPENSION	
Front	MacPherson with stabilizer bar	
Rear	Solid axle with leaf springs	
		
STEERING		
Type	Rack and pinion with hydraulic power steering	
Turns lock to lock 	Short wheelbase – 11.06; medium wheelbase – 12.46; medium-long wheelbase – 13.54; long wheelbase – 14.28	
Steering ratio 	18.85	
BRAKES		
Front Rotor mm (in.): diameter x width	 300 x 32 (11.8 x 1.26)	
Rear Rotor mm (in.): diameter x width	 280 x 16 (11.0 x 0.63)	
Front Caliper, Lining	Cast iron, dual piston (46 mm and 52 mm), Brembo
Cast iron, dual piston (50 mm and 52 mm), Brembo	
Rear Caliper, Lining	Cast iron, single piston (48 mm), Brembo
Cast iron, single piston (52 mm), Brembo	

BODY DIMENSIONS / SPECIFICATIONS	
Vehicle and Body Type	Wheelbase mm (in.)	Height Category	GVWR kg (lb.)	GCWR kg (lb.) Gas/Diesel	Curb Wt kg (lb.) without opt	Payload kg (lb.)	Front Axle GAWR kg (lb.)	Rear Axle GAWR kg (lb.)	Turning Diameter m (ft.)	Body Height mm (in.)	Body Overall Length mm (in.)	Body Width w/o mirrors mm (in.)	Vehicle Width w/ mirrors folded mm (in.)	Vehicle Width w/ mirrors mm (in.) extended	Cab to Rear Axle	Overhang Rear Axle to End of Frame	
1500 Cargo Van SWB low roof	2997
(118)	H1	3878
(8550)	5216 (11500) / 5670 (12500)	2064 (4551) / 2174 (4792)	 1810 (3990)/ 1,701 (3750)	2100 (4630)	 2270 (5004)	11.1 (36.3)	2311 (91)	4953 (195)	2101 (82.7)	2299 (90.5)	2489 (98)	 —	 —	
1500 Cargo Van MWB low roof	3454
(136)	H1	3878
(8550)	5216 (11500) / 5670 (12500)	2097 (4624) / 2205 (4862) 	 1778 (3920) / 1699 (3680)	2100 (4630)	2400 (5291)	12.4 (40.7)	2311 (91)	5413 (213.1)	2101 (82.7)	2299 (90.5)	2489 (98)	 —	 —	
1500 Cargo Van MWB high roof	3454
(136)	H2	4037 (8900)	5216 (11500) / 5670 (12500)	2161 (4764) / 2247 (4954)	1873  (4130)	2100
(4630)	2400 (5291)	12.4 (40.7)	2565 (101)	5413 (213.1)	2101 (82.7)	2299 (90.5)	2489 (98)	 —	 —	
2500 Cargo Van MWB high roof	3454
(136)	H2	4037 (8900)	5216 (11500) / 5670 (12500)	2161 (4764) / 2270 (5005) 	1873  (4130) / 1764 (3890) 	2100
(4630)	2400 (5291)	12.4 (40.7)	2565 (101)	5413 (213.1)	2101 (82.7)	2299 (90.5)	2489 (98)	 —	 —	
2500 Cargo Van LWB high roof	4039 (159)	H2	4037 (8900)	5216 (11500) / 5670 (12500)	2218 (4889)  2334 (5147)	 1819 (4010) / 1701 (3750)	2100 (4630)	2400 (5291)	14.3 (46.8)	2565 (101)	5994 (236)	2101 (82.7)	2299 (90.5)	2489 (98)	 —	 —	
3500 Cargo Van LWB high roof	4039 (159)	H2	4241 (9350)	5216 (11500) / 5670 (12500)	2224 (4903) / 2352 (5185)	 2014 (4440) / 1887 (4160)	2100 (4630)	2400 (5291)	14.3 (46.8)	2565 (101)	5994 (236)	2101 (82.7)	2299 (90.5)	2489 (98)	 —	 —	
3500 Cargo Van LWB high roof extended 	4039 (159)	H2	4241 (9350)	5216 (11500) / 5670 (12500)	2276 (5017) / 2385 (5257)	1964 (4330) / 1855 (4090)	2100 (4630)	2400 (5291)	14.3 (46.8)	2565 (101)	6350 (250)	2101 (82.7)	2299 (90.5)	2489 (98)	 —	 —	
2500 Glazed Van LWB high roof	4039 (159)	H2	4037 (8900)	5216 (11500) / 5670 (12500)	2253 (4968) / 2362 (5208)	1783 (3930) / 1674 (3690)	2100 (4630)	2400 (5291)	14.3 (46.8)	2565 (101)	5994 (236)	2101 (82.7)	2299 (90.5)	2489 (98)	 —	 —	
2500 Chassis Cab MWB	3454
(136)	H1	4037 (8900)	5216 (11500) / 5670 (12500)	1913
(4217) / 2022 (4457) 	 2123 (4680) / 2014 (4440)	2100 (4630)	2400 (5291)	12.4 (40.7)	2311 (91)	5359 (207)	2101 (82.7)	2337 (92)	2769 (109)	2057 (81)	864 (34)	
3500 Chassis Cab LWB	4039 (159)	H1	4241 (9350)	5216 (11500) / 5670 (12500)	1923 (4239) / 2032 (4480)	2318 (5110) / 2209 (4870)	2100 (4630)	2400 (5291)	14.3 (46.8)	2311 (91)	5944 (234)	2101 (82.7)	2337 (92)	2769 (109)	2642 (104)	864 (34)	
3500 Chassis Cab LWB extended	4039 (159)	H1	4241 (9350)	5216 (11500) / 5670 (12500)	1938 (4272) / 2046 (4511) 	2300 (5070) / 2191 (4830)	2100 (4630)	2400 (5291)	14.3 (46.8)	2311 (91)	6198 (244)	2101 (82.7)	2337 (92)	2769 (109)	2642 (104)	1219 (48)	
2500 Cutaway MWB	3454
(136)	H1	4037 (8900)	5216 (11500) / 5670 (12500)	1893 (4173) /  2002 (4414)	2141 (4720) / 2032 (4480)	2100 (4630)	2400 (5291)	12.4 (40.7)	2311 (91)	5258 (207)	2101 (82.7)	2337 (92)	2769 (109)	2057 (81)	864 (34)	
3500 Cutaway LWB	4039 (159)	H1	4241 (9350)	5216 (11500) / 5670 (12500)	1897 (4183) / 2012 (4435)	2341 (5160) / 2227 (4910)	2100 (4630)	2340 (5291)	14.3 (46.8)	2311 (91)	5842 (230)	2101 (82.7)	2337 (92)	2769 (109)	2642 (104)	864 (34)	
3500 Cutaway LWB extended	4039 (159)	H1	4241 (9350)	5216 (11500) / 5670 (12500)	1918 (4228) / 2026 (4468) 	 2322 (5120) / 2214 (4880)	2100 (4630)	2400 (5291)	14.3 (46.8)	2311 (91)	6198 (244)	2101 (82.7)	2337 (92)	2769 (109)	2642 (104)	1219 (48)	

Vehicle and Body Type	Wheelbase mm (in.)	Track Front mm (in.)	Track Rear mm (in.)	Approach Angle	Depart Angle	Ground Clearance mm (in.)	Seating	Width between wheel housings  mm (in.)	Cargo Volume L (cu. ft.)	Airbags	
1500 Cargo Van SWB low roof	2997 (118)	1811 (71.3)	1971 (77.6)	18.6°	20°	175 (6.9)	3	1422 (56)	7340 (259.2)	6	
1500 Cargo Van MWB low roof	3454 (136)	1811 (71.3)	1971 (77.6)	18.6°	20°	175 (6.9)	3	1422 (56)	8600 (303.7)	6	
1500 Cargo Van MWB high roof	3454 (136)	1811 (71.3)	1971 (77.6)	18.6°	20°	175 (6.9)	3	1422 (56)	9993 (352.9)	6	
2500 Cargo Van MWB high roof	3454 (136)	1811 (71.3)	1971 (77.6)	18.6°	20°	175 (6.9)	3	1422 (56)	9993 (352.9) 	6	
2500 Cargo Van LWB high roof	4039 (159)	1811 (71.3)	1971 (77.6)	18.6°	20°	175 (6.9)	3	1422 (56)	11899 (420.2)	6	
3500 Cargo Van LWB high roof	4039 (159)	1811 (71.3)	1971 (77.6)	18.6°	20°	175 (6.9)	3	1422 (56)	11899 (420.2)	6	
3500 Cargo Van LWB high roof extended 	4039 (159)	1811 (71.3)	1971 (77.6)	18.6°	20°	175 (6.9)	3	1422 (56)	13108 (462.9)	6	
2500 Window Van LWB high roof	4039 (159)	1811 (71.3)	1971 (77.6)	18.6°	20°	175 (6.9)	3	1422 (56)	11899 (420.2) 	6	
2500 Chassis Cab MWB	3454 (136)	1811 (71.3)	1971 (77.6)	18.6°	20°	175 (6.9)	3	—	—	6	
3500 Chassis Cab LWB	4039 (159)	1811 (71.3)	1971 (77.6)	18.6°	20°	175 (6.9)	3	—	—	6	
3500 Chassis Cab LWB extended	4039 (159)	1811 (71.3)	1971 (77.6)	18.6°	20°	175 (6.9)	3	—	—	6	
2500 Cutaway MWB	3454 (136)	1811 (71.3)	1971 (77.6)	18.6°	20°	175 (6.9)	3	—	—	6	
3500 Cutaway LWB	4039 (159)	1811 (71.3)	1971 (77.6)	18.6°	20°	175 (6.9)	3	—	—	6	
3500 Cutaway LWB extended	4039 (159)	1811 (71.3)	1971 (77.6)	18.6°	20°	175 (6.9)	3	—	—	6