2016 Ram ProMaster City
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Body Styles	ProMaster City Cargo Van 
ProMaster City Wagon	
Assembly Plant	Bursa (Turkey)	
EnerGuide vehicle class	Small commercial van (Class 1)	
		
BODY AND CHASSIS		
Layout	Front transverse engine, front-wheel drive (FWD) only	
Construction	Body-frame integral (BFI, or Unibody) with electro-galvanized steel body. Integrated steel ladder H-frame with single-piece longitudinal frame rails	
		
ENGINE: 2.4-LITRE I-4 MULTIAIR2 TIGERSHARK GAS ENGINE	
Availability	Standard on all models	
Type and Description	I-4 (inline 4) 16-valve MultiAir2 with multiport fuel injection	
Displacement 	2,360 cu. cm (144 cu. in.)	
Bore & stroke	88.0 x 97.0 (3.46 x 3.82) 	
Block material	Aluminum	
Cylinder head material	Aluminum	
Valvetrain	DOHC, four valves per cylinder (16 total)	
Ignition system	Coil-on-plug ignition, spark plugs with dual precious metals	
Fuel delivery	Sequential, multiport, electronic, returnless	
Compression ratio	10:0:1	
Power 	178 hp at 6,400 rpm 	
Torque 	174 lb.-ft. at 3,800 rpm 	
Fuel requirement	Unleaded regular, 87 octane (R+M)/2 	
Maximum engine speed	6,500 rpm (electronically limited)	
Oil capacity	5.2 litres (5.5 qt.)	
Coolant capacity	6.7 litres (7.1 qt.)	
Emissions controls	GPEC3 engine-management system with close-coupled catalyst; and wide range O2 sensor	
2015 EnerGuide Fuel Economy 
L/100 km (mpg) city/hwy	11.2 (25) / 8.1 (35)	
Engine assembly plant	Trenton, Michigan (U.S.A.)	
TRANSMISSION: 948TE NINE-SPEED AUTOMATIC	
Availability	Standard on all models	
Type	Nine-speed FWD, electronically controlled automatic overdrive transmission with torque converter clutch. Clutch-to-clutch architecture with integral electro/hydraulic controls module	
Fluid capacity	6.15 litres (6.5 qt.) 	
Torque converter	242 mm	
Gear ratios		
1st	4.70	
2nd	2.84	
3rd	1.90	
4th	1.38	
5th	1.00	
6th	0.80	
7th	0.69	
8th	0.58	
9th	0.47	
Reverse	3.81	
Final Drive Ratio	3.73	
		
SUSPENSION		
Front Suspension		
Type	MacPherson Strut, independent	
Stabilizer Bar, Solid	26	
Spring Rate (N/mm)	25	
Shock Type	Twin-tube	
Wheel Travel 	TBD	
Rear Suspension		
Type	Independent bi-link with coil springs, telescopic shock absorbers and stabilizer bar	
Stabilizer Bar, Solid 	16	
Spring Rate (N/mm)	28	
Shock Type	Twin-tube	
Wheel Travel (mm – jounce/rebound)	57/93	
		
BRAKES		
Front Type (diameter x width)	Ventilated disc, 305 x 28 (12 x 1.1) 	
Rear Type (diameter x width)	Drum, 254 x 57 (10 x 2.2) 	
Front Caliper, Lining	Cast iron, dual piston (57 mm)	
Rear Brake, Lining	Leading trailing drum brake assembly with 25 mm wheel cylinder	
Anti-lock braking system (front and rear)	Standard	
Electronic Stability Control (ESC) 	Standard	
Total Front Swept Area (mm)	5,100	
Total Rear Swept Area (mm)	12,155	
		
STEERING		
Type	Specifically calibrated hydraulic power-assisted rack-and-pinion	
Ratio	15:9:1	
Turns Lock-to-Lock	2.9	
Turn Diameter (curb-to-curb)	42 (12.8)	
		
WHEELS AND TIRES		
Wheels	16-in., steel or aluminum	
Tires	215/55R16XL all-season	
		
DIMENSIONS AND CAPACITIES 
mm (in.) unless otherwise noted		
EXTERIOR 		
Wheelbase 	3,109 (122.4)	
Track, Front	1,524 (60.0) 	
Track, Rear 	1,547 (60.9) 	
Overall Length	4,763 (187.5) 	
Overall Width 	1,831 (72.1) 	
Overall Height 	1,880 (74.0) 	
Front Overhang 	917 (36.0) 	
Rear Overhang 	742 (29.2) 	
Approach Angle (degrees)	17.3	
Departure Angle (degrees)	29.4	
Windshield Slope Angle (degrees)	49.2	
Ground Clearance	130 (5.1) 	
Fuel Tank Capacity 	61 litres (13.3 imp. gal.)	

	Cargo Van	Passenger Wagon	
Cargo Length 	2,215 (87.2) 	Behind rear seats = 1,157 (45.6) 
Rear seats folded = 1,746 (68.7) 	
Cargo Width	1,534 (60.4) 	1,191.3 (46.9) 	
Cargo Height @ Roof 	1,315.7 (51.8) 	1,198.9 (47.2) 	
Max. Cargo Volume 	3,729 litres (131.7 cu.ft.)	2,880 litres (101.7 cu.ft.)	
Cargo Width @ Wheel Well 	1,229.4 (48.4) 	1,229.4 (48.4) 	
Load Floor Height 	546.1 (21.5) 	546.1 (21.5) 	
Side Door Openings (w x h)	660 x 1168 (26 x 46)	660 x 1,168 (26 x 46)	
Rear Door Openings (w x h)	1,219 x 1,245 (48 x 49)	1,219 x 1,245 (48 x 49)	
Rear Door Swing (degrees, first detent/full open detent)	90/180	90/180	
Rear Door Split (degrees)	60 (driver side)/40 (passenger side)	60 (driver side)/40 (passenger side)	
Rear Step-in Height 	546.1 (21.5) 	546.1 (21.5) 	
Side Step-in Height 	477.5 (18.8) 	477.5 (18.8) 	
			
ACCOMMODATIONS 
mm (in.) unless otherwise noted	
	Cargo Van	Passenger Wagon	
Seating Capacity (front/rear)	2/0	2/3	
Passenger Volume 	1,821 litres (64.3 cu.ft.)	3,307 litres (116.8 cu.ft.)	
Interior Volume 	5,550 litres (196.0 cu.ft.)	5,409 litres (191.0 cu.ft.)	

Front Row (Passenger & Cargo Vans)		
Headroom 	1,169 (46.0) 	
Leg Room 	1,036 (40.8) 	
Shoulder Room 	1,506 (59.3) 	
Hip Room 	1,373 (54.1) 	
Second Row (Passenger Van Only)		
Headroom 	1,118 (44.0) 	
Leg Room 	969 (38.1) 	
Shoulder Room 	1,472 (58.0) 	
Hip Room 	1,503 (59.2) 	

CAPABILITY	
	Cargo Van	Passenger Wagon	
Gross Vehicle Weight Rating GVWR; 	2,447 kg (5,395 lb.)	2,447 kg (5,395 lb.)	
Curb Weight 	2,409 kg (3,512 lb.)	1,676 kg (3,695 lb.)	
Payload 	854 kg (1,883 lb.)	771 kg (1,700 lb.)	
Tongue Load 	91 kg (200 lb.)	91 kg (200 lb.)	
Towing Capacity 	907 kg (2,000 lb.)	816 kg (1,800 lb.)	
Gross Combined Vehicle Weight Rating 	2,676 kg (5,900 lb.)	2,676 kg (5,900 lb.)