FCA CANADA
2017 Chrysler 300
CANADIAN SPECIFICATIONS

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Vehicle Type	E-segment sedan, rear-wheel drive (RWD), all-wheel drive (AWD)	
Assembly Plant	Brampton, Ontario, Canada	
EnerGuide Vehicle Class	Full-size	
		
BODY/CHASSIS		
Layout	Longitudinal front engine, RWD	
Construction	Unitized steel body and aluminum hood	
		
Engine: 3.6-Litre PENTAStar™ 24-Valve DOHC VARIABLE VALVE TIMING V-6	
Availability	Standard — 300 Touring (RWD/AWD), 300S (RWD/AWD), 
300C (RWD/AWD) and 300C Platinum (RWD/AWD)	
Type and Description	60-degree V-type, liquid-cooled	
Displacement 	3,604 cc (220 cu. in.) 	
Bore x Stroke	96.0 x 83.0 (3.78 x 3.27) 	
Valve System	Chain-driven DOHC, 24 valves, hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum deep-skirt block with aluminum-alloy heads	
Compression Ratio	10.2:1	
Power (SAE net)	292 hp (218 kW) @ 6,350 rpm (81.1 hp/litre) 
300 hp (224 kW) @ 6,350 rpm (83.3 hp/litre) – 300S 	
Torque (SAE net)	260 lb.-ft. (353 N•m) @ 4,800 rpm
264 lb.-ft. (358 N•m) @ 4,800 rpm – 300S	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2 (Federal Bin 5, 
37 state compliant)	
Oil Capacity	5.7 litres (6 quarts) with dry filter	
Coolant Capacity	13.25 litres (14 quarts)	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors and internal engine features	
Max. Gross Trailer Weight (unbraked trailer)	454 kg (1,000 lbs.) 	
EnerGuide (2016) Fuel Consumption Ratings 
L/100 km (MPG – imperial gallon) city/hwy/combined	12.4 (23) / 7.7 (37) / 10.3 (27) (RWD with 845RE eight-speed automatic transmission)
12.8 (22) / 8.6 (33) / 10.9 (26) (AWD with 845RE eight-speed automatic transmission)	
Based on 2016 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca 	
Engine Assembly Plant	Saltillo, Mexico	
	
ENGINE: 5.7-LITRE HEMI® V-8 WITH FOUR-CYLINDER MODE FUELSAVER MULTI-DISPLACEMENT SYSTEM (MDS)	
Availability	Optional — 300S, 300C and 300C Platinum (RWD)	
Type and Description	90-degree V-type, liquid-cooled with variable-cam timing (VCT)	
Displacement	5,654 cc  (345 cu. in.) 	
Bore x Stroke	99.5 x 90.9 (3.92 x 3.58) 	
Valve System	Pushrod-operated overhead valves, 16 valves, eight deactivating 
and eight conventional hydraulic lifters, all with roller followers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.5:1	
Power (SAE net)	363 hp (270 kW) @ 5,200 rpm (63.7 hp/litre) 	
Torque (SAE net)	394 lb.-ft. (534 N•m) @ 4,200 rpm	
Max. Engine Speed	5,800 rpm (electronically limited)	
Fuel Requirement	Unleaded midgrade, 89 octane (R+M)/2 — Recommended 
Unleaded regular, 87 octane (R+M)/2 — Acceptable	
Oil Capacity	6.6 liters (7 quarts) 	
Coolant Capacity	13.9 (14.7 quarts) 	
Emission Controls 	Dual close-coupled three-way catalytic converters, 
Quad heated oxygen sensors and internal engine features	
Max. Gross Trailer Weight	454 kg (1,000 lbs.) 	
EnerGuide (2016) Fuel Consumption Ratings 
L/100 km (MPG – imperial gallon) city/hwy/combined	14.8 (19) / 9.3 (30) / 12.3 (23) (RWD with 8HP70 eight-speed automatic transmission)	
	
TRANSMISSION: 845RE TORQUEFLITE EIGHT-SPEED AUTOMATIC 	
Availability	Included with 3.6-litre Pentastar V-6 engine on 300 Touring, 
300S, 300C and 300C Platinum	
	300S and 300C Platinum include Sport mode and die-cast 
paddle shifters	

Description	Adaptive electronic control, Sport mode or paddle-shifted 
driver-interactive manual control. Five-clutch pack design with only two open clutches in any gear. Off-centre line pump with low-viscosity oil for reduced spin loss. Torque converter lock with turbine torsional damper for low lock-up speeds in 1st through 8th gear 	
Gear Ratios		
1st	4.71	
2nd	3.14	
3rd	2.10	
4th	1.67	
5th	1.29	
6th 	1.00	
7th 	0.84	
8th 	0.67	
Reverse	3.30	
Final Drive Ratio	2.62 (RWD)
3.07 (AWD)	
Overall Top Gear	1.75 (RWD)
2.05 (AWD)	
		
TRANSMISSION: 8HP70 TORQUEFLITE EIGHT-SPEED AUTOMATIC 	
Availability	Optional on 300S, 300C, and 300C Platinum	
Description	Includes Sport mode and die-cast paddle shifters	
Gear Ratios		
1st	4.714	
2nd	3.143	
3rd	2.106	
4th	1.667	
5th	1.285	
6th 	1.000	
7th 	0.839	
8th 	0.667	
Reverse	3.317	
Overall Top Gear	1.75	
		
TRANSFER CASE		
Availability	Included on 300 Touring AWD, 300S AWD, 300C AWD and 300C Platinum AWD models	
Type	Active, fully variable with front-axle disconnect 	
Center Differential	Planetary	
Torque Split, Front/Rear	Fully variable	
		
ELECTRICAL SYSTEM		
Alternator	160-amp — standard on 300 Touring	
	180-amp — standard on 300S, 300C and 300C Platinum	
Battery	H7 Case, 730 CCA, maintenance-free	
		
SUSPENSION		
Front 	Independent SLA with high upper “A” arm, coil spring over gas-charged-monotube shock absorbers and stabilizer bar. Lateral and diagonal lower links with dual ball joint knuckles	
	One piece lower-control arms — included with AWD	
Rear	Five-link independent with coil springs, gas-charged monotube shock absorbers, stabilizer bar and isolated suspension cradle 	
Comfort-tuned Suspension 	Standard on 300 Touring and 300C (RWD)	
Touring-tuned Suspension 	Standard on 300C Platinum (RWD) 
Available on 300 Touring and 300C (RWD) with 20-in.wheels	
AWD Touring-tuned Suspension 	Standard on 300 Touring, 300S, 300C and 300C Platinum  (AWD)	
Performance-tuned Suspension	Standard on 300S (RWD)	
		
STEERING		
Type	Rack and pinion with hydraulic power assist	
Overall Ratio	V-6 (RWD) — 15.5:1	
	V-6 (AWD) — 16.5:1	
	V-8 (RWD) — 15.5:1	
Steering Turns (lock-to-lock)	V-6 (RWD) — 2.8	
	V-6 (AWD) — 3.1	
	V-8 (RWD) — 2.8	
		
BRAKES		
Touring Brake Package 	Standard on 300 Touring, 300S, 300C and 300C Platinum (RWD)	
Front		
Rotor Size and Type	320 x 28 (12.6 x 1.1) vented	
Caliper Size and Type	60 (2.36) single-piston sliding with aluminum housing	
Swept Area	1,358 sq. cm (210 sq. in.) 	
Rear		
Rotor Size and Type	320 x 10 (12.6 x 0.4)	
Caliper Size and Type	42 (1.65) single-piston sliding with aluminum housing	
Swept Area	1,703 sq. cm (264 sq. in.)	
		
Sport Brake Package 	Standard on 300 Touring, 300S, 300C and 300C Platinum (AWD)	
	Included with 5.7-litre HEMI V-8 engine on 300S, 300C and 300C Platinum (RWD)	
Front		
Rotor Size and Type	345 x 28 (13.6 x 1.26) vented	
Caliper Size and Type	42 (1.65) dual-piston sliding with aluminum housing	
Swept Area	1,606 sq. cm 249 sq. in. 	
Rear		
Rotor Size and Type	320 x 22 (12.6 x 0.87) vented	
Caliper Size and Type	42 (1.65) single-piston sliding with aluminum housing	
Swept Area	1,703 sq. cm (264 sq. in.) 	
		
DIMENSIONS AND CAPACITIES		
Wheelbase	3,052 (120.2) 	
Track, Front	1,611 (63.4) 	
Track, Rear	1,620 (63.8) 	
Overall Length	5,044 (198.6) 	
Overall Width	1,902 (75.0) 	
Overall Height	300 (RWD with 18-in. wheels) — 1,485.2 (58.5) 	
	300 (RWD with 20-in. wheels) — 1,492.0 (58.7) 	
	300 (AWD with 19-in. wheels) — 1,503.9 (59.2) 	
Ground Clearance		300 (RWD with 18-in. wheels) — 120.3 (4.7) 	
	300 (RWD with 20-in. wheels) — 127.9 (5.0) 	
	300 (AWD with 19-in. wheels) — 122.3 (4.8) 	
Drag Coefficient (Cd)	0.320 	
		
Curb Weight, kg, (lb)	V-6 (RWD) — 1,820 (4,013) 	
	V-6 (AWD) — 1,935 (4,267) 	
	V-8 (RWD) — 1,987 (4,380) 	
Weight Distribution, percent F/R	V-6 (RWD) — 52/48	
		V-6 (AWD) — 53/47	
	V-8 (RWD) — 53/47	
Fuel Tank Capacity, litre (imperial gallon)	70 (15.4) 	
		
ACCOMMODATIONS		
Seating Capacity, F/R	2/3	
Front		
Headroom	981 (38.6) 
936.6 (36.9)  with dual-pane sunroof	
Legroom	1,061 (41.8) 	
Shoulder Room	1,510 (59.5) 	
Hip Room	1,428 (56.2) 	
Seat Travel	Driver — 270 (10.6) 
Passenger — 220 (8.66) 	
Recliner angle range, deg.	Power — 70.7
Manual — 70	
EPA front row interior volume, litres (cu. ft.)	1,574 (55.6) 	
Rear Seat		
Headroom	963 (37.9) 
937 (36.9) with dual-pane sunroof	
Legroom	1,019 (40.1) 	
Knee Clearance	99 (3.9) 	
Shoulder Room	1,465 (57.7)  	
Hip Room	1,425 (56.1) 	
EPA second row interior volume, litres (cu. ft.)	1,435 (50.7) 	
Total Interior Volume, litres, (cu. ft.)	3,010 (106.3)  	
EPA Luggage Compartment Volume, 
litres, (cu. ft.)	462 (16.3) 	
EPA Interior Volume Index, litres (cu. ft.)	3,471 (122.6) 	
Trunk Liftover Height	768.9 (30.1) 	
		
TIRES		
Availability	Standard on 300 Touring and 300C (RWD) 	
Size and Type	P225/60R18 BSW Touring tires	
Mfr. and Model	Firestone FR710	
		
Availability	Standard on 300 Touring, 300S, 300C and 300C Platinum (AWD)	
Size and Type	235/55R19 BSW All-season performance 	
Mfr. and Model	Michelin MXM4	
		
Availability	Standard on 300S and 300C Platinum (RWD)
Available on 300 Touring and 300C	
Size and Type	245/45R20 BSW All-season performance	
Mfr. and Model	Firestone Firehawk GTV	
		
WHEELS		
Availability 	Standard on 300 Touring and 300C (RWD)	
Type and Material	18-in. cast-aluminum, polished	
Size	18 x 8.0	
		
Availability	Standard on 300 Touring and 300C (AWD)	
Type and Material	19-in. cast-aluminum, polished 	
Size	19 x 7.5	
		
Availability	Standard on 300S (AWD)	
Type and Material	19-in. cast-aluminum, Hyper Black painted	
Size	19 x 7.5	
		
Availability	Standard on 300S Alloy Edition (AWD)	
Type and Material	19-in. cast-aluminum, Dark Bronze painted	
Size	19 x 7.5	
		
Availability	Standard on 300C Platinum (AWD)	
Type and Material	19-in. cast-aluminum, polished with satin clear 	
Size	19 x 7.5	

Availability	Standard on 300S (RWD)	
Type and Material	20-in. cast-aluminum, Hyper Black painted	
Size	20 x 8.0	
		
Availability	Standard on 300S Alloy Edition (RWD)	
Type and Material	20-in. cast-aluminum, Dark Bronze painted	
Size	20 x 8.0	
		
Availability	Available on 300 Touring and 300C (RWD)	

Type and Material	20-in. cast-aluminum, polished	
Size	20 x 8.0	
		
Availability	Standard on 300C Platinum (RWD) 	
Type and Material	20-in. cast-aluminum, polished with satin clear 	
Size	20 x 8.0