FCA CANADA
2017 Chrysler Pacifica
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

General Information		
Vehicle Type	Multipurpose vehicle 	
Assembly Plant	Windsor, Ontario, Canada 	
EnerGuide Vehicle Class	Minivan	
Introduction Date	Spring 2016	
		
BODY/CHASSIS		
Layout	Transverse front engine, front-wheel drive	
Construction	Steel unibody with hinged front doors; aluminum-skinned sliding left and right side doors — power available; magnesium-structured/aluminum-skinned rear liftgate with gas props — power available	
		
Engine: 3.6-Litre PENTAStar™ 24-Valve DOHC VARIABLE VALVE TIMING V-6	
Availability	Standard on gas engine models	
Type and Description	60-degree dual overhead cam engine. 	
Displacement	3,605 cu. cm (220 cu. in.) 	
Bore x Stroke	96mm x 83mm	
Valve System	24-valve, end pivot roller finger followers with variable valve lift (intake only) and continuous variable-valve timing on both intake and exhaust cams; chain-driven	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	High-pressure die-cast A380 aluminum block with iron liners and semi-permanent mold A319 aluminum heads	
Compression Ratio	11.3:1	
Power (SAE net)	287 hp (214 kW) @ 6,400 rpm	
Torque (SAE net)	262 lb.-ft. (355 N•m) @ 4,000 rpm	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane, or E0 to E15	
Oil Capacity	4.7 litre (5 quarts) 	
Coolant Capacity	6.8 litre (7.2 quarts) 	
	
Emission Controls 
	Integrated cast-aluminum header manifolds; positive crankcase ventilation; inlet and exhaust cam phasers with internal cooled exhaust gas recirculation; evaporative emissions system	
EnerGuide  2016 Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	12.9 (22) / 8.4 (34) / 10.9 (26)	
Based on EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca 
	
Assembly Plant	Saltillo Engine Plant, Saltillo, Mexico	

Engine: 3.6-Litre Pentastar V-6 HYBRID	
Availability	Standard on hybrid models	
Type and Description	60-degree dual overhead cam engine	
Displacement	3,605 cu. cm (220 cu. in.) 	
Bore x Stroke	96mm x 83mm	
Valve System	24-valve, end pivot roller finger followers and continuous variable-valve timing on both intake and exhaust cams; chain-driven	
Fuel System	Port-fuel injection (PFI)	
Construction	High-pressure die-cast A380 aluminum block with iron liners and semi-permanent mold A319 aluminum heads	
Compression Ratio	12.5:1	
Total System Power	Estimated 260 hp	
Fuel Requirement	Unleaded regular, 87 octane, or E0 to E15	
Oil Capacity	4.7 litre (5 quarts) 	
Coolant Capacity	6.8 litre (7.2 quarts) 	
Emission Controls 	Integrated cast-aluminum header manifolds; positive crankcase ventilation; intake and exhaust cam phasers; evaporative emissions system	
EnerGuide  Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	TBD	
Assembly Plant	Trenton Engine Complex, Trenton, Mich., USA  and 
Saltillo Engine Plant, Saltillo, Mexico	
	
TRANSMISSION: 948TE  NINE-SPEED AUTOMATIC	
Availability	Standard on gas engine models	
Description	Nine-speed FWD, electronically controlled automatic overdrive transmission with torque converter clutch. Clutch-to-clutch architecture, 
with integral electro/hydraulic control module	
Gear Ratios		
1st 	4.70	
2nd	2.84    	
3rd 	1.91	
4th	1.38  	
5th 	1.00	
6th 	0.81	
7th 	0.70	
8th 	0.58	
9th 	0.48	
Reverse 	3.81    	
Spread	9.81	
Final Drive Ratio	3.25	
	
TRANSMISSION: ELECTRICALLY VARIABLE 	
Availability	Standard on hybrid models	
Description	Electrically variable transmission with dual-motor EV drive capability 	
		
Suspension		
Front	Independent MacPherson strut, coil over gas-charged shock absorbers, stabilizer bar with hydroformed steel perimeter cradle 	
Rear	Independent twist-blade with coil springs, twin-tube shock absorbers with integrated rebound springs (gas engine models)
Independent twist-blade with coil springs, twin-tube shock absorbers with integrated rebound springs (hybrid models)	
		
STEERING		
Type	Electric rack and pinion	
Overall Ratio	16.2:1	
Turning Diameter (curb-to-curb)	12.1 m (39.7 ft.) 	
Steering Turns (lock-to-lock)	3.13	

BRAKES		
Power-assist Type	Vacuum assist	
Availability	Standard on all models	
Front		
Size and type	330 x 28 (13.0 x 1.1) vented rotor with (51.0) single-piston floating caliper	
Swept area	475 sq. cm (73.6 sq. in.) 	
Rear		
Size and type	330 x 12 (13.0 x 0.47) solid rotor with (44.0) single-piston floating caliper	
Swept area	429 sq. cm (66.5 sq. in.) 	
Parking Brake Type	Electric park brake 	
Anti-lock Brake System (ABS)	Standard    	
Electronic Stability Control (ESC) 	Standard	
Traction Control	Standard	
Brake Assist	Standard	
		
Dimensions and Capacities		
Wheelbase	3,089 (121.6) 	
Overhang—Front	960 (37.8) 	
Overhang—Rear	1,127 (44.3) 	
Track—Front	1,735 (68.3) gas engine models
1,734 (68.2) hybrid models	
Track—Rear	1,736 (68.3) gas engine models
1,735 (68.2) hybrid models	
Overall Length	5,176 (203.8) 	
Overall Width	2,022 (79.6) 	
Overall Width with Mirrors	2.297 (90.4) 	
Overall Height 	1,777 (69.9) 	
Liftover Height 	617 (24.3)	
Cargo Width at Wheelhouse 	1,239 (48.8) 	
Maximum Cargo Height 	1,208 (47.6) 	
Approach Angle (degrees)	14.0 gas engine models
13.5 hybrid models	
Ramp Breakover Angle (degrees)	12.5	
Departure Angle (degrees)	18.7 gas engine models
18.6 hybrid models	
	
Ground Clearance 	131 (5.1) gas engine models
130 (5.1) hybrid models	
Drag Coefficient (Cd)	0.300	
Aero CdA	9.95	
Fuel Tank Capacity, litres (imperial gallons)	71.9 (15.8) gas engine models
64.3 (14.1) hybrid models	
Gross Vehicle Weight Rating (GVWR), kg (lbs.)	2,724 (6,005) gas engine models
2,858 (6,300) hybrid models	
Towing Capacity, kg (lbs.)	1,633 (3,600)  gas engine models (when properly equipped)
Not recommended for hybrid models	
EPA Curb Weight, kg (lbs.)		1,964 (4,330) gas engine models
2,242 (4,943) hybrid models	
Weight Distribution (percent front/rear)	55/45 gas engine models
56.5/43.5 hybrid models	
		
Accommodations		
Seating Capacity (front/second/third rows)	2/2/3 or 2/3/3 gas engine models
2/2/3 hybrid models	
Total SAE Volume, litres (cu. ft.)	5,586.9 (197.3)	
Front		
Head Room	1,020 (40.1) 	
Head Room with Sunroof 	975 (38.4) 	
Leg Room	1,045 (41.1) 	
Shoulder Room	1,622 (63.8) 	
Hip Room	1,500 (59.0) 	
Seat Travel	220 (8.7) 	
Recliner Angle Range (degrees)	1.73 (58)	
First Row SAE Volume, litres 
(cu. ft.)	1,730 (61.1) 	
Second Row 		
Head Room	1,006 (39.6) 	
Head Room with Sunroof 	966 (38.0) 	
Legroom	992 (39.0) 	
Minimum Knee Clearance	123 (4.8) 	
Shoulder Room	1,602 (63.0) 	
Hip Room	1,647 (64.8) 	
	
Second Row SAE Volume, litres (cu. ft.)	1,599.9 (56.5)	
Third Row 		
Head Room	984 (38.7) 	
Head Room with Sunroof 	984 (38.7) 	
Legroom	929 (36.5) 	
Knee Clearance	89 (3.5) 	
Shoulder Room	1,555 (61.2) 	
Hip Room	1,258 (49.5)	
Third Row SAE Volume, litres   (cu. ft.)	1,345 (47.5)	
Cargo Volume 			
Maximum Passenger Volume, litres (cu. ft.)	4,672 (165.0)	
Maximum SAE Volume 
behind First Row, litres (cu. ft.)	3,979 (140.5)	
Maximum SAE Volume 
behind Second Row, litres (cu. ft.)	2,478 (87.5)	
Maximum SAE Volume 
behind Third Row, litres (cu. ft.)	915 (32.3)	
Total Passenger plus Volume 
behind Third Row, litres (cu. ft.)	5,586.9 (197.3)	
		
Wheels		
Availability	Standard on Touring-L and Touring-L Plus	
Type and Material	Cast aluminum 	
Size	17 x 7	
Availability	Standard on Limited; Optional on Touring-L Plus	
Type and Material	Cast aluminum	
Size	18 x 7.5	
Availability	Optional on Limited	
Type and Material	Cast aluminum	
Size	20 x 7.5	

Tires		
Availability	Standard on Touring-L and Touring-L Plus	
Size and Type	235/65R17 BSW, All-season 	
Model	Kumho Solus TA31, Yokohoma Avid S34	
Availability	Standard on Limited; Optional on Touring-L Plus	
Size and Type	235/60R18 BSW, All-season	
Model	Michelin Premier A/S, Bridgestone Turanza EL440, Nexen N’Priz RH7α	
Availability	Optional on Limited	
Size and Type	245/50R20 BSW, All-season 	
Model	Kumho Solus TA31, Falken Ziex CT50