FCA CANADA
2017 Dodge Charger / Charger SRT
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

General Information		
Vehicle Type	E-segment sedan	
Assembly Plant	Brampton, Ontario, Canada	
EPA Vehicle Class	Large car	
		
Body and CHASSIS		
Layout	Longitudinal front engine, rear-wheel drive (RWD) or all-wheel drive (AWD)	
Construction	Unitized steel body and aluminum hood	
	
Engine: 3.6-Litre PENTAStar™ 24-Valve DOHC VARIABLE VALVE TIMING V-6	
Availability	Standard — Dodge Charger SE (RWD/AWD), SXT (RWD/AWD)	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	3,604 cu. cm (220 cu. in.) 	
Bore x Stroke	96.0 x 83.0 (3.78 x 3.27 in.) 	
Valve System	Chain-driven DOHC, 24 valves, hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum deep-skirt block with aluminum-alloy heads	
Compression Ratio	10.2:1	
Power (SAE net)	292 hp (218 kW) @ 6,350 rpm (81.1 hp/litre)
300 hp (224 kW) @ 6,350 rpm (83.3 hp/litre) with Rallye Group	
Torque (SAE net)	260 lb.-ft. (353 N•m) @ 4,800 rpm
264 lb.-ft. (358 N•m) @ 4,800 rpm with Rallye Group	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity	5.7 litres (6 quarts) with dry filter	
Coolant Capacity	13.25 (14.0 quarts) 	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors and internal engine features	
Max. Gross Trailer Weight	454 kg (1,000 lbs.) 	
EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	12.4 (23) / 7.7 (37) / 10.3 (27) (RWD with 845RE eight-speed automatic transmission)
12.8 (22) / 8.6 (33) / 10.9 (26) (AWD with 845RE eight-speed automatic transmission)	
Based on 2016 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca	
Engine Assembly Plant	Saltillo, Mexico 	
		
ENGINE: 5.7-LitRE HEMI® V-8 WITH FOUR-CYLINDER MODE FUELSAVER MULTI-DISPLACEMENT SYSTEM (MDS) 	
Availability	Standard — Charger R/T 	
Type and Description	90-degree V-type, liquid-cooled with variable-cam timing (VCT)	
Displacement	5,654 cu. cm (345 cu. in.) 	
Bore x Stroke	99.5 x 90.9 (3.92 x 3.58) 	
Valve System	Pushrod-operated overhead valves, 16 valves, eight deactivating and eight conventional hydraulic lifters, all with roller followers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.5:1	
Power (SAE net)	370 hp (276 kW) @ 5,250 rpm (64.9 hp/litre) 	
Torque (SAE net)	395 lb.-ft. (536 N•m) @ 4,200 rpm 	
Max. Engine Speed	5,800 rpm (electronically limited)	
Fuel Requirement	Unleaded midgrade, 89 octane (R+M)/2 — recommended 
Unleaded regular, 87 octane (R+M)/2 — acceptable	
Oil Capacity	6.6 litres (7 quarts) 	
Coolant Capacity	13.9 (14.7 quarts) 	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad heated oxygen sensors and internal engine features	
Max. Gross Trailer Weight	454 kg (1,000 lbs.) 	
EnerGuide (2016) Fuel Consumption Ratings, L/100 km (MPG – imperial gallon) city/hwy/combined	14.8 (19) / 9.5 (30) / 12.3 (23) (RWD with 8HP70 eight-speed automatic transmission)	

ENGINE: 6.4-LitRE HEMI V-8 POWERED BY SRT	
Availability	Standard — R/T Scat Pack and SRT 392 	
Type and Description	90-degree V-type, liquid-cooled	
Displacement	6,417 cu. cm (392 cu. in.) 	
Bore x Stroke	103.9 x 94.5 (4.09 x 3.72) (103.9 x 94.5)	

Valve System	Pushrod-operated overhead valves, 16 valves with sodium-filled exhaust valves and hollow stem intake valves, 16 conventional hydraulic lifters, all with roller tips 	
Fuel Injection	Sequential, multiport, electronic, returnless; automatic features Fuel Saver mode	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.9:1	
Power (estimated SAE net)	485 hp (362 kW) @ 6,100 rpm (75.8 hp/litre)	
Torque (estimated SAE net)	475 lb.-ft. (644 N•m) @ 4,100 rpm	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Premium 91 octane (R+M)/2 — recommended	
Oil Capacity	6.6 litres (7 quarts) 	
Factory Oil Fill	0W-40 Pennzoil Ultra synthetic	
Coolant Capacity	13.25 (14 quarts) 	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad-heated oxygen sensors and internal engine features	
Exhaust Type	Dual 6.9 cm (2.75-in.) straight-through exhaust system using twin electronic exhaust valves (EEV) with 10.1 cm (4-in.) chrome round tips	
Max. Gross Trailer Weight	Not rated for trailer-tow	
EnerGuide (2016) Fuel Consumption Ratings, L/100 km (MPG – imperial gallon) city/hwy/combined	15.7 (18) / 9.5 (30) / 12.9 (22) (RWD with 8HP70 eight-speed automatic transmission)	
	
ENGINE: 6.2-LITRE SUPERCHARGED HEMI SRT HELLCAT V-8	
Availability	Standard — Charger SRT Hellcat	
Type and Description	90-degree V-type, liquid-cooled	
Displacement	6,166 cu. cm (370 cu. in.) 	
Bore x Stroke	103.9 x 90.9 (4.09 x 3.58) 	
Valve System	Pushrod-operated overhead valves, 16 valves with sodium-filled exhaust valves and hollow stem intake valves, 16 conventional hydraulic lifters, all with roller tips	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, unique aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	9.5:1	
Power (SAE J2723)	707 hp (527 kW) at 6,200 rpm	
Torque (SAE J2723)	650 lb.-ft. (881 N•m) at 4,800 rpm	
Max. Engine Speed	6,200 rpm (electronically limited)	
Fuel Requirement	Premium 91 octane (R+M)/2 — recommended	
Oil Capacity	6.6 litres (7 quarts) 	
Factory Oil Fill 	0W-40 Pennzoil Ultra synthetic	
Coolant Capacity	13.25 (14 quarts) 	
Emission Controls 	Dual close-coupled three-way catalytic converters heated wide range upstream and switching downstream O2 sensors and internal engine features 	
Exhaust Type 	Dual 6.9 cm (2.75-in.) straight-thru exhaust system using twin electronic exhaust valves (EEV) with 10.1 (4-in.) chrome round tips	
EnerGuide (2016) Fuel Consumption Ratings, L/100 km (MPG – imperial gallon) city/hwy/combined	17.6 (16) / 10.7 (26) / 14.5 (23) (RWD with 8HP90 eight-speed automatic transmission)	
Assembly Plant	Saltillo, Mexico	
	
TRANSMISSION: 845RE TORQUEFLITE EIGHT-SPEED AUTOMATIC WITH AUTO/STICK™	
Availability	Standard — Charger SE (RWD/AWD) and SXT (RWD/AWD)	
Description	Adaptive electronic control, optional Sport mode or paddle-shifted driver-interactive manual control. Five clutch-pack design with only two open clutches in any gear. Off-centre line pump with low-viscosity oil for reduced spin loss. Torque converter lock with turbine torsional damper for low lock-up speeds in 1st through 8th gear  	
Gear Ratios		
1st	4.71	
2nd	3.14	
3rd	2.10	
4th	1.67	
5th	1.29	
6th 	1.00	
7th 	0.84	
8th 	0.67	
Reverse	3.30	
Overall Top Gear	Charger SE and SXT (RWD) — 2.62	
	Charger SE and SXT (AWD) — 3.07	
	Charger SE and SXT (RWD) — 1.78 	
		Charger SE and SXT (AWD) — 2.05	
		
TRANSMISSION: 8HP70 TORQUEFLITE EIGHT-SPEED AUTOMATIC WITH AUTO/STICK™	
Availability	Standard on Charger R/T, R/T Scat Pack and SRT 392	
Description	Adaptive electronic control with optional Sport mode or paddle-shifted driver-interactive manual control. (SRT: Adaptive electronic control with full manual control via gear selector or paddle shifters – with three SRT-unique selectable modes: Street, Sport and Track)	
	
Gear Ratios			
1st	4.714	
2nd	3.143	
3rd	2.106	
4th	1.667	
5th	1.285	
6th 	1.000	
7th 	0.839	
8th 	0.667	
Reverse	3.317	
Overall Top Gear	1.75 – R/T
2.07 – R/T Scat Pack, SRT 392 	
		
TRANSMISSION: 8HP90 TORQUEFLITE EIGHT-SPEED AUTOMATIC	
Availability	Standard on Charger SRT Hellcat	
Description	Adaptive electronic control with full manual control via gear selector or paddle shifters, with three SRT-unique selectable modes: Street, Sport and Track (features performance shifting and gear holding feature)	
Gear Ratios		
1st	4.714	
2nd	3.143	
3rd	2.106	
4th	1.667	
5th	1.285	
6th	1.000	
7th	0.839	
8th	0.667	
Reverse	3.317	
Final Drive Ratio	2.62 — Asymmetric-limited slip, performance-tuned	
Overall Top Gear	1.76	
		
TRANSFER CASE		
Availability	Standard — Charger SE and SXT AWD models	
Type	Active, fully variable with front-axle disconnect 	
Centre Differential	Planetary	
Torque Split, Front/Rear	Fully variable	
		
Electrical System		
Alternator	160-amp — standard on Charger SE 	
		180-amp — standard on Charger SXT and R/T	
		220-amp — standard on Charger R/T Scat Pack, SRT 392 and SRT Hellcat	
Battery		H7 Case, 730 CCA, maintenance-free	
		
Suspension		
Front 	Independent SLA with high upper “A” arm, coil spring over gas-charged monotube shock absorbers and stabilizer bar	
	Lateral and diagonal lower links with dual ball joint knuckles and sway bar	
	One piece lower-control arms — standard on Charger AWD models only	
Rear	Five-link independent with coil springs, gas-charged monotube shock absorbers, stabilizer bar and isolated suspension cradle 	
Touring-tuned Suspension 	Standard on Charger SE and SXT (RWD)	
AWD Touring-tuned Suspension 	Standard on Charger SE and SXT (AWD)	
Sport-tuned Suspension 	Standard on Charger R/T and optional on SXT	
Performance-tuned Suspension 	Standard on Charger R/T Scat Pack	
SRT-Tuned	SRT-tuned three-mode adaptive damping system with ADS Bilstein shock absorbers: Street mode = sporty, compliant ride; Sport mode = firm, improved handling; Track mode = firmest, maximum handling	
		
Steering		
Type	Rack and pinion with electric power assist	
Performance Steering Gear 	Standard on R/T Scat Pack and SRT 392	
		
Dimensions and Capacities		
Wheelbase	SE, SXT and R/T — 3,052 (120.2) 
R/T Scat Pack — 3,052 (120.2) 
SRT 392 — 3,058 (120.4) 
SRT Hellcat  — 3,058 (120.4) 	
Track, Front	SE, SXT and R/T — 1,610 (63.4) 
R/T Scat Pack — 1,610 (63.4) 	
Track, Rear

	SE, SXT and R/T — 1,620 (63.8) 
R/T Scat Pack — 1,602.7 (63.1)
SRT 392 — 1,618 (63.7) 
SRT Hellcat  — 1,618 (63.7) 	

Overall Length	SE, SXT and R/T — 5,040 (198.4)  	
	R/T Scat Pack — 5,100.3 (200.8)	
	SRT 392 — 5,100.3 (200.8)	
	SRT Hellcat  — 5,100.3 (200.8)	
Overall Width	1,905 (75.0) 	
Overall Height	SE, SXT and R/T — 1,510 (58.5) to shark fin antenna tip 	
	SE, SXT and R/T — 1,479 (58.2) to roof sheet metal	
	R/T Scat Pack — 1,480 (58.26)	
	SRT 392 — 1,480 (58.26) 	
	SRT Hellcat  — 1,480 (58.26)	
Frontal Area, sq. m (sq. ft.) 	SE, SXT and R/T — 2.39 (25.8) 	
	R/T Scat Pack — 2.4 (26.2)	
	SRT 392 — 2.4 (26.2)	
	SRT Hellcat  — 2.4 (26.2)	
Drag Coefficient (Cd)	SE, SXT and R/T — 0.304 	
	R/T Scat Pack — 0.335	
	SRT 392 — 0.335	
	SRT Hellcat  — 0.335	
Curb Weight, kg (lbs.)	SE (RWD) — 1,796.2 (3,960)  	
	SE (AWD) — 1,907.8 (4,206)	
	SXT (RWD) — 1,822.5 (4,018)	
	SXT (AWD) — 1,914.2 (4,220)	
	R/T  — 1941.3 (4,280)	
	R/T Scat Pack — 1,987.6 (4,395)	
	SRT 392 — 1,987.6 (4,382) 	
	SRT Hellcat  — 2,072.9 (4,570)	
Weight Distribution, percent F/R	SE (RWD) — 52/48	
	SE (AWD) — 53/47	
	SXT (RWD) — 52/48	
	SXT (RWD) — 52/48	
	SXT (AWD) — 54/46	
	R/T — 53/47	
	R/T Scat Pack — 55/45	
	SRT 392 — 55/45	
	SRT Hellcat  — 56/44	
Fuel Tank Capacity, litres 
(imperial gal.)	70 (15.4) 	
Accommodations		
Seating Capacity, F/R	2/3	
Front		
Headroom	981 (38.6) 
938.4 (36.9) with sunroof	
Legroom	1,061 (41.8) 	
Shoulder room	1,510 (59.5) 	
Hip room	1,428 (56.2) 	
Seat travel	Driver — 255 (10.0) 
Passenger — 220 (8.66) 	
Recliner angle range, deg.	Power — 70.7
Manual — 70	
EPA front row interior volume, litres 
(cu. ft.) 	1,574.4 (55.6) 	
Rear Seat		
Headroom	930.6 (36.6) 
930.6 (36.6) with sunroof	
Legroom	1,019 (40.1) 	
Knee clearance	99 (3.9) 	
Shoulder room	1,472 (57.9) 	
Hip room	1,425 (56.1) 	
EPA second row interior volume, 
litres (cu. ft.) 	1,393.1 (49.2) 	
Total Interior Volume, litres (cu. ft.)	2,964.7 (104.7) 	
EPA Luggage Compartment Volume, 
litres (cu. ft.)	467.2 (16.5) 	
EPA Interior Volume Index, l
itres (cu. ft.) 	3,420.6 (120.8) 	
Trunk Liftover Height	764.0 (30.1) 	
		
Tires		
Availability 	Standard — Charger SE 	
Size and type	P215/65R17 low rolling resistance 	
Mfr. and model	Michelin Energy Saver	
	
Availability
	Standard — Charger SXT 
Optional on Charger SE 	
Size and type	235/55R18 BSW All-season performance	
Mfr. and model		Michelin 	
		
Availability	Standard — Charger SE and SXT AWD 	
Size and type	P235/55R19 BSW All-season performance 	
Mfr. and model	Hankook Optimo	
		
Availability	Optional — Charger SXT AWD with Rallye Group	
Size and type	235/55R19 BSW All-season performance 	
Mfr. and model	Michelin Primacy MXM4	
		
Availability	Standard — Charger R/T 
Optional — Charger SE and SXT	
Size and type	245/45R20 BSW All-season performance	
Mfr. and model	Firestone Firehawk GTV	
		
Availability	Standard — R/T Scat Pack 
Available with Super Track Pak on SXT	
Size and type	245/45ZR20 BSW All-season performance 	
Mfr. and model	Goodyear RS-A	
		
Availability	Standard on SRT 392 and SRT Hellcat	
Size and type	275/40ZR20 All-Season	
Mfr. and model	Pirelli P Zero Nero All-Season	
		
Availability	Optional on SRT 392 and SRT Hellcat	
Size and type	275/40ZR20 summer tires 	
Mfr. and model	Pirelli P Zero	
		
WHEELS		
Availability	Standard on SE (RWD)	
Type and material	Five-spoke design, Satin Silver aluminum 	
Size	17 x 7.0	
	
Availability
	Standard on Charger SXT (RWD)
Optional on Charger SE (RWD) with Sport Appearance Group (fleet only)	
Type and material	Five-spoke design Satin Carbon aluminum 	
Size		18 x 7.5	
		
Availability	Standard on Charger SE (AWD) and SXT (AWD)	
Type and material	Five-spoke design, polished with Graphite painted pockets; Hyper Black painted finish on SXT with Rallye Appearance Group	
Size	19 x 7.5	
		
Availability	Optional on Charger SXT with Plus Group 	
Type and material	Five-spoke Satin Carbon aluminum 	
Size	20 x 8.0	
		
Availability	Standard on R/T; Optional on Charger SXT with Rallye Group	
Type and material	Hyper Black Aluminum	
Size	20 x 8.0	
		
Availability	Optional on Charger SXT and R/T with Premium Group 
Optional on Charger SE, SXT and R/T with Blacktop Appearance Package	
Type and material	Polished aluminum with black pockets and satin finish (Premium Group); 
Includes Gloss Black finish on SE, SXT and R/T with Blacktop Appearance Package 	
Size	20 x 8.0	
		
Availability	Optional on Charger R/T	
Type and material	“Classic” five-spoke polished aluminum	
Size	20 x 8.0	
		
Availability	Standard on Charger R/T Scat Pack	
Type and material	Polished aluminum with black pockets and satin finish	
Size	20 x 9.0	
		
Availability	Optional on Charger R/T Scat Pack	
Type and material	Lightweight forged aluminum, Hyper Black II finish 	
Size	20 x 9.0	
	
Availability 		Standard on SRT 392 		
Type and material	“Slingshot” split seven spoke, forged aluminum with Hyper Black finish	
Size	20 x 9.5	
	
Availability 		Standard on SRT Hellcat		
Type and material	Five-spoke Low-gloss Black lightweight aluminum 	
Size	20 x 9.5	
		
Availability	Optional on SRT Hellcat	
Type and material	“Slingshot” split seven spoke, forged aluminum with Brass Monkey Finish	
Size	20 x 9.5	
		
Brakes		
Touring Brake Package 	Standard on Charger SE and SXT RWD	
Front		
Rotor size and type	320 x 28 (12.6 x 1.1) vented	
Caliper size and type	60 (2.36) single-piston sliding with aluminum housing	
Swept area	1,358 sq. cm (210 sq. in.) 	
Rear		
Rotor size and type	320 x 10 (12.6 x 0.4)  solid	
Caliper size and type	42 (1.65) single-piston sliding with aluminum housing	
Swept area	1,703 sq. cm (264 sq. in.) 	
		
Sport Brake Package 	Standard on Charger SE AWD, SXT AWD and R/T 	
Front		
Rotor size and type	345 x 28 (13.6 x 1.26) vented	
Caliper size and type	42 (1.65) dual-piston sliding with aluminum housing	
Swept area	1,606 sq. cm (249 sq. in.) 	
Rear		
Rotor size and type	320 x 22 (12.6 x 0.87) vented	
Caliper size and type	42 (1.65) single-piston sliding with aluminum housing	
Swept area	1,703 sq. cm (264 sq. in.) 	
		
Brembo High-performance Brake Package 	Standard on Charger R/T Scat Pack	
Front				
Rotor size and type	360 x 32 (14.2 x 1.26) vented and slotted	
Caliper size and type	44 (1.73) Brembo four-piston fixed with aluminum housing	
Swept area	2,261 sq. cm (351 sq. in.) 	
	
Rear			
Rotor size and type	350 x 28 (13.8 x 1.10) vented and slotted	
Caliper size and type	32 (1.26) Brembo four-piston fixed with aluminum housing	
Swept area	2,036 (316 sq. in.) 	
		
Brembo Ultra-high Performance Brake Package 	Standard on Charger SRT 392 and SRT Hellcat	
Front		
Rotor size and type	390 x 34 (15.4 x 1.34) two-piece aluminum hat, vented and slotted	
Caliper size and type	36 (1.42) Brembo six-piston fixed monoblock aluminum	
Swept area	2,735 sq. cm (424 sq.in.) 	
Rear		
Rotor size and type	350 x 28 (13.8 x 1.10) vented and slotted	
Caliper size and type	32 (1.26)  Brembo four-piston fixed with aluminum housing	
Swept area	2,036 sq. cm (316 sq. in.)