FCA CANADA
2017 Dodge Durango
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

General Information		
Vehicle Type	Four-door sport-utility vehicle	
Assembly Plant	Jefferson Avenue North, Detroit, Mich., USA	
EPA Vehicle Class	Multipurpose vehicle 	
		
BODY AND CHASSIS		
Layout	Longitudinal front engine, transfer case with full-time all-wheel drive 	
Construction	Steel unibody	
	
Engine: 3.6-LitRE pentastar v6	
Availability	Standard — SXT, GT and Citadel (not available on R/T)	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	3,604 cu. cm (220 cu. in.)	
Bore x Stroke	 96 x 83 (3.78 x 3.27)	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads	
Compression Ratio	10.2:1	
Power (est.) (SAE J2723)	Single Exhaust - 293 hp @ 6400 rpm
Dual Exhaust - 295 hp @ 6400 rpm	
Torque (est.) (SAE J2723)	260 lb.-ft. (353 N•m) at 4,000 rpm (both single and dual exhaust)	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R + M)/2  	
Oil Capacity	5.7 litres (6.0 quarts) 	
Coolant Capacity	9.9 litres (10.4 quarts) without trailer tow
10.4 litres (11 quarts) with trailer tow	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors 
and internal engine features)	

EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	12.8 (22) / 9.5 (30)/11.3 (25)	
Based on 2016 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca	
Assembly Plant	Trenton, Mich., USA	
		
ENGINE: 5.7-LITRE HEMI® V8		
Availability	Standard — R/T and optional on GT and Citadel 	
Type and Description	90-degree V-type, liquid-cooled	
Displacement	5,654 cu. cm (345 cu. in.) 	
Bore x Stroke	99.5 x 90.9 (3.92 x 3.58) 	
Valve System	Variable-valve timing (VVT), pushrod-operated overhead valves, 
16 valves, eight deactivating and eight conventional hydraulic lifters, 
all with roller followers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, 
aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.5:1	
Power (est.) (SAE J2723)	360 hp (268 kW) at 5,150 rpm	
Torque (est.) (SAE J2723)	390 lb.-ft. (529 N•m) at 4,250 rpm	
Max. Engine Speed	5,800 rpm (electronically limited)	
Fuel Requirement	Unleaded mid-grade, 89 octane (R+M)/2—recommended;
unleaded regular, 87 octane (R+M)/2—acceptable	
Oil Capacity	6.6 litres (7 quarts) 	
Coolant Capacity	14.6 litres (15.4 quarts) without trailer tow
15.2 litres (16 quarts) with trailer tow	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad heated oxygen 
sensors and internal engine features	
EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	 16.7 (17) / 10.7 (26)/14.0 (20)	
Assembly Plant	Saltillo, Mexico	
	
TRANSMISSION: torqueflite EIGHT-SPEED automatic	
Availability	Standard — all models	
Description	Driver-interactive manual control via steering wheel paddle shifters and electronically modulated torque converter clutch	
Gear Ratios		
1st 	4.714	
2nd 	3.143	
3rd  	2.106	
4th 	1.667	
5th 	1.285	
6th	1.000	
7th	0.839	
8th	0.667	
Reverse 	3.295	
		
TRANSFER CASE: MP 3010 		
Availability	Standard with V6 engine and AWD	
Type	Single-speed	
Operating Mode	Full-time AWD	
Low Range Ratio	None	
Torque Split, Front/Rear	50/50	
		
TRANSFER CASE: MP 3023		
Availability	Standard with V8 engine and AWD	
Type	Two-speed, electronically shifted	
Operating Modes	AWD Low (Lock), Neutral; full-time active AWD	
Low Range Ratio	2.72	
Torque Split, Front/Rear	Variable	
		
Axles		
Front		
Differential Type	Conventional	
Availability	Standard on all models 	
Ring Gear Diameter	195 (7.7) 	
Axle Ratios	3.45:1 (V-6 AWD)  
3.09:1 (V-8)	
		
Rear		
Differential Type	Conventional	
Availability	Standard on all engines	
Ring Gear Diameter	195 (7.7) (V-6) 
9.1 (230) (V-8)	
Axle Ratios	3.45:1 (V-6)  
3.09:1 (V-8)	
		
Electrical System		
Alternator	160-amp; 180-amp or 220-amp depending on option content	
Battery	Maintenance-free 
H6 650 CCA + Auxiliary 200 CCA on Electronic Stop/Start (ESS) (V-6)
H7 700 CCA (V-8)	
		
Suspension		
Front	Short- and long-arm independent (SLA), coil springs, gas-charged, twin-tube coil-over shock absorbers, steel upper- and aluminum lower-control arms (“A” arms), aluminum knuckle, stabilizer bar	
Rear	Multi-link rear suspension, coil spring, twin tube shocks (including load leveling for towing), aluminum lower control arm, independent upper links (tension and camber) plus a separate toe link	
		
STEERING		
Type	Rack and pinion with electric power assist	
Steering Ratio	16.7 	
Lock-to-Lock Steering Wheel Rotations	3.2 	
		
BRAKES		
Type	Power-assisted, anti-lock braking system (ABS)	
Front		
Rotor size and type	330 x 32 (13.0 x 1.26) vented disc (V-6)
350 x 32 (13.8 x 1.26) vented disc (V-8)	
Caliper size and type	1.89 (48) two-piston pin-slider caliper	
Swept area, (sq. cm / sq. in.)	1,969 (305) (V-6) 
2,088 (324)  (V-8)	

Rear		
Rotor size and type	330 x 14 (13.0 x 0.55)  solid disc (V-6) 
330 x 22 (13.0 x 0.87)  vented disc (V-8)	
Caliper size and type	48 (1.89)  single-piston floating caliper	
Swept area, (sq. cm / sq. in.) 	1,658 (257) 	
		
Dimensions and Capacities		
Wheelbase	3,043 (119.8) 	
Track, Front	1,623 (63.9) 	
Track, Rear	1,628 (64.1) 	
Overall Length	5,110 (201.2) 	
Overall Width (Width at Mirrors)	2,172 (85.5) 	
Body Width	1,924 (75.8) 	
Overall Height (at Roof Rail / at Antenna)	1,801 (70.9)  / 1,847 (72.7) , R/T – 1,827  (71.9) 	
Load Floor Height	817 (32.2) , R/T – 797.6 (31.4) 	
Sill Step Height	521.5 (20.5) , R/T – 500.4 (19.7) 	
Ground Clearance (with P265/60R18 Tire and 3.6-litre engine)	207 (8.1) 	
Ground Clearance Chassis (Fuel Tank) 	254 (10.0) 	
Ground Clearance Front Axle	243.2 (9.6) 	
Ground Clearance Rear Axle	256 (10.1) 	
Approach Angle (degrees)	16.3 	
Ramp Breakover Angle (degrees)	18.1	
Departure Angle (degrees)	21.5 	
Frontal Area	2.88 (sq. m) 31.0 sq. ft. 	
Drag Coefficient 	0.35	
Fuel Tank Capacity	93.1 litres (24.6 gal.) 	
		
Accommodations		
Seating Capacity (front/second/third rows)	2/3 (standard), 2/2/2 with optional second-row captain’s chairs	
Front		
Headroom	1,013 (39.9)  	
Legroom	1,024 (40.3) 	
		
Shoulder Room	1,486 (58.5) 	
Hip Room	1,448 (57.0) 	
Seat Travel	280 (11.0) driver, 230 (9.0)  passenger	
SAE Front Volume Index, litres (cu. ft.)	1,540 (54.4 cu. ft.) 	
Second Row		
Headroom	1,011 (39.8) 	
Legroom	980 (38.6) 	
Shoulder Room	1,280 (50.4) 	
Hip Room 	1,087 (42.8) 	
SAE Volume, litres (cu. ft.)	1,268. 5 (44.8 cu. ft.) 	
Third Row 		
Headroom	960 (37.8) 	
Legroom	800 (31.5) 	
Shoulder Room	1,280 (50.4) 	
Hip Room 	1,087 (42.8) 	
SAE Volume	982.5 litres (34.7 cu. ft.) 	
SAE Cargo Volume		
Behind Third Row	487.0 litres (17.2 cu. ft.) 	
Behind Second Row	1350.7 litres (47.7 cu. ft.) 	
Behind Front-row Seats with 
Rear Seats Folded	2392.7 litres (84.5 cu. ft.) 	

WEIGHTS (Estimates)		
	MODEL	ENGINE	GVWR kg (lbs.)	CURB WEIGHT kg (lbs.)	PAYLOAD kg (lbs.)	
AWD	SXT 	3.6-litre	2,948 (6,500) 	2,229 (4,913) 	640 (1,410) 	
	GT	3.6-litre
5.7-litre	2,948 (6,500) 3,221 TBD	2,262 (4,987) 
TBD	645 (1,420) 
TBD	
	Citadel	3.6-litre
5.7-litre	3,221 (7,100) 
3,221 (7,100) 	2,312 (5,097) 
2,448 (5,397) 	615 (1,360) 
620 (1,370) 	
	R/T	5.7-litre	3,221 (7,100) 	2,418 (5,331) 	605 (1,340) 	
		
Wheels		
Availability	Standard — SXT 	
Type and Material	Painted machine cast-aluminum, 10-spoke Satin Carbon	
Size (inches)	18 x 8	
		
Availability	Standard — GT and Blacktop Package	
Type and Material	Polished machined cast-aluminum, 10-spoke
(Hyper Black on GT and Gloss Black on Blacktop Package)	
Size (inches)	20 x 8	
Availability	Standard — Brass Monkey Appearance Package available on GT and R/T 	
Type and Material	Painted machined cast-aluminum, 10-spoke 
(Burnished Bronze on Brass Monkey Appearance Package and Low Gloss Granite on R/T)	
Size (inches)	20 x 8	
		
Availability	Standard — Citadel and Anodized Platinum Appearance Package	
Type and Material	Polished (Satin Carbon on Anodized Platinum Appearance Package) machined cast-aluminum, 10-spoke 	
Size (inches)	20 x 8	
		
Tires		
Availability 	Standard — SXT 	
Size and Type	265/60R18	
Mfr. and Model	Michelin Black Premier LTX Sidewall All-season	
		
Availability 	Available — SXT and GT	
Size and Type	P265/60R18	
Mfr. and Model	Kumho Crugen Black Sidewall All-season	
		
Availability 	Standard — GT
Available — RT	
Size and Type	P265/50R20	
Mfr. and Model	Pirelli Scorpian Verde Black Sidewall Performance All-season	
		
Availability 	Standard — R/T and Citadel	
Size and Type	265/50R20	
Mfr. and Model	Bridgestone Ecopia H/L 422 Plus Black Sidewall All-season	

Parking Brake Type	Rear, mechanical, drum-in-hat	
Power Assist	Single-rate, tandem diaphragm vacuum	
Four–wheel Anti-lock Brakes	Standard	
Electronic stability control	Standard	
All-speed traction control	Standard	
Brake Assist	Standard	

TRAILER TOWING		
	Engine	Axle Ratio	Maximum Trailer Weight kg (lbs.)	
AWD 	3.6-litre V-6
5.7-litre V-8	3.45 
3.09	2,812 (6,200) 
3,265 (7,200)