FCA CANADA
2017 Dodge Journey
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

General Information		
Body Style	Four-door; five- or seven-passenger	
Assembly Plant	Toluca, Mexico	
EnerGuide Vehicle Class	Sport-utility vehicle	
	
BODY/CHASSIS	
Layout	Transverse front engine, front-wheel drive or all-wheel drive	
Construction	Steel unibody	
		
Engine: 2.4-litRE dohc 16-valve, DUAL vARIABLE vALVE tIMING, smpi i-4	
Availability	CVP and SE Plus	
Type and Description	Four cylinders in-line, tuned intake manifold with dual counter-rotating balance shafts and dual variable-valve timing	
Displacement	2,360 cu. cm (144 cu. in.) 	
Bore x Stroke	88 x 97 (3.46 x 3.82) 	
Compression Ratio	10.5:1	
Power (SAE net, estimated)	173 hp (129 kW) @ 6,000 rpm (71 hp/litre)	
Torque (SAE net, estimated)	166 lb.-ft. (225 N•m) @ 4,000 rpm	
Maximum Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity	4.26 litres (4.5 quarts) with filter SAE 5W-20	
Coolant Capacity	7.5 litres (7.9 quarts)— single-zone climate control 	
Emission Controls	Single catalytic converter, dual heated oxygen sensors 
and internal engine features	
EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	12.7/9.1/11.1 (22/31/25)	
Based on 2016 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca
	
Engine Assembly Plant	Dundee, Michigan, USA	
Engine: 3.6-litre dohc 24-valve, VARIABLE VALVE TIMING, V6	
Availability	SXT, Crossroad and GT	
Type and Description	60-degree bank angle, liquid-cooled, three-plenum intake manifold with electronically controlled manifold tuning valve and short-runner valves 	
Displacement	3,605 cu. cm (220 cu. in.) 	
Bore x Stroke	96 x 81 (3.78 x 3.19) 	
Compression Ratio	10.2:1	
Valve System	DOHC, 24 valves, hydraulic, center-pivot roller rocker arms 	
Fuel Injection	  Sequential, multiport, electronic 	
Power (SAE net, estimated)	283 hp (211 kW) @ 6,350 rpm (67.1 hp/litre)	
Torque (SAE net, estimated)	260 lb.-ft. (353 N•m) @ 4,400 rpm 	
Maximum Engine Speed	6,800 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2 
Ethanol E85	
Oil Capacity	5.2 litres (5.5 quarts) with filter  SAE 10W-30 MAF 	
Coolant Capacity	10 litres (10.6 quarts)— single- or dual-zone climate control 
11 litres (11.6 quarts)— tri-zone climate control 	
Emission Controls	Three-way catalytic converter, electronic EGR, 
and internal engine features	
EnerGuide Fuel Consumption Ratings 
L/100 km (MPG – imperial gallon) city/hwy/combined	14.2/9.4/12.1 (20/30/23) – FWD
14.5/9.9/12.4 (19/29/23) – AWD 	
Engine Assembly Plant	Trenton, Michigan, USA	
	
Transmission: 40TES Automatic four-speed overdrive	
Availability	CVP and SE Plus 	
Description	Four-speed overdrive, adaptive electronic control, 
electronically modulated converter clutch	
Gear Ratios		
1st	2.842	
2nd	1.57	
3rd	1.0	
4th	0.69	
Reverse	2.21	
Final-drive Ratio	4.28	
Overall Top-gear	2.95	
	
Transmission: 62te/62tea Automatic six-speed overdrive	
Availability	SXT, Crossroad and GT	
Description	Six-speed, adaptive electronic control and electronically 
modulated torque converter clutch	
Gear Ratios		
1st	4.127	
2nd	2.842	
3rd	2.283	
4th	1.452 — Upshift 
1.570 — WOT kickdown		
5th	1.00	
6th	0.690	
Reverse	3.214	
Transfer Ratio	0.95	
Final-drive Ratio	3.16	
Overall Top-gear	2.06	
	
Drivetrain 	
Front-wheel-drive		
Availability	CVP and SE Plus	
All-wheel-drive		
Availability	Crossroad and GT with 3.6-litre V-6	
Type	Electronically controlled coupling (ECC) with variable torque output	
Rear Differential	Open	
	
Electrical System	
Alternator	160-amp — Standard on all Journey models	
Battery	525-amp maintenance-free	
	
Suspension	
Front	Independent MacPherson strut, coil spring over gas-charged shock absorbers, stabilizer bar with isolated suspension cradle	
Rear	Multi-link independent with coil springs, link-type stabilizer bar, 
gas-charged shock absorbers and isolated rear suspension cradle	
	
STEERING	
Type	Power rack and pinion	
Overall Ratio	16.45	
Turning Diameter (curb-to-curb) metres (ft.)	11.7 (38.5)  — 17-in. wheels and tires 
11.9 (39.0)  — 19-in. wheels and tires 		
Steering Turns (lock-to-lock)	2.92	
P/S pump	Hydraulic	
	
BRAKES	
Front		
Rotor size and type	330 x 28 (13.0 x 1.1)  vented rotor	
Caliper size and type	51.0 (2.0)  two-piston floating caliper	
Swept area, sq. cm (sq in.)	475 (73.6) 	
Rear		
Rotor size and type	328 x 12 (12.9 x 0.47) solid rotor	
Caliper size and type	45.0 (1.8)  single-piston floating caliper	
Swept area, sq. cm (sq. in.)	429 (66.5) 	
	
Dimensions and Capacities	
Wheelbase	2,889.8 (113.8) 	
Overhang — Front	989.3 (38.9)	
Overhang — Rear	1008.5 (39.7) 	
Track — Front	1,570.8 (61.8) 	
Track — Rear	1,581.8 (62.3) 	
Overall Length	4,887.6 (192.4) 	
Overall Width	1,834.5 (72.2) 	
Overall Width with Mirrors 	2,127.0 (83.7) 	
Overall Height	1,692.6 (66.6) 	
Vehicle Height including Roof Rack Assembly	1,765.2 (69.5) 	
Drag Coefficient (Cd)	0.368	
Fuel Tank Capacity, litres (imperial gal.)	2.4-litre and 3.6-litre FWD — 77.6 (17) 
3.6-litre AWD — 79.8 (17.6) 	
Gross Vehicle Weight Rating (GVWR), kg (lbs.) 		
Five-passenger vehicle, FWD 2.4-litre	2,270 (5,005) 	
Seven-passenger vehicle, FWD 2.4-litre	2,404 (5,300) 	
Five-passenger vehicle, FWD 3.6-litre	2,313 (5,100) 	
Seven-passenger vehicle, FWD 3.6-litre	2,472 (5,450) 	
Five-passenger vehicle, AWD 3.6-litre	2,540 (5,600)	
Seven-passenger vehicle, AWD 3.6-litre	2,540 (5,600) 	
Towing Capabilities, kg (lbs.) 		
2.4-litre I-4 with Automatic Transaxle	450 (1,000) 	
3.6-litre V-6 with Automatic Transaxle, FWD or AWD	1,134 (2,500) 	
Curb Weight, Five-passenger Vehicle, Automatic Transaxle, kg (lbs.)		
2.4-litre I-4 Engine	FWD — 1,732 (3,818) 	
3.6-litre V-6 Engine	FWD — 1,839 (4,054) 
AWD — 1,922 (4,238) 		
	
Accommodations	
Seating Capacity (front/second/third rows)	2/3 standard, 2/3/2 optional	
EPA Volume Index, litres (cu. ft.)	3,794 (133.9) – seven-passenger 
3,810 (134.5) – five-passenger	
Total Interior Passenger Compartment Volume, litres (cu. ft.)	3,503 (123.701) – seven-passenger 
2,820.3 (99.6) – five-passenger	
Front row		
Headroom without Sunroof	1,036.3 (40.8) 	
Headroom with Sunroof	995.0 (39.2) 	
Legroom	1,036.3 (40.8) 	
Shoulder Room	1,459.7 (57.5) 	
Hip Room	1,366.5 (53.8) 	
Seat Travel	260 (10.23) 	
Front Compartment Volume, litres (cu. ft)	1,568.5 (55.39) 	

Second row		
Headroom without Sunroof	1,013.0 (39.9) 	
Headroom with Sunroof	994.8 (39.2) 	
Legroom	916.7 (36.1) 	
Couple, First to Second Row	773.8 (30.5) 	
Shoulder Room	1,444.4 (56.9) 	
Hip Room	1,381.9 (54.4) 	
EPA Rear Seat Volume Index or Third row Volume, litres (cu. ft.) 	1,248.7 (44.1) 	
Third row 		
Headroom	957.4 (37.7) 	
Legroom	595.5 (23.4) 	
Couple, Second to Third Row	765.1 (30.1) 	
Shoulder Room	1,104.9 (43.5) 	
Hip Room	1,016.3 (40.0) 	
Rear Passenger Volume, litres (cu. ft.)	628.6 (22.2) 	
Cargo Width at Wheelhouse	1,050.5 (41.4) 	
Trunk Liftover Height	782.4 (30.8) 	
Cargo Volume		
Behind First-Row Seat, litres (cu. ft.)	1,914.2 (67.6) 	
Behind Second-Row Seat, litres (cu. ft.) (five-passenger vehicles)	1,121.6 (39.61) 	
Behind Second-Row Seat, litres (cu. ft.) (seven-passenger vehicles)	1,047.7 (37.0) 	
Behind Third-Row Seat, litres (cu. ft.)	302.9 (10.7) 	
	
Wheels	
Availability	Available – CVP 	
Type and Material	Steel with wheel covers 	
Size	17 x 6.5	
		
Availability	Standard – CVP and SE Plus	
Type and Material	Machined cast-aluminum, five-spoke	
Size	17 x 6.5	
	
Availability		Standard — SXT		
Type and Material	Machined cast-aluminum, twin five-spoke	
Size	17 x 6.5	
		
Availability	Standard — GT
Optional — SXT		
Type and Material	Machined cast-aluminum, 10-spoke Tech Silver 
or Gloss Black finish (SXT with Blacktop Appearance Package)	
Size	19 x 7.0	
	
Availability		Standard — Crossroad		
Type and Material	Machined cast-aluminum, five-spoke Hyper Black finish 	
Size	19 x 7.0	
		
Availability	Optional — GT	
Type and Material	Chrome-clad cast-aluminum, six-spoke	
Size	19 x 7.0	
		
Availability	Available — all models	
Type and Material		Temporary spare steel wheel	
		
Tires	
Availability	Standard — CVP, SE Plus and SXT 	
Size and Type	P225/65R17, All-season Touring	
Model	Kumho Solus KH16	
		
Availability	Standard — Crossroad and GT
Available – SXT 	
Size and Type	225/55R19, All-season Touring	
Model	Kumho Solus KH16	
		
Availability	Optional — all Journey models	
Size and Type	T145/70R17 temporary spare tire	

Parking Brake Type	Standard — all Journey models		
Power-assist Type	230 x 230 (9 x 9)  tandem-diaphragm vacuum	
Four–wheel Anti-lock Brakes	Standard	
Electronic Stability Control	Standard	
All-speed Traction Control	Standard	
Brake Assist	Standard