FCA CANADA
2017 Dodge Viper
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Vehicle Type	Coupe 	
Assembly Plant	Conner Avenue, Detroit, Michigan, USA	
EPA Vehicle Class	Two-seater	
Introduction Date	Third quarter 2016 as 2017 model 	
	
BODY AND CHASSIS	
Layout	Longitudinal mid-front engine, rear-wheel drive (RWD)	
Construction	Backbone tubular steel space frame with magnesium cowl structure. Carbon fiber clamshell hood, roof, and liftgate assemblies. Aluminum doors and sills. RIM quarter panels and fascias.  	
	
ENGINE: 8.4-LITRE V10		
Type and Description	10-cylinder, 90-degree V-type, liquid-cooled 	
Displacement, litre (cu.in.) 	512 (8.4) 	
Bore x Stroke	103 x 100.6 (4.055 x 3.96) 	
Flywheel	Low-inertia aluminum with steel wear surface	
Intake	Three-piece shell molded, vibration-welded composite for improved flow, reduced weight and improved thermal performance	
Valve System	Overhead valve, variable-valve timing (VVT), 20 valves, roller-type hydraulic lifters	
Fuel Injection	Sequential, multiport, electronic	
Construction	Aluminum-alloy block with cast-iron liners, forged-aluminum pistons, forged-steel crankshaft, aluminum-alloy heads	
Compression Ratio	10.2:1	
Power (SAE net)	645 bhp (481 kW) @ 6,200 rpm (77 bhp/litre) 	
Torque (SAE net)	600 lb-ff (814 N•m) @ 5,000 rpm	
Max. Engine Speed	6,400 rpm (fuel cutoff)	
Fuel Requirement	Unleaded premium — 91 octane (R+M)/2	
Oil Capacity (with Filters)	10.4 litres (11 quarts) 	
Coolant Capacity	15 litres (16 quarts) 	
Emission Controls	Four three-way catalytic converters, heated oxygen sensors, engine internal features	
EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy	19. 2 (15) / 11.3 (25)	
Based on 2016 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca
	
ELECTRICAL SYSTEM	
Alternator	180-amp high-speed	
Battery	Leak-resistant, maintenance-free, 590 CCA (Standard)
Lightweight, leak-resistant, maintenance-free, 520 CCA (ACR)	

TRANSMISSION: MANUAL SIX-SPEED OVERDRIVE	
Description	Synchronized in all gears, electronic 1-4 skip-shift and reverse lockout mechanisms	
Gear Ratios		
1st	2.26	
2nd 	1.58	
3rd	1.19	
4th	1.00  	
5th 	0.77	
6th	0.50 	
Axle Ratio	3.55	
Overall Top-gear	1.78 	
		
FINAL DRIVE		
Description	Frame-mounted hypoid bevel gear with GKN ViscoLok speed-sensing limited-slip differential; 3.55:1	
		
SUSPENSION		
Type	All models: four-wheel independent with high-performance aluminum control arms and knuckles and lightweight coil-over shock absorbers 	
	GTC and GTS models: two-mode, driver selectable Bilstein DampTronic shock absorbers	
	TA 2.0 model: unique two-mode, driver selectable Bilstein DampTronic shock absorbers and springs	
	ACR model: 10-setting, double-adjustable, coil-over Bilstein racing shocks with unique spring rates	
Front	Cast-aluminum unequal-length upper and lower “A” arms, coil springs, 
low-pressure gas-charged shock absorbers, stabilizer bar	
Rear	Cast-aluminum unequal-length upper and lower “A” arms, toe-control links, coil springs, low-pressure gas-charged shock absorbers, stabilizer bar	

		GTC and GTS  	TA 1.0 / TA 2.0	ACR	
X-brace Weight kg (lb)		2.7 (6.0) (1.4 (3.1) optional carbon GTC only)	1.4 (3.1)	2.7 (6 0) (1.4 (3.1) optional carbon)	
Spring Rates (lb/in)			
Front		220	240	600	
Rear		550	600	1300	
Sway Bar Weight kg (lb)			
Front		4.5 (10)	7.7 (17)	7.7 (17)	
Rear		4.5 (10)	7.7 (17)	7.7 (17)	
Sway Bar Stiffness (N/MM)			
Front		50.9  	68.9	68.9	
Rear		35.4	46.5	46.5	
Alignment (deg.)			
Camber: front		-1.4	-2.5	-2.8	
Camber: rear		-1.15	-1.5	-1.7	
Caster: front		6.6	6.3	6.0	
Caster: rear		0.7 	0.7	0.7	
Total toe: front		0.14	0.14 	0.14	
Total toe: rear		0.24 	0.24	0.24	
	
STEERING		
Type	Power-assisted rack-and-pinion	
Overall Ratio	16.7:1	
Turning Diameter (curb-to-curb), 
m (ft)	12.34 (40.5) 	
Steering Turns (lock-to-lock)	2.4	
		
BRAKES		
Front	Standard — GTS  	
Size and Type	355.0 x 32.0 (14.0 x 1.26) curved fin vented StopTech two-piece slotted rotors with Brembo 44/40 opposing piston calipers	
Rear 	Standard — GTS 	
Size and Type	355.0 x 32.0 (14.0 x 1.26) curved fin vented StopTech two-piece slotted rotors with Brembo 42/38 dual opposing calipers	
Power-assist Type	Tandem diaphragm vacuum with zero lost travel	
		
Front 	Available — TA 1.0 and 2.0, and with optional ACR Package on GTC models	
Size and Type 	355.0 x 32.0 (14.0 x 1.26) (unique Brembo slotted, vented high thermal capacity two-piece wide annulus rotors and pads with Brembo 44/40 opposing piston anodized calipers with orange Viper logo	
Rear 	Available — TA 1.0 and 2.0, and with optional ACR package on GTC models	
Size and Type 	355.0 x 32.0 (14.0 x 1.26) unique Brembo slotted, vented high thermal capacity two-piece wide annulus rotors and pads) with Brembo 42/38 dual opposing anodized calipers with orange Viper logo	
Power-assist Type 	Booster with revised response; tandem diaphragm vacuum with zero lost travel 	
		
Front 	Standard — ACR
Available on GTC (must have ACR Package)  	
Size and Type 	390.0 x 34.0 (15.4 x 1.3) Brembo Carbon Ceramic Matrix with Brembo 6 piston calipers	
Rear 	Standard — ACR	
Size and Type 	360.0 x 32.0 (14.2 x 1.25) Brembo Carbon Ceramic Matrix with Brembo 4 piston calipers	
Power-assist Type 	Booster with revised response (same as TA); tandem diaphragm vacuum with zero lost travel	

	GTS	TA 1.0 / TA 2.0	ACR	
Rotor OD (mm)	355  	355	390	
Rub Surface ID (mm)	245	226	226	
Width (mm)	32 	32	34	
Swept Area per Rotor (cm2)	1,036	1,176	1,587	
Rotor Weight kg (lb)	8.1 (18)	10.2 (22.6)	6.0 (13.4)	
	
Stability Control/Traction Control	GTS: five-mode with launch control (Full-on, Sport, Track, Rain 
and Full-off) (included in TA 1.0 and 2.0 - and ACR with unique tuning)	
Launch Control 		Engine only controlled wheel slip with control button on steering wheel 
(standard in all models)	
		
DIMENSIONS AND CAPACITIES	
Wheelbase	2,510 (98.8) 	
Track, Front	1,598 (62.9) 	
Track, Rear	1,550 (61.0) 	
Overall Length	4,463 (175.7) 	
Overall Width 	1,941 (76.4) 	
Overall Height	1,246 (49.1) 	
Ground Clearance	127 (5.0) 	
Approach angle, degrees 	12.7 base, 9.0 ACR Extreme Aero	
Departure angle, degrees	16.2 base, 12.9 ACR Extreme Aero	
Curb Weight, kg (lb)  	1,549 (3,415) – Viper GTS model	
	1,541 (3,399) – Viper GTS model with lightweight Sidewinder II wheels
1,539 (3,392) – Viper ACR model with Extreme Aero		
	1,549 (3,415) – Viper GTS model	
Weight Distribution, percent F/R	49.6/50.4	
Drag Coefficient, Cd	0.369 GTS, 0.433 TA 1.0 and TA 2.0, 0.544 ACR, 0.541 ACR Extreme	
Fuel-Tank Capacity, litres (imperial gallons)	61 (13.4) 	
	
ACCOMMODATIONS 		
Seating Capacity	2	
Head Room	930.2 (36.62) 	
Leg Room	1,085.2 (42.72) 	
Shoulder Room	1,347.9 (53.07)  	
Cargo space, cu. ft. 	14.65	
Seat Travel	200 (7.87) : fore/aft
40 (1.57) : up/down		
Seat back recliner range, degrees 	30   	
		
TIRES		
Front	Standard 	
Size and Type	P295/30ZR18	
Manufacturer and Model	Pirelli P Zero with low-pressure sensors in valve stems 	
Revs per Mile (rpm)	835 	
Rear 	Standard 	
Size and Type	P355/30ZR19 	
Manufacturer and Model	Pirelli P Zero with low-pressure sensors in valve stems 	
Revs per Mile (rpm)	764 	
Front 	Available — must have optional lightweight Sidewinder II wheels (standard with TA 1.0 and 2.0)	
Size and Type	P295/30ZR18	
Manufacturer and Model	Pirelli P Zero Corsa with low-pressure sensors in valve stems 	
Revs per Mile (rpm)	835 	
Rear 	Available — must have optional lightweight Sidewinder II wheels (standard with TA 1.0 and 2.0)	
Size and Type	P355/30ZR19 	
Manufacturer and Model	Pirelli P Zero Corsa with low-pressure sensors in valve stems	
Revs per Mile (rpm)	764	
Front 	Standard on ACR 	
Size and Type	295/25R19	
Manufacturer and Model	Kumho Ecsta V720 with low-pressure sensors in valve stems	
Revs per Mile (rpm)	824	
Rear 	Standard on ACR 	
Size and Type	355/30R19	
Manufacturer and Model	Kumho Ecsta V720 with low-pressure sensors in valve stems	
Revs per Mile (rpm)	743	
		
WHEELS		
Type and Material 	Forged aluminum	
Size		
Front	18.0 x 10.5 base, 19.0 x 11.0 ACR	
Rear	19.0 x 13.0 	
Styles	Five-spoke “Rattler” polished aluminum (standard on GTC; optional on GTS)	
	Five-spoke “Rattler” painted aluminum – Hyper Black finish (optional on GTS)	
	Five-spoke “Rattler” painted aluminum – Matte Black finish (optional on GTS)	
	Five-spoke “Rattler” painted aluminum – Black Vapor Chrome finish (optional on GTC and GTS)	
	Split-six spoke “Venom” polished face aluminum – (optional on GTC, standard on GTS)	
	Split-six spoke “Venom” painted aluminum – Hyper Black finish (optional on GTC and GTS)	
	Split-six spoke “Venom” painted aluminum – Matte Black (optional on GTC and GTS)	
	Multi-spoke ultra-lightweight “Sidewinder II” – Hyper Black finish (optional on GTS)	
	Multi-spoke ultra-lightweight “Sidewinder II” – Matte Black finish (optional on GTS)	
	ACR painted forged aluminum – Gloss Black finish (standard on ACR)	
	ACR painted forged aluminum – Brass Monkey finish (optional on ACR)