FCA CANADA
2017 Fiat 500L
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Vehicle Type	B-segment multipurpose vehicle (MPV)	
EPA Vehicle Class	Small Station Wagon	
Assembly Plant	Kragujevac, Serbia	
	
BODY AND CHASSIS	
Layout	Transverse-mounted front engine, front-wheel drive	
Construction	Unitized steel body 	
	
ENGINE: 1.4-LITRE SOHC 16-VALVE TURBOCHARGED MULTIAIR INLINE FOUR-CYLINDER	
Availability	Standard — all 500L models	
Type and Description	Inline four-cylinder, liquid-cooled, turbocharged	
Displacement	1,368 cu. cm (83.48 cu. in.) 	
Bore x Stroke	72 x 84 (2.83 x 3.31) 	
Valve System	Belt-driven, MultiAir, SOHC, 16 valves, hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Cast-iron block with aluminum-alloy head and aluminum-alloy bedplate	
Compression Ratio	9.8:1	
Maximum Turbo Boost (psi / bar)	21 psi / 1.45 bar	
Power (SAE)	160 hp  @ 5,500 rpm	
Torque (SAE)	184 lb.-ft. @ 2,500-4,000 rpm	
Max. Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	87 octane (R+M)/2 acceptable 
91 octane recommended		
Oil Capacity	3.8 litres (4.0 quarts)  with dry filter	
Coolant Capacity	4.4 litres (4.6 quarts) 	
Emission Controls 	Three-way catalytic converters, heated oxygen sensors and internal engine features	
Max. Gross Trailer Weight	Not rated for trailer tow	

EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	10.6 (27) / 7.8 (36) / 9.4 (30) 	
Based on 2016 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca 
	
Engine Assembly Plant	Termoli, Italy	
		
AISIN SIX-SPEED AUTOMATIC TRANSMISSION	
Availability	Standard — all 500L models	
Gear Ratios		
1st	4.04	
2nd	2.37	
3rd	1.56	
4th	1.16	
5th	0.85	
6th	0.67	
Reverse	3.19	
Final-drive Ratio	3.683	
Overall Top Gear	2.47	
Steering Turns (lock-to-lock)	3.0	
		
BRAKES		
Availability	Standard — all 500L models	
Front		
Rotor size and type	305 x 28 (12.0 x 1.10)  vented	
Caliper size and type	57 (2.24)  single-piston with cast iron	
Swept area	876.1 sq. cm (345 sq. in.) 	
Rear		
Rotor size and type	264 x 10 (10.4 x 0.4)  solid	
Caliper size and type	38 (1.49) single-piston with aluminum housing	
Swept area	591.8 sq. cm (233 sq. in.) 	

DIMENSIONS AND CAPACITIES(a)		
Wheelbase	2,612 (102.8)	
Track, Front	1,502 (59.1) 	
Track, Rear	1,510 (59.4) 	
Overall Length	4,249 (167.3) 
4,270 (168.1)  — 500L Trekking	
Overall Width	1,774 (69.8) — without mirrors 
2,036 (80.2)  — with mirrors
1,800 (70.9)   — 500L Trekking	
Overall Height	1,670 (65.7) 	
Ground Clearance	120 (4.7) 	
Drag Coefficient (Cd) (estimated)	0.310 — 500L Sport/Lounge
0.320 — 500L Trekking		
Curb Weight, kg (lbs.) (estimated)	1,476 (3,254) 	
Weight Distribution, percent F/R	60/40 	
Fuel Tank Capacity, litres (gallons)	50 (13.2)	
(a) All dimensions measured at curb weight with standard tires.	
		
ACCOMMODATIONS		
Seating Capacity, F/R	2/3	
Front Seat		
Headroom	1,034 (40.7) 
1,028 (40.5)  with dual-pane sunroof		
Legroom	1.015 (40.0) 	
Shoulder room	1,456 (57.3) 	
Hip room	1.394 (54.9) 	
Total seat travel	211 (8.3) — driver
229 (9.0) — passenger 		
EPA front row interior volume	1,529 litres (54.0 cu. ft.)	
Rear Seat		
Headroom	983 (38.7)
966 (38.0) with dual-pane sunroof		
Legroom	931 (36.7) 	
Shoulder room	1,388 (54.6) 	
Hip room	1,256 (49.4) 	
Total seat travel	120 (4.7) 	
EPA second row interior volume	1,268 litres (44.8 cu. ft.) 	
Total Interior Volume	2,797 litres (98.8 cu. ft.) 	
EPA Luggage Compartment Volume	633 litres (22.4 cu. ft.)	
EPA Volume behind front row (max. cargo)	1,927 litres (68.0 cu. ft.) 	
EPA Interior Volume Index	3,429 litres (121.1 cu. ft.) 	
Trunk Liftover Height	657 (25.9) 	
		
TIRES		
Availability 	Standard — 500L Sport and Lounge	
Size and Type	205/55R16 BSW All-season 	
Mfr. and Model	Continental Conti ProContact or Goodyear Eagle LS2 or Nexen CP671 Classe Premiere	
Revs per kilometre (mile)	519 (836) 	
		
Availability	Standard — 500L Trekking ; available on 500L Lounge		
Size and Type	225/45R17 BSW All-Season	
Mfr. and Model	Continental Conti ProContact or Goodyear Eagle LS2 or Nexen CP671 Classe Premiere	
Revs per kilometre (mile)	517 (832)