FCA CANADA
2017 Fiat 500X
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Body Style 	Crossover	
Assembly Plant	Melfi, Italy	
EPA Vehicle Class 	Multipurpose vehicle	
	
BODY AND CHASSIS	
Layout	Transverse front engine	
Construction 	Steel uniframe	

ENGINE: 1.4-LITRE TURBOCHARGED MULTIAIR I-4	
Availability	Standard — Pop FWD, Sport FWD and Trekking FWD	
Type and Description	In-line four-cylinder, liquid-cooled, turbocharged	
Displacement	1,368 cu. cm (83.48 cu. in.) 	
Bore x Stroke	72.0 x 84.0 (2.83 x 3.31) 	
Valve System	Belt-driven, MultiAir, SOHC, 16 valves, hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Cast-iron block with aluminum-alloy head and aluminum-alloy bedplate	
Compression Ratio	9.8:1	
Maximum Turbo Boost (psi / bar)	22 psi / 2.49 bar	
Power (SAE)	160 hp @ 5,500 rpm	
Torque (SAE)	184 lb.-ft. @ 2,500-4,000 rpm	
Max. Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	87 octane (R+M)/2 acceptable 
91 octane recommended		
Oil Capacity	3.8 litres (4.0 quarts) with dry filter	
Coolant Capacity	5.2 litres (5.5 quarts)	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors and internal engine features	
	
EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined 	9.5 (30)/6.9 (41)/8.3 (34)
	
Based on 2016 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca
	
Towing	Not recommended 	
Engine Assembly Plant	Termoli, Italy	
		
ENGINE: 2.4-LITRE MULTIAIR2 TIGERSHARK 	
Availability	Standard —Sport AWD, Trekking AWD , Lounge FWD & AWD
Available — Pop FWD, Sport FWD and Trekking FWD	
Type and Description	In-line four-cylinder, 16-valve MultiAir with multiport fuel injection	
Displacement	2,360 cu. cm (144 cu. in.) 	
Bore x Stroke	88 X 97 (3.46 X 3.82)	
Valve System	SOHC, four valves per cylinder 	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum block, aluminum cylinder head	
Compression Ratio	10:1	
Power (SAE net) 	180 hp @ 6,400 rpm	
Torque (SAE net) 	175 lb.-ft. @ 3,900 rpm	
Max. Engine Speed	6,400 rpm	
Fuel Requirement	Unleaded regular, 87 octane	
Oil Capacity	5.2 litres (5.5 quarts) (total)	
Coolant Capacity	6.45 litres (6.8 quarts) 	
Emission Controls	Single catalytic converter, heated wide band lambda sensor upstream and 
mid-catalyst heated oxygen sensor	
EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	10.6 (27)/7.6 (37)/9.3 (30) (FWD)
11.0 (26)/7.9 (36)/9.6 (29) (AWD)	
Towing	454 kg (1,000 lbs.)  (not recommended for FWD)	
Engine Assembly Plant 	Dundee, Mich., USA	
		
TRANSMISSION: 948TE NINE-SPEED AUTOMATIC	
Availability	2.4-litre MultiAir2 Tigershark engine (FWD or AWD)	
Description 	Planetary gear train, transverse layout	
Ratio Spread	9.81	
	
Gear Ratios			
1st	4.71	
2nd	2.84	
3rd	1.91	
4th	1.38	
5th	1.00	
6th	0.81	
7th	0.70	
8th	0.58	
9th	0.48	
Reverse	3.83	
Axle Ratio	3.734	
		
C635 SIX-SPEED MANUAL TRANSMISSION	
Availability	1.4-litre MultiAir Turbo engine 	
Description	1st, 2nd, 3rd gear: Triple cone 	
	4th: Double cone	
Gear Ratios		
1st	4.154	
2nd	2.118	
3rd	1.361	
4th	0.978	
5th	0.756	
6th	0.622	
Reverse	4.00	
Final-drive Ratio	4.438 	
Overall Top Gear	2.38	
Axle Ratio	4.438	
		
ELECTRICAL SYSTEM		
Alternator 	150-amp (1.4-litre MultiAir Turbo) 
160-amp (2.4-litre Tigershark with MultiAir2) 		
Battery	500-amp  (1.4-litre MultiAir Turbo)
600-amp (2.4-litre Tigershark with MultiAir2) 		
SUSPENSION		
Front 	MacPherson strut, coil springs, high-strength steel front cross member, high-strength steel mono shell lower control arms, stabilizer bar	
Rear	Chapman strut, high-strength steel links, isolated steel rear cradle, coil springs, stabilizer bar	
		
STEERING		
Type 	Electric power rack and pinion	
Overall Ratio 	15.7 	
Turning Diameter (curb-to-curb) 	11.07 (36.3) 	
Steering Turns (lock-to-lock)	2.68 	
		
BRAKES		
Front		
Size and Type	305 x 28 (12 x 1.1)  vented rotor with 60 (2.36)  single-piston floating caliper	
Swept Area (per caliper)	895.3 sq. cm (138.77 sq. in.) 1 x 60	
Rear		
Size and Type 	278 x 12 (10.95 x 0.47) solid rotor with 38 (1.5) single-piston floating caliper	
Swept Area (per caliper)	656.4 sq. cm (101.7 sq. in.) (), 1 x 38	
Power-assist Type 	254 (10 in.) vacuum assist 	
Four-wheel anti-lock brake system (ABS)	Standard	
Electronic stability control (ESC)	Standard	
Parking Brake Type	Electric motor on caliper	
		
DIMENSIONS AND CAPACITIES		
Wheelbase	2,570 (101.2) 	
Track, Front	1,548 (60.9) front-wheel-drive	
	1,543 (60.7) all-wheel-drive	
Track, Rear	1,549 (61.0) front-wheel-drive	
	1,543 (60.7) all-wheel-drive	
Overall Length	4,248 (167.2) Pop, Lounge 	
	4,273 (168.2) Trekking	
Overall Width	1,796 (75.5) with mirrors folded	
	2,025 (79.7) 	
Overall Height 	1,602 (63.1) front-wheel-drive
1,617 (63.7) all-wheel-drive		
Load-floor Height	758 (29.8) 	
Sill-step Height	494 (19.4) front, 497 (19.6) rear 	
Ground Clearance	178 (7.0) front-wheel-drive
202 (7.9) all-wheel-drive		
Curb Weight, kg (lbs.)	1,356 (2,989)  manual transmission
1,417 (3,124)  automatic transmission, front-wheel-drive
1,499 (3,305)  automatic transmission, all-wheel-drive		
Aero Cd	0.350	
Fuel-tank Capacity, litres (imp.gallons)	48 (10.6) 	
	
ACCOMMODATIONS		
Seating Capacity — F/R	2/3	
Front Row		
Headroom	993 (39.1) 	
Legroom	1.053 (41.4) 	
Shoulder Room 	1,380 (54.3) 	
Hip Room	1,354 (53.3) 	
Seat Travel 	230 (9.0) driver / 260 (10.2) front passenger	
Recliner Range (degrees)	From 25 nominal, 38 forward and 30 rearward (from vertical 13 forward, 
55 rearward)	
First Row Interior Volume (standard roof), litres (cu.ft)	1,458 (51.5 cu. ft.) 	
Second Row		
Headroom 	961 (37.8) 	
Legroom 	883 (34.8) 	
Shoulder Room	1,342 (52.8) 	
Hip Room	1,326 (52.2) 	
Second Row Interior Volume, litres (cu. ft.)	1,138 (40.2 cu. ft.) 	
Cargo Access		
Liftover Height	774 (30.5)  front-wheel-drive	
	797 (31.4)) all-wheel-drive	
Maximum Cargo Width at Liftgate Opening	1,048 (41.3) 	
Minimum Cargo Width at Liftgate Opening	943 (37.1) (at floor)	
Cargo Height 	731 (28.8) 	
Rear Opening Height 	676 (26.6) 	
Distance Between Wheelhouse Interior Trim	960 (37.8)	
ISO Cargo Volume		
Rear Seats Up, litres (cu. ft.) 	345 (12.2) 	
Rear Seats Folded, litres (cu. ft.)	563 (19.9) 	
Rear Seats Folded (to headliner), litres (cu. ft.)	908  (32.1) 	
Consumer Reports Cargo, litres (cu. ft.)	566 (20.0) 	
		
TIRES		
Availability	Standard — Pop 	
Size and Type 	215/60R16 All-season 	
Mfr. and Model 	Continental, Procontact TX	
		
Availability	Standard — Sport, Trekking, Lounge (FWD)	
Size and Type 	215/55R17 BSW All-season 	
Mfr. and Model 	Continental, Procontact TX or Nexen Class Premiere	
		
Availability	Standard — Sport, Trekking, Lounge (AWD)	
Size and Type 	215/60R17 BSW All-season 	
Mfr. and Model	Nexen Class Premiere 	
		
Availability	Available — Trekking and Lounge (FWD)	
Size and Type 	225/45R18 BSW All-season 	
Mfr. and Model	Continental 	
		
Availability	Available — Trekking and Lounge (AWD)	
Size and Type 	215/55R18 BSW All-season 	
Mfr. and Model	Continental