FCA CANADA
2017 Fiat 500 Abarth / 500c Abarth
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Vehicle Type	A-segment hatchback (500) and cabrio (500c)	
EPA Vehicle Class	Mini-compact	
Assembly Plant	Toluca, Mexico	
	
BODY AND CHASSIS	
Layout	Transverse-mounted front engine, front-wheel drive	
Construction	Unitized steel body 	
	
ENGINE: 1.4-LITRE TURBOCHARGED MULTIAIR I-4	
Availability	Standard — Fiat 500 Abarth and 500c Abarth 	
Type and Description	Inline four-cylinder, liquid-cooled, turbocharged	
Displacement	1,368 cu. cm (83.48 cu. in.)	
Bore x Stroke	72.0 x 84.0 (83 x 3.31) 	
Valve System	Belt-driven, MultiAir, SOHC, 16 valves, hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Cast-iron block with aluminum-alloy head and aluminum-alloy bedplate	
Compression Ratio	9.8:1		
Maximum Turbo Boost (psi / bar)	18 psi / 1.24 bar	
Power (SAE)	160 hp @ 5,500 rpm (117 hp/litre) (with five-speed manual)
157 hp @ 5,500 rpm (114.8 hp/litre) (with six-speed automatic)	
Torque (SAE)	170 lb.-ft. @ 2,500-4,000 rpm (with five-speed manual)
183 lb.-ft. @ 2,400-4,000 rpm (with six-speed automatic)	
Max. Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	87 octane (R+M)/2 acceptable 
91 octane recommended		
Oil Capacity	3.8 litres (4.0 quarts) with dry filter	
Coolant Capacity	4.4 litres (4.6 quarts) 	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors and internal engine features	
Max. Gross Trailer Weight	Not rated for trailer tow	
EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	8.5(33)/6.9(41)/7.8(36) with five-speed manual transmission
9.6(29)/7.3(39)/8.6(33) with six-speed automatic transmission		
Engine Assembly Plant	Dundee, Mich.	
Based on 2016 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca	
		
TRANSMISSION: C510 PERFORMANCE FIVE-SPEED MANUAL	
Availability	Standard — Fiat 500 Abarth and 500c Abarth	
Description	1st, 2nd gear: Double Cone
3rd, 4th, 5th, gear: Single Cone	
Gear Ratios		
1st	3.909	
2nd	2.238 	
3rd	1.520 	
4th	1.156	
5th	0.872 	
Reverse	3.909	
Final-drive Ratio	3.353	
		
TRANSMISSION: AISIN SIX-SPEED AUTOMATIC	
Availability	Optional — Fiat 500 Abarth and 500c Abarth	
Description	Auto Stick driver-interactive manual control and electronically modulated torque converter clutch	
Gear Ratios		
1st	4.04	
2nd	2.37 	
3rd	1.56 	
4th	1.16	
5th	0.85	
6th 	0.67 	
Reverse	3.19	
Final-drive Ratio	3.50	
Overall Top Gear	2.35	
Turning Diameter (curb-to-curb)	11.45 m (37.6 ft.) 	
Steering Turns (lock-to-lock)	2.3	
BRAKES		
Front		
Rotor size and type	282 x 22 (11.1 x 0.86) vented	
Caliper size and type	54 (2.12) single-piston with aluminum housing	
Swept area	1,244 sq. cm (193 sq. in.) 	
Rear	240 x 11 (9.4 x 0.4) solid	
Rotor size and type	34 (1.33) single-piston with aluminum housing	
Caliper size and type	984 sq. cm (153 sq. in.) 	
Swept area	282 x 22 (11.1 x 0.86) vented	
		
DIMENSIONS AND CAPACITIES(b)		
Wheelbase	2,300 (90.6) 	
Track, Front	1,407(55.4) 	
Track, Rear	1,397 (55.0) 	
Overall Length	3,667 (144.4) 	
Overall Width	1,627 (64.1) 
1,866 (73.5) with side mirrors		
Overall Height	500 Abarth: 1,502 (59.2) to antenna base 
500 Abarth: 1,490 (58.7) to roof
500c Abarth: 1,504 (59.2) to roof 		
Ground Clearance	500 Abarth: 103.7 (4.1) 
500c Abarth: 117.2 (4.6) 		
Drag Coefficient (Cd)	500 Abarth: 0.352 — with 16-in. wheels
500 Abarth: 0.365 — with 17-in. wheels
500c Abarth: 0.352 — with 16-in. wheels
500c Abarth: 0.365 — with 17-in. wheels		
Curb Weight, kg (lbs.)	500 Abarth: 1,142 (2,512) 
500c Abarth: 1,154 (2,545)		
Weight Distribution, % F/R	500 Abarth: 64/36 
500c Abarth: 64/36 			
Fuel Tank Capacity, litres (imperial gallons)	40 (8.8) 	
(b) All dimensions measured at curb weight with standard tires.	

ACCOMMODATIONS (Estimated)		
Seating Capacity, F/R	2/2	
Front Seat		
Headroom	500 Abarth: 989 (38.9) 
500 Abarth: 956 (37.6) with sunroof
500c Abarth: 980 (38.6) 	
Legroom	500 Abarth: 1,035 (40.7) 
500c Abarth: 1,035 (40.7) 	
Shoulder Room	500 Abarth: 1,255 (49.4) 
500c Abarth: 1,255 (49.4) 	
Hip Room	500 Abarth: 1,215 (47.8) 
500c Abarth: 1,215 (47.8) 	
Total seat travel	500 Abarth: Driver — 210 (8.2) 
500 Abarth: Passenger — 210 (8.2)	
EPA Front Row Interior Volume, litres (cu. ft.) 	500 Abarth: 1,283 (45.3) 
500c Abarth: 1,271 (44.9) 	
Rear Seat		
Headroom	500 Abarth: 903 (35.5) 
500c Abarth: 994 (36.8) 	
Legroom	500 Abarth: 805 (31.7)
500c Abarth: 805 (31.7) 	
Shoulder Room	500 Abarth: 1,178 (46.4) 
500c Abarth: 1,179 (46.4) 	
Hip Room	500 Abarth: 1,083 (42.6) 
500c Abarth: 1,083 (42.6) 	
EPA Second Row Interior Volume, litres (cu. ft.) 	500 Abarth: 855 (30.2) 
500c Abarth: 886 (31.3) 	
Total Passenger Interior Volume, litres (cu. ft.)	500 Abarth: 2,138 (75.5) 
500c Abarth: 2,158 (76.2) 	
EPA Luggage Compartment Volume, litres (cu. ft.) *	500 Abarth: 269 (9.5)
500 Abarth: 759 (26.8) with rear seats folded
500c Abarth: 153 (5.4) 
500c Abarth: 663 (23.4) with rear seats folded	
EPA Interior Volume Index, litres. 
(cu. m)	500 Abarth: 2,404 (84.9) 
500c Abarth: 2,311 (81.6) 	
Trunk Liftover Height	500 Abarth: 690.2 (27.2) 
500c Abarth: 705.0 (27.7) 	
* BeatsAudio system reduces compartment volume by 17 litres (0.6 cu. ft. )	
WHEELS		
Availability	Standard — Fiat 500 Abarth and 500c Abarth	
Type and material	Cast-aluminum, Hyper Black	
Size	16 x 6.5	
		
Availability	Optional — Fiat 500 and 500c Abarth	
Type and material	Forged-aluminum with Hyper Nero (black) or Bronze painted	
Size	17 x 7.0	
		
TIRES		
Availability	Standard — Fiat 500 Abarth and 500c Abarth	
Size and type	195/45R16 XL 84V BSW All-season	
Mfr. and model	Pirelli Cinturato P7 A/S	
Revs per kilometre (mile)	560 (901) 	
		
Availability	Optional — Fiat 500 Abarth and 500c Abarth	
Size and type	205/40R17 XL 84W BSW	
Mfr. and model	Pirelli P-Zero Nero Three-season	
Revs per kilometre (mile) 	545 (877)