FCA Canada
All-new 2017 Jeep® Compass
Specifications

Specifications are based on the latest product information available at the time of publication. 
All dimensions are in millimetres (inches) unless otherwise noted. 
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Body Style 	Sport Utility Vehicle (SUV)	
Assembly Plant	Toluca, Mexico	
EPA Vehicle Class 	Multipurpose vehicle	
	
BODY AND CHASSIS	
Layout	Transverse front engine, 4x2 and 4x4	
Construction 	Steel uniframe	
	
ENGINE: 2.4-LITRE TIGERSHARK WITH MULTIAIR	
Availability	Standard — All Models	
Type and Description	In-line four-cylinder, 16-valve MultiAir with multiport fuel injection	
Displacement	2,360 cc (144 cu. in.)  	
Bore x Stroke	88 x 97 (3.46 X 3.82) 	
Valve System	SOHC, four valves per cylinder 	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum block, aluminum cylinder head	
Compression Ratio	10:1	
Power (SAE net) 	180 hp (134 kW) @ 6,400 rpm	
Torque (SAE net) 	175 lb.-ft. (237 N•m) @ 3,900 rpm	
Max. Engine Speed	6,400 rpm	
Fuel Requirement	Unleaded regular, 87 octane	
Oil Capacity	5.2 litres (5.5 quarts)  (total)	
Coolant Capacity	6.45 litres (6.8 quarts) 	
Emission Controls	Single catalytic converter, heated wide band lambda sensor upstream and mid-catalyst heated oxygen sensor	
Fuel Economy* city / highway	N/A	
	
Towing	907 kg (2,000 lbs.)  (not recommended for 4x2)	
Engine Assembly Plant 	Saltillo Engine Plant, Saltillo, Mexico	

		
TRANSMISSION: 9HP48 NINE-SPEED AUTOMATIC	
Availability	2.4-litre Tigershark engine with MultiAir (4x4)	
Description 	Planetary gear train, transverse layout	
Ratio Spread	9.81	
Gear Ratios		
1st	4.71	
2nd	2.84	
3rd	1.91	
4th	1.38	
5th	1.00	
6th	0.81	
7th	0.70	
8th	0.58	
9th	0.48	
Reverse	3.81	
Final-drive Ratio	3.734	
	4.334 (Trailhawk)	
		
C635 SIX-SPEED MANUAL TRANSMISSION		
Availability	2.4-litre Tigershark engine with MultiAir (4x2 and 4x4)	
Description	Planetary gear train, transverse layout	
Gear Spread	6.635	
Gear Ratios		
1st	4.459	
2nd	2.508	
3rd	1.556	
4th	1.142	
5th	0.852	
6th	0.672	
		
AT6 AISIN SIX-SPEED AUTOMATIC TRANSMISSION	
Availability	2.4-litre Tigershark engine with MultiAir (4x2)	
Description	Planetary gear train, transverse layout	
Gear Spread	6.635	
Gear Ratios		
1st	4.459	
2nd	2.508	
3rd	1.556	
4th	1.142	
5th	0.852	
6th	0.672	
	
4X4 SYSTEMS: JEEP ACTIVE DRIVE, JEEP ACTIVE DRIVE LOW	
Availability 	Jeep Active Drive is optional on Sport and North, standard on Limited
Jeep Active Drive Low is standard on Trailhawk	
Type	Fully disconnecting 4x2 mode with automatic 4x4 engagement
Full-time 4x4 mode with active on demand clutch	
Operating Modes	Auto 4x2/4x4, Neutral	
Center Differential Type	None	
Terrain Response	Unique tuning in all terrain modes	
Crawl Ratio	20:1 (with Jeep Active Drive Low)	
		
ELECTRICAL SYSTEM		
Alternator 	160-amp (2.4-litereTigershark with MultiAir)  	
Battery	Dual batteries when equipped with electronic stop-start system: 500-amp (primary) 150-amp (secondary) (2.4-litre Tigershark 
with MultiAir with ESS)	
		
SUSPENSION		
Front 	MacPherson strut, coil springs, flat front steel crossmember, high-strength steel double shell lower control stabilizer bar	
Rear	Chapman strut, high-strength steel links, isolated steel rear cradle for 4x4 and not-isolated for 4x2, coil springs, 
stabilizer bar	
		
STEERING		
Type 	Electric power rack and pinion	
Overall Ratio 	15.7	
Turning Diameter (curb-to-curb) 	11.07 (36.3) 4x2 and 4x4
10.76 (35.3)  Trailhawk 4x4	
Steering Turns (lock-to-lock)	2.68 (4x2 and 4x4)	
2.76 (Trailhawk 4x4)	
		
BRAKES		
Front		
Size and Type	305 x 28 (12 x 1.1) vented rotor with 60 (2.36)  single-piston floating caliper	
	
Swept Area (per caliper)
		895.3 sq. cm . (138.77 sq. in.) 1 x 60	
747.6 sq. cm. (115.88 sq. in.) , 1 x 57		
Rear		
Size and Type 	278 x 12 (10.95 x 0.47) solid rotor with 38 (1.5)  single-piston floating caliper	
Swept Area (per caliper)	656.4 sq. cm (101.7 sq. in.), 1 x 38	
Power-assist Type 	254 (10) vacuum assist	
Four-wheel anti-lock brake system (ABS)	Standard	
Electronic stability control (ESC)	Standard	
Parking Brake Type	Electric Motor	
		
DIMENSIONS AND CAPACITIES		
Wheelbase	2,636 (103.8) 	
Track, Front	1,542 (60.7) 	
Track, Rear	1,532 (60.3) 	
Overall Length	4,394 (173) 	
Overall Width (with folded side mirrors)	1,874 (73.8) 	
Overall Width (with open side mirrors)	2,033 (80) 	
Overall Height 	1,641 (64.6)  without rails; 1,647 (64.8)  with rails	
Load-floor height	754 (29.7)  (height measured from curb ground to load floor)	
Sill-step height	494 (19.4)  (height measured from curb ground to sill trim)	
Ground Clearances 	4x2 198 (7.8) 
4x4 208 (8.2) 
Trailhawk 4x4 216 (8.5) 	
Approach Angle, (with air dam) (degrees)	4x2 15.8
4x4 16.8
Trailhawk 4x4 30.3	
Breakover Angle (degrees)	4x2 21.8
4x4 22.9
Trailhawk 4x4 24.4	
Departure Angle (degrees)	4x2 30.8
4x4 31.7
Trailhawk 4x4 33.6	
Curb Weight (kg)	1,444 (3,184)  4x2 and 2.4-litre Tigershark with MultiAir
1,509 (3,327)  4x4 and 2.4-litre Tigershark with MultiAir
1,648 (3,633)  Trailhawk 4x4 with 2.4-litre Tigershark 
with MultiAir	
Fuel-tank Capacity	51 litres (11.2 imperial gal.) 	
	
ACCOMMODATIONS		
Seating Capacity — Front/Rear 	2/3 	
Front Row		
Headroom without Sunroof	995 (39.2) 	
Headroom with Sunroof	981 (38.6) 	
Legroom 	1,046 (41.8) 	
Shoulder Room 	1,439 (56.7)	
Hip Room	1,375 (54.1) 	
Seat Travel 	220 (8.7)  fore/aft travel range	
Recliner Range (degrees)	Manual/power recliner travel: 69 degrees	
Manual fold FWD recliner travel: 107.5 degrees	
SAE Volume (standard roof), Litres (cu. ft.)	1,498 (52.9)  front passenger volume	
Second Row		
Headroom 	978 (38.5) 	
Legroom 	973 (38.3) 	
Shoulder Room 	1,400 (55.1) 	
Hip Room	1,264 (49.8)  	
   SAE Volume, Litres (cu. ft.) 	1,322 (46.7)  Second Row Passenger Volume	
Cargo Access		
Liftover Height	790 (31.1)  (Height measured from Curb Ground to Liftgate 
Scuff Trim)	
Maximum Cargo Width at Liftgate Opening	1,069 (42.1)  	
Minimum Cargo Width at Liftgate Opening 	938 (36.9) 	
Maximum Cargo Height at Liftgate Opening	691 (27.2) 	
Distance Between Wheelhouse Interior Trim	968 (38.1) 	
SAE Cargo Volume		
Rear Seats Up, Litres (cu. ft.)	770 (27.2) 	
Rear Seats Folded, Litres (cu. ft.)	1,693 (59.8) 	
EPA Interior Volume Index, Litres (cu. ft.)	3,587.7 (126.7) 	

TIRES		
Availability	Standard — Sport 4x2, Sport 4x4	
Size and Type 	215/65R16 BSW All-season 	
Mfr. and Model 	Continental CrossContact LX Sport or Kumho Crugen Premium	
Revs per Kilometre (Mile) 	479 (770) 	
		
Availability	Standard — North 4x2, North 4x4	
Size and Type 	225/60R17 BSW All-season 	
Mfr. and Model 		Kumho Crugen Premium or Firestone Destination LE2	
Revs per Kilometre (Mile)	466 (749) 	
		
Availability	Optional-Limited 4x4	
Size and Type 	235/45R19 BSW All Season	
Mfr. and Model	Continental ContiProContact	
Revs per Kilometre (Mile)	476 (766) 	
		
Availability	Standard on Trailhawk  	
Size and Type	215/65R17 OWL All-season	
Mfr. and Model	Falken WildPeak H/T	
Revs per Kilometre (Mile)	462.8 (744) 	
		
Availability	Optional - North, Limited	
Size and Type	225/55 R18 BSW All-season 	
Mfr. and Model	Continental 	
Revs per Mile (km)	744 (462)	
		
Availability	Optional - North, Limited 	
Size and Type	225/55 R18 BSW All-season	
Mfr. and Model	Yokohama 	
Revs per Mile (km)	744 (462)