FCA CANADA
2017 Jeep® Grand Cherokee / Grand Cherokee SRT
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Vehicle Type	Four-door sport-utility vehicle	
Assembly Plant	Jefferson Avenue North, Detroit, Mich., USA	
EPA Vehicle Class	Multipurpose vehicle	
Introduction Date	Spring 1992 as a 1993 model	
		
BODY AND CHASSIS		
Layout	Front engine, four-wheel drive	
Construction	Steel uniframe	
		
ENGINE: 3.6-LITRE PENTASTAR V6	
Availability	Standard on all models other than SRT	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	3,604 cu. cm (220 cu. in.) 	
Bore x Stroke	96 x 83 (3.77 x 3.26) 	
Valve System	Chain-driven DOHC, 24 valves and hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum deep-skirt block, aluminum alloy heads	
Compression Ratio	10.2:1	
Power (est.) (SAE J2723)	Up to 295 hp at 6,400 rpm	
Torque (est.) (SAE J2723)	260 lb.-ft. at 4,800 rpm	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R + M)/2	
Oil Capacity	5.7 litres (6.0 quarts) 	
Coolant Capacity	13.2 litres (14.0 quarts) 	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors  and internal engine features	
Max. Gross Trailer Weight	2812.2 kg (6,200 lbs.) —  4WD	

EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	12.8 (22)/9.5 (29)/11.3 (25)	
Based on 2016 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca
	
Assembly Plant	Trenton, Mich., USA	
		
ENGINE: 5.7-LITRE V8		
Availability	Optional — Limited, Trailhawk, Overland and Summit 	
Type and Description	90-degree V-type, liquid-cooled	
Displacement	5,654 (345 cu. in.) 	
Bore x Stroke	99.5 x 90.9 (3.92 x 3.58) 	
Valve System	Variable-valve timing (VVT), pushrod-operated overhead valves, 16 valves, eight deactivating and eight conventional hydraulic lifters, all with roller followers	
Fuel Injection	Sequential, multi-port, electronic, returnless	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.5:1	
Power (est.) (SAE J2723)	360 hp (268 kW) at 5,150 rpm	
Torque (est.) (SAE J2723)	390 lb.-ft. (520 N•m) at 4,250 rpm	
Max. Engine Speed	5,800 rpm (electronically-limited)	
Fuel Requirement	Unleaded mid-grade, 89 octane (R+M)/2 — recommended; unleaded regular, 
87 octane (R+M)/2 — acceptable	
Oil Capacity	6.6 litres (7 quarts) 	
Coolant Capacity	13.7 litres (14.5 quarts) 	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad heated oxygen sensors and internal engine features	
Max. Gross Trailer Weight	3265.8 (7,200 lbs.) (4x4) 	
EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	16.7 (17)/10.7 (26)/14.0 (20)	
Assembly Plant	Saltillo, Mexico	
		
ENGINE:  3.0-LITRE DOHC ECODIESEL V6	
Availability	Optional — Overland and Summit	
Type and Description	60-degree V-type, liquid-cooled	
Displacement	2,988 cu. cm (182 cu. in.) 	
Bore x Stroke	83 x 92 (3.27 x 3.60) 	
Valve System	Chain-driven DOHC, 24 valves 	
Fuel Injection	Common-rail, 2000 bar, Solenoid Injectors	
Construction	Iron block, aluminum alloy heads	
Compression Ratio	16.5:1	
Power (est.) (SAE J2723)	240 hp (179 kW) at 3,600 rpm 	
Torque (est.) (SAE J2723)	420 lb.-ft. (569 N•m) at 2,000 rpm	
Max. Engine Speed	4,800 rpm (electronically limited)	
Fuel Requirement	Ultra Low-sulfur diesel	
Oil Capacity	7.8 litres (8.2 quarts) 	
Coolant Capacity	11.4 litres (12 quarts) 	
Emission Controls 	Cooled EGR, Oxidation catalyst, Diesel particulate filter, SCR with urea injection	
Max. Gross Trailer Weight	3,265 kg (7,200 lbs.)	
EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	11.2 (25)/8.4 (34)/9.9 (29)	
Assembly Plant	VM Motoric Cento, Ferrara, Italy	
		
ENGINE: 6.4-LITRE V8	
Availability	Standard — SRT 	
Type and Description	90-degree V-type, liquid-cooled	
Displacement	6,417 cu. cm (392 cu. in.)	
Bore x Stroke	103.9 x 94.5 (4.09 x 3.72) 	
Valve System	Pushrod-operated overhead valves, 16 valves with sodium-filled exhaust valves and hollow stem intake valves, 16 conventional hydraulic lifters, all with roller tips	
Fuel Injection	Sequential, multi-port, electronic, returnless; automatic features Fuel Saver mode	
Construction	Deep-skirt cast-iron block with cross-bolted main bearing caps, aluminum alloy heads with hemispherical combustion chambers	
Compression Ratio	10.9:1	
Power (SAE J2723)	475 hp (354 kW) at 6,000 rpm 	
Torque (SAE J2723)	470 lb.-ft. (637 N•m) at 4,300 rpm 	
Max. Engine Speed	6,400 rpm (electronically limited)	
Fuel Requirement	Premium 91 octane (R+M)/2 — recommended	
Oil Capacity 	6.6 litres (7.0 quarts) 	
Coolant Capacity	13.2 litres (14.0 quarts) 	
Factory Oil Fill 	0W-40 Pennzoil Ultra synthetic	
Emission Controls 	Dual close-coupled three-way catalytic converters, quad-heated oxygen sensors and internal engine features	
Exhaust Type 	Dual exhaust with dual 10.1 cm (4-in.) oval black chrome tips 	
EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	18.5 (15)/12.6(22)/15.8 (18)	
Assembly Plant	Saltillo, Mexico 	
		
TRANSMISSION: ZF AUTOMATIC, EIGHT-SPEED OVERDRIVE	
Availability	Standard — all models	
Description	Driver-interactive manual control via steering wheel paddle shifters and electronically-modulated torque converter clutch with Eco mode	
Gear Ratios		
1st	4.71	
2nd 	3.14	
3rd	2.11	
4th 	1.67	
5th 	1.29	
6th	1.00	
7th	0.84	
8th 	0.67	
Reverse 	3.30	
		
TRANSFER CASE: MP 3010		
Availability	Optional with V6	
Type	Single-speed	
Operating Mode	Full-time AWD	
Low Range Ratio	None	
Torque Split, Front/Rear	50/50 	

TRANSFER CASE: MP 3010		
Availability	Standard with 6.4-litre V8 engine 	
Type	Single-speed, electronic proportioning	
Operating Mode	Full-time 4WD	
Torque Split, Front/Rear	Variable – 40/60 Auto, 50/50 Snow and Tow, 35/65 Sport and 30/70 Track	
		
TRANSFER CASE: MP 3022		
Availability	Optional with the V6, 5.7-litre V8 and EcoDiesel engines	
Type	Two-speed, electronically shifted	
Operating Modes	4x4 Low (Lock), Neutral; full-time active 4x4	
Low Range Ratio	2.72	
Torque Split, Front/Rear	Variable	
		
AXLES		
Front		
Differential Type	Conventional	
Availability	Standard all models 	
Ring Gear Diameter	195 (7.7) 	
Axle Ratios	3.45:1 — 3.6-litre V6 and EcoDiesel
3.09:1 — 5.7-litre V8
3:70:1 — 6.4-litre V8	
Rear		
Differential Type	Conventional (optional Electronic Limited Slip on 5.7-litre V8 and EcoDiesel, Standard on 6.4-litre V8)	
Availability	Standard on all engines	
Ring Gear Diameter 	195 (7.7) — V6 4x4 
230 (9.1 )— V6 EcoDiesel, 5.7-litre V8 and 6.4-litre V8	
Axle Ratios
	3.45:1 — V6 and EcoDiesel
3.09:1 — 5.7-litre V8
3:70:1 — 6.4-litre V8	

ELECTRICAL SYSTEM		
Alternator	160-amp; 180-amp or 220-amp depending on model	
Battery	Maintenance-free 
H6 650 CCA + Auxiliary 200 CCA on Electronic Stop/Start (ESS)
H7 700 CCA on V8, H8 800 CCA on 3.0-liter EcoDiesel 
(not equipped with ESS)	
		
SUSPENSION		
Front	Short- and long-arm independent (SLA), coil springs, gas-charged, twin-tube coilover shock absorbers, steel upper- and aluminum lower-control arms 
(“A” arms), aluminum knuckle, hollow stabilizer bar	
Front – SRT 	Short- and long-arm independent (SLA) with aluminum lower control arm, aluminum knuckle, aluminum clevis, coil springs, Bilstein adaptive damping suspension (ADS), upper- and lower-control arms (“A” arms), hollow stabilizer bar	
Rear	Multi-link rear suspension, coil spring, twin tube shocks (including load leveling for towing), aluminum lower control arm, independent upper links (tension and camber) plus a separate toe link, hollow stabilizer bar	
Rear - SRT	Multi-link rear suspension, coil spring, Bilstein adaptive damping suspension (ADS), aluminum lower control arm, independent upper links (tension and camber) plus a separate toe link, hollow stabilizer bar	
		
STEERING		
Type	Electric rack and pinion, SRT-tuned on SRT model	
Overall Ratio	16.7:1 	
Turning Diameter (curb-to-curb) 	11.3 m (37.1 ft) 	
Steering Turns (lock-to-lock)	3.2 	
	
BRAKES		
Type	Power, single-rate, tandem diaphragm vacuum, anti-lock braking system (ABS)	
Availability	Standard	
Front		
Rotor size and type	330 x 32 (13.0 x 1.3) vented disc – V6
350 x 32 (13.8 x 1.3) – EcoDiesel and 5.7-litre V8
380 x 34 (15.0 x 1.34) vented disc with Brembo six-piston caliper and ABS – 
SRT 6.4-litre V8
380 x 34 (15.0 x 1.34) 2-piece aluminum hat performance rotor, directionally slotted with Brembo six-piston caliper and ABS – available on SRT model	
Caliper size and type	48 (1.89) two-piston pin-slider caliper	
Swept area, (sq. cm  / sq. in.)	1,820 (282) 
672 (104.2) —  SRT	
Rear		
Rotor size and type	330 x 14 (13.0 x 0.55) disc – V6
330 x 22 (13.0 x 0.87) vented disc – EcoDiesel and V8
350 x 28 (13.78 x 1.10) disc with Brembo four-piston caliper and single-channel ABS – SRT
350 x 28 (13.78 x 1.10)  Performance disc , directionally slotted with Brembo 
four-piston caliper and single-channel ABS available on SRT	
Caliper size and type	48 (1.89)  single-piston pin-slider caliper	
Swept area, (sq. cm / sq. in.)	1,658 (257) 
508 (79.0) — SRT		
		
DIMENSIONS AND CAPACITIES		
Wheelbase	2,915 (114.8) 	
Track, Front	1,623 (63.9) 
1,636 (64.4) — SRT		
Track, Rear	1,627 (64.1) 
1,634 (64.7) — SRT	
Overall Length	4,822 (189.8) 	
Overall Width (Width at Mirrors)	2,154 (84.8) 	
Body Width	1,943 (76.5) 	
Overall Height (at Roof Rail / at Antenna)	1,761 (69.3)  / 1,779 (70.0) 
1,717 (67.6) / 1,773 (69.8)   — SRT		
Load Floor Height	822 (32.4) — standard suspension and SRT
807 (31.8) — air suspension	
Sill Step Height	530 (20.5) — standard suspension
508 (20.0) — air suspension
527 (20.7) — SRT	
Ground Clearance  (with P245/70R17 Tire and 3.6-litre engine)	218 (8.6) — standard suspension
264 (10.4) — air suspension (Off-Road 2)
274(10.8) — air suspension (Off-Road 2)– Trailhawk with 265/50R20 Tire 
210 (8.3) — SRT	
Chassis (Fuel Tank) 	243 (9.6) — standard suspension
271 (10.7) — air suspension (Off-Road 2)
230 (9.0) — SRT	
Front Axle 	236 (9.3) — standard suspension
246 (9.7) — air suspension (Off-Road 2)
(227.8 (8.97) — SRT		

Rear Axle 	253 (10.0) — standard suspension
282 (11.1) — air suspension (Off-Road 2)
228.3 (8.99) — SRT	

Approach Angle (degrees)	26.2 — standard suspension
36.1 — air suspension (Off-Road 2, air-dam off)
29.8 (Off-Road II w/air dam on)
18.45 — SRT	
Ramp Breakover Angle (degrees)	19.0 — standard suspension
22.8 — air suspension (Off-Road 2)
25.7 with air suspension - Trailhawk
17.84 — SRT	
Departure Angle (degrees)	24.0 — standard suspension
27.1 — air suspension (Off-Road 2)
21.9 — SRT	
Frontal Area sq. m. (sq. ft.)	2.88 (31.0) 
2.93 (31.5) — SRT	
Drag Coefficient 	0.371
0.39 — SRT	
Aero CdA	11.5 (Cd x cross-sectional area)
12.2 (Cd x cross-sectional area) — SRT	
Fuel Tank Capacity, litres (imp. gal.)	93. 1 (20.5) 	
		
ACCOMMODATIONS		
Seating Capacity (front/rear) 	2/3	
SAE Total Interior Passenger Volume, litres (cu. ft.)	2984.5 (105.4)	
Front		
Headroom	1,013 (39.9) 	
Legroom	1.025 (40.3) 	
Shoulder Room	1,491 (58.7) 	
Hip Room	1,449 (57.0) 	
Seat Travel	280 (11.0) 	
EPA Front Volume Index, litres 
(cu. ft.)	1546.1 (54.6) 	
Rear 				
Headroom	995 (39.2) 	
Legroom	981 (38.6) 	
Knee Clearance	110 (4.3)	
Shoulder Room	1,474 (58.0) 	
Hip Room	1,428 (56.2) 	
EPA Rear Seat Volume Index, litres (cu. ft.) 	1438.4 (50.8) 	
Maximum Cargo Volume, litres (cu. ft.) 	1934.0 (68.3) 	
Behind Second-row Seats, litres (cu. ft.) 	1027.9 (36.3) 	
Total Passenger plus Cargo Volume, litres (cu. ft.) 	3978.5 (140.5) 	

WEIGHTS (Estimates)	
	MODEL	ENGINE	GVWR(a) kg (lbs.)	CURB WEIGHT(b) kg (lbs.)	PAYLOAD(c) kg (lbs.)	
4WD	Laredo	3.6-litre	2,948 (6,500)	2,121 (4,677) 	600 (1,320) 	
	Limited	3.6-litre
5.7-litre	2,948 (6,500)
3,084 (6,800) 	2,211 (4,875) 
2,329 (5,135) 	580 (1,270) 
585 (1,290) 	
	Trailhawk	3.6-litre
5.7-litre	2,948 (6,500)
3,084 (6,800) 	2,209 (4,869) 
2,238 (5,154) 	540 (1,190) 
540 (1,190) 	
		3.6-litre	2,948 (6,500) 	2,261 (4,984)	520 (1,150)	
	Overland	5.7-litre	3,084 (6,800)	2,381 (5,250)	520 (1,150)	
		3.0-litre EcoDiesel	3,084 (6,800)	2,446 (5,393)	530 (1,170)	
		3.6-litre	2,948 (6,500)	2,247 (4,952)	520 (1,150)	
	Summit	5.7-litre	3,084 (6,800)	2,367 (5,192)	520 (1,150)	
		3.0-litre EcoDiesel	3,084 (6,800)	2,437 (5,374)	520 (1,150)	
	SRT	6.4-litre 	2,948 (6,500)	2,315 (5,104) 	612 (1,350) 	
(a) Gross Vehicle Weight Rating. 
(b) Curb weight includes standard equipment and full quantities of fuel, lubricant and coolant.
(c) Payload is the maximum allowable weight of driver, passengers, cargo, and options, rounded to the nearest 10 lbs. (5kg).	

WEIGHT DISTRIBUTION, F/R	
	MODEL	ENGINE	DISTRIBUTION 	
4WD	Limited	3.6-litre
5.7-litre	52/48
54/46	
	Trailhawk        	3.6-litre
5.7-litre	52/48
54/46	
	Overland	3.6-litre
5.7-litre
3.0-litre EcoDiesel	52/48
53/47
53/47	
	Summit	3.6-litre
5.7-litre
3.0-litre EcoDiesel	51/49
53/47
53/47	
	SRT 	6.4-litre	55/45	

Wheels	
Availability	Standard on Laredo 	
Type and Material	Painted machine cast-aluminum, five-spoke 	
Size (inches)	17 x 8	
		
Availability		Available on Laredo, available on Overland 	
Type and Material	High-Gloss Silver aluminum 	
Size (inches)	18 x 8	
		
Availability 	Standard on Trailhawk	
Type and Material	Polished machine cast-aluminum with low gloss painted pockets	
Size (inches)	18x8	
		
Availability	Standard on Limited	
Type and Material	Premium polished aluminum with Technical Grey pockets	
Size (inches)	18 x 8	
		
Availability	Available on Limited	
Type and Material	Satin Silver aluminum	
Size (inches)	20 x 8	
		
Availability 	Standard on Overland 	
Type and Material	Polished aluminum with Technical Grey pockets	
Size (inches)	20 x 8 	
		
Availability	Standard on Summit	
Type and Material	Full polished aluminum with Satin Clear Coat	
Size (inches)	20 x 8	
		
Availability	Optional on Summit with the Premium Plus Appearance Group	
Type and Material	Satin Carbon aluminum	
Size (inches)	20 x 8	
		
Availability	Standard on SRT	
Type and Material	Full polished with Satin Clear Coat	
Size (inches)	20 x 10	
		
Availability	Available on SRT	
Type and Material	Matte Black split-spoke	
Size (inches)	20 x 10	
		
Availability	Available on SRT	
Type and Material	Polished face and Satin Clear Coat with Low-Gloss Titanium pockets	
Size (inches)	20 x 10	

TIRES		
Availability	Standard — Laredo	
Size and Type	P245/70R17	
Mfr. and Model	Goodyear Fortera HL Black Sidewall On/Off road 	
Revs per km (mile)	1,103 (685)	
	
Availability	Standard — Limited; Optional — Laredo	
Size and Type	265/60R18 	
Mfr. and Model	Michelin Premier LTX Black Sidewall All-Season 	
Revs per km (mile)	1,903 (679)	
		
Availability 	Standard on Trailhawk	
Size and Type 	265/60R18	
Mfr. And Model 	Goodyear All-Terrain Adventure with Kevlar reinforcement	
Revs per km (mile) 	1,106 (687)	
		
Availability	Standard — SRT	
Size and Type	P295/45ZR20	
Mfr. and Model	Pirelli Scorpion Verde  —  All-season Performance (run flat)	
Revs per km (mile)	1,125 (699)	
		
Availability	Optional — SRT	
Size and Type 	P295/45ZR20	
Mfr. and Model	Pirelli P-Zero  — Three-season (run flat)	
Revs per km (mile)	1,125 (699)	
		
Availability 	Standard — Overland Optional - Laredo, Limited and Summit	
Size and Type	265/50R20	
Mfr. and Model	Bridgestone Ecopia H/L 422 Plus Black Sidewall All-Season 	
Revs per km (mile)	1,103 (685)	
		
Availability	Standard on Summit
Optional — Overland and Limited	
Size and Type	265/50R20 	
Mfr. and Model	Pirelli Scorpion Verde Black Sidewall All-Season	
Revs per km (mile)	1,105 (686)	
		
Packaged with Off-road Adventure II (AWY)	Packaged with Off-road Adventure II (AWY)	
Size and Type	265/60R18	
Mfr. and Model	Goodyear Wrangler All-Terrain Adventure with Kevlar Black Sidewall	
Revs per km (mile)	1,103 (685)	
		
Parking Brake Type	Drum-in-hat	
Four–wheel Anti-lock Brakes	Standard	
Electronic stability control	Standard	
All-speed traction control	Standard	
Brake Assist	Standard	

TRAILER TOWING				
	Engine	Axle Ratio	Maximum Trailer  
Weight kg (lbs.)	
4WD	3.6-litre V6	3.45	2,818 (6,200)	
	5.7-litre V8	3.09	3265 (7,200)	
	3.0-litre EcoDiesel V6	3.45	3,300 (7,200)	
	6.4-litre V8	3.70	3265 (7,200)