FCA CANADA
2017 Jeep® Patriot
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION		
Vehicle Type	Sport-utility vehicle	
Assembly Plant	Belvidere, Illinois, USA	
EPA Vehicle Class	Compact SUV	
Introduction Date	December 2006 as a 2007 model	
		
BODY AND CHASSIS		
Layout	Transverse front-engine front-wheel drive or four-wheel drive	
Construction	Unitized steel body 	
		
ENGINE: 2.0-LITRE I-4  WORLD GAS ENGINE	
Availability	Standard — 2WD Patriot Sport and 2WD Patriot High Altitude	
Type and Description 	Four cylinders in-line, tuned intake manifold with electronic active charge motion control valves, dual counter-rotating balance shafts	
Displacement	1,998 cu. cm (121.9 cu. in.) 	
Bore x Stroke	86 x 86 (3.39 x 3.39) 	
Valve System	Chain-driven DOHC, 16 valves, electronically-controlled dual variable-valve timing (VVT), direct-acting shimless mechanical bucket tappets	
Fuel Injection 	Sequential, multiport, electronic, returnless	
Construction 	High-pressure die-cast aluminum block with dry iron liners, cast-aluminum cylinder head, cast-aluminum ladder frame, forged-steel crankshaft	
Compression Ratio	10.5:1	
Power (SAE net, estimated)	158 bhp (117 kW) @ 6,400 rpm (79 bhp/litre)	
Torque (SAE net, estimated) 	141 lb.-ft. (191 N•m) @ 5,000 rpm 	
Maximum Engine Speed	6,750 rpm (electronically limited)	
Fuel Requirement 	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity	4.7 litres (5.0 quarts) SAE 5W/20	
Coolant Capacity	6.8 litres (7.2 quarts)	
Emission Controls	Single catalytic converter, dual heated oxygen sensors and engine features	
		
EnerGuide 2016 Fuel Consumption Ratings, L/100 km (MPG – imperial gallon) (city/hwy) 	7.8 (36) / 10.3 (27) — 2WD with five-speed manual transaxle
8.9 (32) / 10.8 (26) — 2WD with continuously-variable transmission (CVT) automatic transmission	
		
ENGINE: 2.4-LITRE WGE I-4		
Availability	Standard — North Edition, Sport Altitude II, Sport 4x4, High Altitude 4x4 	
Type and Description	Four-cylinder in-line, tuned intake manifold with electronic active charge motion control valves, dual counter-rotating balance shafts	
Displacement	2,360 cu. cm (144 cu. in.) 	
Bore x Stroke	88 x 97 (3.46 x 3.82) 	
Valve System	Chain-driven DOHC, 16 valves, electronically-controlled dual VVT, direct-acting shimless mechanical bucket tappets	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	High-pressure die-cast aluminum block with dry iron liners, cast-aluminum cylinder head, cast-aluminum ladder frame, forged steel crankshaft	
Compression Ratio	10.5:1	
Power (SAE net, estimated)	172 bhp (129 kW) @ 6,000 rpm (72 bhp/litre)	
Torque (SAE net, estimated)	165 lb.-ft. (224 N•m) @ 4,400 rpm 	
Maximum Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	Unleaded regular, 87 octane (R+M)/2	
Oil Capacity	4.7 litres (5.0 quarts) SAE 5W/20	
Coolant Capacity	6.8 litres (7.2 quarts) 	
Emission Controls 	Single catalytic converter — 2WD 	
		Dual catalytic converter — 4x4	
	Dual heated oxygen sensors and engine features	
Maximum Gross Trailer Weight	454 kg (1,000 lbs.) 	
	907 (2,000 lbs.) — with Freedom Drive II Package, Trailer-tow Prep Group	
EnerGuide 2016 Fuel Consumption Ratings, L/100 km (MPG – imperial gallon) (city/hwy) 	8.2 (34) / 10.2 (28) — 2WD with five-speed manual transaxle
8.6 (33) / 11.2 (25) — 2WD with six-speed automatic transmission  
8.6 (33) / 10.6 (27) — 4x4 with five-speed manual transaxle
9.1 (31) / 11.7 (24) — Freedom Drive I 4x4x4 with six-speed automatic transmission 
10.3 (27) / 11.7 (24) — Freedom Drive II Off-road Package 4x4x4 with continuously-variable transaxle with low range (CVT2)	
Based on 2016 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca	

		
TRANSAXLE: MAGNA DRIVELINE T355 FIVE-SPEED MANUAL	
Availability	Standard — 2.0-litre engine Sport 4x2	
	Standard — 2.4-litre engine Sport 4x4	
Description	Five-speed, overdrive, synchronized in all forward ratios, cable-operated, 
3-plane shifter	
Gear Ratios		
1st	3.77	
2nd	2.16	
3rd	1.41	
4th	1.026	
5th	0.72	
Reverse	3.417	
Final-drive Ratio	4.12	
Overall Top-gear	2.97	
		
TRANSAXLE: SIX-SPEED AUTOMATIC 6F24 PowerTech WITH AUTO STICK	
Availability	Standard — 2.4-litre High Altitude 4x4, Sport Altitude II and North Edition
Optional — 2.4-litre engine Sport	
Description	Six-speed automatic transmission, lockup torque converter, electronic controls	
Gear Ratios		
1st	4.212	
2nd	2.637	
3rd	1.800	
4th	1.386	
5th	1.000	
6th	0.772	
Reverse 	3.285	
Final-drive Ratio	3.367:1 (2.4-litre engine)	
Overall Top-gear Ratio	2.600:1 (2.4-litre engine)	
Auto Stick	Standard	
		
TRANSAXLE: AUTOMATIC JATCO MODEL CVT	
Availability	Standard — 2.0-litre engine High Altitude	
Description	Continuously variable ratio, lockup torque converter, electronic controls	
Gear Ratios		
Forward	2.349:1 to 0.394:1 continuously variable	
Reverse	1.75:1	
Final-drive Ratio	6.12:1	
Overall Top-gear Ratio	2.41:1	
Effective Maximum Low-gear Ratio	19.11:1	
		
TRANSAXLE: AUTOMATIC JATCO MODEL CVT2	
Availability	Optional — Patriot Sport and North Edition 4x4x4 with 2.4-litre engine and Freedom Drive II	
Description	Continuously variable ratio, lockup torque converter, electronic controls	
Gear Ratios		
Forward	2.349:1 to 0.394:1 continuously variable	
Reverse	1.75:1	
Final-drive Ratio	8.135:1	
Overall Top-gear Ratio	3.21:1	
Effective Maximum Low-gear Ratio	19.11:1	
		
DRIVETRAIN		
Front-Wheel-Drive		
Availability	Standard	
Front Differential 	Open	
Four-Wheel-Drive		
Availability	Optional	
Type	Electronically-controlled coupling (ECC) with four-wheel drive Lock	
Rear Differential 	Open	
		
ELECTRICAL SYSTEM		
Alternator	120-amp	
	140-amp with CVT2	
Battery	525 CCA, maintenance-free	
		
DIMENSIONS AND CAPACITIES		
Wheelbase	2,635 (103.7) 	
Track — Front	1,520 (59.8) 	
Track — Rear	1,520 (59.8) 	
Overall Length	4,413.6 (173.8) 	
Overall Width	1,757.1 (69.2) 	
Overall Height	1,662.9 (65.5) — 2WD; 1,695.6 (66.8) — 4x4 	
Overhang — Front	885.1 (34.7)	
Overhang — Rear	893.5 (35.1) 	
Approach Angle with P215/60/R17 Tire (degrees)	26.4	
Breakover Angle with P215/60/R17 Tire (degrees)	20.9	
Departure Angle with P215/60/R17 Tire (degrees)	28.5	
Ground Clearance with P215/60/R17 Tire	205 (8.1)	
Approach Angle with Freedom Drive II Off-road Package including P215/65/R17 Tire (degrees)	29.0	
Breakover Angle with Freedom Drive II Off-road Package including P215/65/R17 Tire (degrees)	23.7	
Departure Angle with Freedom Drive II Off-road Package including P215/65/R17 Tire (degrees)	33.9	
Ground Clearance with Freedom Drive II Off-road Package including P215/65/R17 Tire	231 (9.1) 	
Aero (CdA)	10.4 — 2WD	
	11.0 — 4x4	
Curb Weight, kg (lbs.), Estimated	1,421 (3,133) — 2WD, 2.0-litre MTX	
	1,456 (3,211) — 2WD, 2.0-litre CVT ATX	
	1,423 (3,137) — 2WD, 2.4-litre MTX	
	1,457 (3,213) — 2WD, 2.4-litre ATX	
	1,492 (3,290) — 4x4, 2.4-litre MTX	
	1,527 (3,367) — 4x4, 2.4-litre ATX	
	1,530 (3,373) — 4x4, 2.4-litre CVT2 ATX	

Weight Distribution, percent F/R	58/42 — 2WD	
	57/43 — 4x4	
Fuel Tank Capacity, litres (gal.)	51.5 (13.6) — 2WD	
	51.1 (13.5) — 4x4	
		
ACCOMMODATIONS		
Seating Capacity — F/R	2/3	
Front		
Headroom without Sunroof	1,040.3 (41.0) 	
Legroom	1,032.1 (40.6) 	
Shoulder Room	1,385 (54.5) 	
Hip Room	1,328.4 (52.3) 	
Seat Travel	Driver — 260 (10.2) 	
	Passenger — 260 (10.2) 	
Recliner Angle Range (degrees)	Driver — Up to 88 	
	Passenger — up to 88	
SAE Front Volume Index, litres (cu. ft.)	1,480.9 (52.3) 	
Rear		
Headroom	1,013.5 (39.9) 	
Leg Room	1,000.8 (39.4) 	
Knee Clearance	44.1 (1.7) 	
Shoulder Room	1,371.9 (54.0)	
Hip Room	1,294.5 (51.0) 	
SAE Rear Seat Volume Index, 
litres (cu. ft.)	1.390.3 (49.1) 	
SAE Interior Volume,  litres (cu. ft.)	2,956.2 (104.4) 	
Cargo Volume Indexes		
Rear Seats Up,  litres (cu. ft.)	651.2 (23.0) 	
Rear Seats Folded,  litres (cu. ft.)	1,514.9 (53.5) 	
Interior Volume Index,  litres (cu. ft.)	3522.6 (124.4) 	
Trunk Lift-over Height	779.8 (30.7) 	
Minimum Cargo Width at 
Liftgate Opening	988 (38.9) 	
Minimum Cargo Height at 
Liftgate Opening	656 (25.9) 	
Maximum Cargo Width at 
Liftgate Opening	1,146 (45.1) 	
Maximum Cargo Height at 
Liftgate Opening	696 (27.4) 	
Distance Between Wheelhouse Interior 	965 (38.0) 	
		
SUSPENSION 		
Front	Independent MacPherson strut, coil spring over gas-charged shock absorbers and stabilizer bar — standard	
Rear	Multi-link independent with coil springs, link-type stabilizer bar, gas-charged shock absorbers — standard 	
		
STEERING		
Type	Rack and pinion with hydraulic power assist	
Overall Ratio	16.4:1	
Turning Diameter (curb-to-curb)	With 16- or 17-in. wheels — 10.8 m (35.6 ft.) 	
Steering Turns (lock-to-lock)	With 16- or 17-in. wheels and tires — 2.88	
		
WHEELS		
Availability	Standard on Patriot Sport and North Edition	
Type and Material	Styled steel	
Size	16 x 6.5 	
		
Availability	Available on Patriot Sport and North Edition 	
Type and Material	Mineral Grey aluminum	
Size	17 x 6.5	
		
Availability	Standard on Patriot Sport Altitude II 	
Type and Material	Polished aluminum 	
Size	17 x 6.5	
		
Availability	Standard on Patriot High Altitude	
Type and Material	Polished aluminum with Granite painted pockets	
Size	17 x 6.5	
		
TIRES		
Availability	Standard on Patriot Sport and North Edition	
Size and Type	P205/70R16 BSW All-season Touring	
Manufacturer and Model	Goodyear Eagle LS2	
Revs per Kilometre (Mile)	470 (758) 	
Availability	Available on Patriot Sport and North Edition 	
	Standard on Patriot Sport Altitude II 4x2 and High Altitude	
Size and Type	P215/60R17 BSW All-season Touring	
Manufacturer and Model	Firestone Affinity	
Revs per  Kilometre (Mile)	479 (771) 	
		
Availability	Standard on Sport Altitude II 4x4	
	Included with Freedom Drive II Off-road Package and Tire and Wheel Group	
Size and Type	P215/65R17 OWL All-terrain	
Manufacturer and Model	Goodyear Wrangler GTA 03	
Revs per Kilometre (Mile)	462 (743) 	
		
BRAKES 		
Availability	Standard on Patriot 4x2	
Front		
Size and Type	294 x 26 (11.5 x 1.0) vented disc with 57 (2.2) single-piston floating caliper	
Swept Area	1,442 sq. cm (223 sq. in.) 	
Rear		
Size and Type	229 x 35 (9.0 x 1.38) drums 	
Swept Area	503.6 sq. cm (78.1 sq. in.) 	
Power-assist Type	254 (10.0) single-diaphragm vacuum	
Anti-lock Brake System (ABS)	Standard	
Electronic Stability Control (ESC)	Standard	
		
Availability	Standard on Patriot 4x4	
Front		
Size and Type	294 x 26 (11.5 x 1.0) vented disc with 57 (2.2) single-piston floating caliper	
Swept Area	1,442 sq. cm (223 sq. in.) 	
Rear		
Size and Type	262 x 10 (10.3 x 0.39) solid disc with 35 (1.4) single-piston 
floating caliper	
Swept Area	894.6 sq. cm (138.64 sq. in.) 	
Power-assist Type	254 (10) single-diaphragm vacuum	

Anti-lock Brakes with On- and Off-road Calibrations	Standard	
Electronic Stability Control (ESC)	Standard	
Hill-start Assist (HSA)	Standard with manual transmission and Freedom Drive II Off-road Package	
Off-road brake Traction-control System (BTCS)	Included with Freedom Drive II Off-road Package 	
Hill-descent Control (HDC)	Included with Freedom Drive II Off-road Package