FCA CANADA
2017 Jeep® Renegade
Canadian Specifications

Specifications are based on the latest product information available at the time of publication.  
All dimensions are in millimetres (inches) unless otherwise noted.  
All dimensions measured at curb weight with standard tires and wheels.

GENERAL INFORMATION	
Body Style 	Sport-utility vehicle (SUV)	
Assembly Plant	Melfi, Italy	
EPA Vehicle Class 	Multipurpose vehicle	
	
BODY AND CHASSIS	
Layout	Transverse front engine, 4x2 and 4x4	
Construction 	Steel uniframe	

ENGINE: 1.4-LITRE TURBOCHARGED MULTIAIR I-4	
Availability	Standard — Renegade Sport (4x2 and 4x4) and North (4x2 and 4x4)	
Type and Description	In-line four-cylinder, liquid-cooled, turbocharged	
Displacement	1,368 cu. cm (83.48 cu. in.) 	
Bore x Stroke	72.0 x 84.0 (2.83 x 3.31) 	
Valve System	Belt-driven, MultiAir, SOHC, 16 valves,hydraulic end-pivot roller rockers	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Cast-iron block with aluminum-alloy head and aluminum-alloy bedplate	
Compression Ratio	9.8:1	
Maximum Turbo Boost (psi / bar)	22 psi / 2.49 bar	
Power (SAE)	160 hp @ 5,500 rpm	
Torque (SAE)	184 lb.-ft. @ 2,500-4,000 rpm	
Max. Engine Speed	6,500 rpm (electronically limited)	
Fuel Requirement	87 octane (R+M)/2 acceptable 
91 octane recommended	
Oil Capacity	3.8 litres (4.0 quarts) with dry filter	
Coolant Capacity	5.2 litres (5.5 quarts) 	
Emission Controls 	Dual three-way catalytic converters, heated oxygen sensors and internal engine features	
	
EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	9.9 (29) / 7.5 (38) / 8.8 (32) (4x2 and 4x4)
		
Based on 2016 EnerGuide fuel consumption ratings. Government of Canada test methods used. Your actual fuel consumption will vary based on driving habits and other factors. For EnerGuide information, please visit the Government of Canada website: www.vehicles.nrcan.gc.ca 
	
Towing	Not recommended 	
Engine Assembly Plant	Termoli, Italy	
		
ENGINE: 2.4-LITRE TIGERSHARK WITH MULTIAIR2	
Availability	Standard — Renegade Limited (4x4) and Trailhawk (4x4)
Available — Renegade Sport and North (4x2 and 4x4)	
Type and Description	In-line four-cylinder, 16-valve MultiAir with multiport fuel injection	
Displacement	2,360 cu. cm (144 cu. in.) 	
Bore x Stroke	88 x 97 (3.46 X 3.82) 	
Valve System	SOHC, four valves per cylinder 	
Fuel Injection	Sequential, multiport, electronic, returnless	
Construction	Aluminum block, aluminum cylinder head	
Compression Ratio	10:1	
Power (SAE net) 	180 hp @ 6,400 rpm	
Torque (SAE net) 	175 lb.-ft. @ 3,900 rpm	
Max. Engine Speed	6,400 rpm	
Fuel Requirement	Unleaded regular, 87 octane	
Oil Capacity	5.2 litres (5.5 quarts) 	
Coolant Capacity	6.45 litres (6.8 quarts) 	
Emission Controls	Single catalytic converter, heated wide band lambda sensor upstream and 
mid-catalyst heated oxygen sensor	
EnerGuide (2016) Fuel Consumption Ratings L/100 km (MPG – imperial gallon) city/hwy/combined	10.8 (26) / 7.7 (37) / 9.4 (30) (4x2)
11.2 (25) / 8.0 (35) / 9.8 (29) (4x4)	
Towing	907 kg (2,000 lbs.) (not recommended for FWD)	
Engine Assembly Plant 	Dundee Engine Plant, Dundee, Mich.	
		
TRANSMISSION: 948TE NINE-SPEED AUTOMATIC	
Availability	2.4-litre Tigershark engine with MultiAir2 (4x2 or 4x4)	
Description 	Planetary gear train, transverse layout	
Ratio Spread	9.81	

Gear Ratios		
1st	4.71	
2nd	2.84	
3rd	1.91	
4th	1.38	
5th	1.00	
6th	0.81	
7th	0.70	
8th	0.58	
9th	0.48	
Reverse	3.83	
Final-drive Ratio	3.734
4.334 (Trailhawk)	
		
C635 SIX-SPEED MANUAL TRANSMISSION	
Availability	1.4-litre MultiAir Turbo engine (4x2 or 4x4)	
Description	1st, 2nd, 3rd gear: Triple cone 
4th: Double cone	
Gear Ratios		
1st	4.154	
2nd	2.118	
3rd	1.361	
4th	0.978	
5th	0.756	
6th	0.622	
Reverse	4.00	
Final-drive Ratio	4.438	
Overall Top Gear	2.38	
	
4X4 SYSTEMS: JEEP ACTIVE DRIVE, JEEP ACTIVE DRIVE LOW	
Availability 	Jeep Active Drive is optional on all models
Jeep Active Drive Low is standard on Trailhawk	
Type	Fully disconnecting 4x2 mode with automatic 4x4 engagement
Full-time 4x4 mode with active on demand clutch		
Operating Modes	Auto 4x2/4x4	
Center Differential Type	None	
Terrain Response	Unique tuning in all terrain modes	
Crawl Ratio	20:1 (with Jeep Active Drive Low)	
		
ELECTRICAL SYSTEM		
Alternator 	150-amp (1.4-litre MultiAir Turbo) 
160-amp (2.4-litre Tigershark with MultiAir)  	
Battery	500-amp  (1.4-litre MultiAir Turbo) 
600-amp (2.4-litre Tigershark with MultiAir) 	

SUSPENSION		
Front 	MacPherson strut, coil springs, flat front steel crossmember, high-strength steel double shell lower control arms for 4x4 and high-strength steel mono shell lower control arms for 4x2, stabilizer bar	
Rear	Chapman strut, high-strength steel links, isolated steel rear cradle for 4x4 and not-isolated for 4x2, coil springs, stabilizer bar	
		
STEERING		
Type 	Electric power rack and pinion	
Overall Ratio 	15.7 	
Turning Diameter (curb-to-curb) 	11.07 (36.3) 4x2 and 4x4
10.76 (35.3) Trailhawk 4x4		
Steering Turns (lock-to-lock)	2.68 (4x2 and 4x4)
2.76 (Trailhawk 4x4)		
		
BRAKES		
Front		
Size and Type	305 x 28 (12 x 1.1) vented rotor with 
60 (2.36) single-piston floating caliper	
Swept Area (per caliper)	895.3 sq. cm (138.77 sq. in.),1 x 60
747.6 sq. cm (115.88 sq. in.),1 x 57 		

Rear		
Size and Type 	278 x 12 (10.95 x 0.47) solid rotor with 
38 (1.5) single-piston floating caliper	
Swept Area (per caliper)	656.4 sq. cm (101.7 sq. in.) (), 1 x 38	
Power-assist Type 	254 (10) vacuum assist 	
Four-wheel anti-lock brake system (ABS)	Standard	
Electronic stability control (ESC)	Standard	
Parking Brake Type	Electric motor on caliper	
	
DIMENSIONS AND CAPACITIES		
Wheelbase	2,570 (101.2) 	
Track, Front	1,540 (60.6) 	
Track, Rear	1,540 (60.6) 	
Overall Length	4,232 (166.6) 	
Overall Width (with folded side mirrors)	1,886.8 (74.2) 	
Overall Width (with open side mirrors)	2,023.1 (79.6) 	
Overall Height 	1,689 (66.5) 	
Load-floor height	758 (29.8) 	
Sill-step height	494 (19.4) front, 497 (19.6) rear	
Ground Clearances 	170 (6.7) 4x2
203 (8.0) 4x4  
221 (8.7) Trailhawk 4x4 		
Approach Angle, (with air dam) (degrees)	17.9 - 4x2
21.0 - 4x4
30.5 - Trailhawk 4x4		
Breakover Angle (degrees)	21.2 - 4x2
24.0 - 4x4
25.7 - Trailhawk 4x4		
Departure Angle (degrees)	29.7 - 4x2
32.1 - 4x4 
34.3 - Trailhawk 4x4		

Curb Weight kg (lbs.)	1,386 (3,056) 4x2 and 1.4-litre MultiAir Turbo
1,456 (3,210) 4x4 and 1.4-litre MultiAir Turbo
1,436 (3,166) 4x2 and 2.4-litre Tigershark with MultiAir
1,509 (3,327) 4x4 and 2.4-litre Tigershark with MultiAir 
1,602 (3,532) Trailhawk 4x4 with 2.4-litre Tigershark with MultiAir	
Aero Cd	0.35 4x2
0.36 4x4
0.37 Trailhawk 4x4		
Fuel-tank Capacity	48 litres (10.6 gal.) 	
	
ACCOMMODATIONS		
Seating Capacity — Front/Rear 	2/3	
Front Row		
Headroom without Sunroof	1,045 (41.1) 	
Headroom with Sunroof	1,009 (39.7) 	
Legroom 	1,046 (41.2) 	
Shoulder Room 	1,419 (55.9) 	
Hip Room	1,348 (53.1) 	
Seat Travel 	230 (9.0) driver / 260 (10.2) front passenger	
Recliner Range (degrees)	From 25 nominal, 38 forward and 30 rearward (from vertical 13 forward, 
55 rearward)	
SAE Volume (standard roof), 
litres (cu. ft.)	1,551.7 (54.8) 	
Second Row		
Headroom 	1,029 (40.5) 	
Legroom 	891 (35.1) 	
Shoulder Room 	1,400 (55.1) 	
Hip Room	1,319 (51.9) 	
SAE Volume, litres (cu. ft.) 	1,282.7 (45.3) 	
Cargo Access		
Liftover Height	766 (30.2) 	
Maximum Cargo Width at Liftgate Opening	1,020 (40.1) 	
Minimum Cargo Width at Liftgate Opening 	990 (39.0) at bottom of opening	

Maximum Cargo Height at Liftgate Opening	749 (29.5) 	
Minimum Cargo Height at Liftgate Opening	739 (29.0) 	
Distance Between Wheelhouse Interior Trim	956 (37.6) 	
SAE Cargo Volume		
Rear Seats Up, litres (cu. ft.)	523.8 (18.5) 	
Rear Seats Folded, litres (cu. ft.)	1438.4 (50.8) 	
EPA Interior Volume Index, litres (cu. ft.)	3,358.3 (118.6) 	
	
TIRES		
Availability	Standard — Sport / North 	
Size and Type 	215/65R16 LBL All-season 	
Mfr. and Model 	Unspecified	
		
Availability	Standard — North (with 2.4-litre Tigershark with MultiAir) 	
Size and Type 	215/60R17 BSW All-season 	
Mfr. and Model 	Dunlop	
		
Availability	Standard — Limited 
Optional — North 		
Size and Type 	225/55R18 BSW All-season 	
Mfr. and Model	Unspecified 	
		
Availability	Standard on Trailhawk  	
Size and Type	215/65R17 BSW All-season	
Mfr. and Model	Unspecified 	
Revs per Mile (km)	722 (448)